{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":287,"n_cols":10,"rows_kept":287,"cut":false,"hidden":false,"merged":[]}
["new Item no","Item no long","Descr Russian","Pack unit","Sub pack unit","2015.07.01 Price / piece in RUB, exclude VAT","Product Group","Series","Скидка от Прайс-Листа, %","Цена за единицу продукции с учётом скидки без НДС, руб"]
[20000115,"2000-115","Предупр.марк. TOPJOB S 5 марк.",100,25,15.7,22,2000,0.5,7.85]
[51221370,"2000-1201","Кл. TOPJOB S 1мм2 2пр ",100,0,32.61,22,2000,0.5,16.305]
[51221371,"2000-1202","Кл. TOPJOB S 1мм2 2пр ор.",100,0,33.21,22,2000,0.5,16.605]
[51221372,"2000-1203","Кл. TOPJOB S 1мм2 2пр кр.",100,0,33.21,22,2000,0.5,16.605]
[51221373,"2000-1204","Кл. TOPJOB S 1мм2 2пр с.",100,0,33.21,22,2000,0.5,16.605]
[51221374,"2000-1205","Кл. TOPJOB S 1мм2 2пр черн.",100,0,33.21,22,2000,0.5,16.605]
[51221375,"2000-1206","Кл. TOPJOB S 1мм2 2пр жел.",100,0,33.21,22,2000,0.5,16.605]
[51221376,"2000-1207","Кл. TOPJOB S 1мм2 2пр РЕ",100,0,131,22,2000,0.5,65.5]
[20000121,"2000-121","Держ.марк. TOPJOB S",50,25,12.08,22,2000,0.5,6.04]
[20001291,"2000-1291","Торц.пл. TOPJOB S 0,7мм 2пр ",100,25,19.32,22,2000,0.5,9.66]
[20001292,"2000-1292","Торц.пл. TOPJOB S 0,7мм 2пр ор.",100,25,19.32,22,2000,0.5,9.66]
[51221378,"2000-1301","Кл. TOPJOB S 1мм2 3пр ",100,0,39.86,22,2000,0.5,19.93]
[51221379,"2000-1302","Кл. TOPJOB S 1мм2 3пр ор.",100,0,41.07,22,2000,0.5,20.535]
[51221380,"2000-1303","Кл. TOPJOB S 1мм2 3пр кр.",100,0,41.07,22,2000,0.5,20.535]
[51221381,"2000-1304","Кл. TOPJOB S 1мм2 3пр с.",100,0,41.07,22,2000,0.5,20.535]
[51221382,"2000-1305","Кл. TOPJOB S 1мм2 3пр черн.",100,0,41.07,22,2000,0.5,20.535]
[51221383,"2000-1306","Кл. TOPJOB S 1мм2 3пр жел.",100,0,41.07,22,2000,0.5,20.535]
[51221384,"2000-1307","Кл. TOPJOB S 1мм2 3пр РЕ",100,0,154,22,2000,0.5,77]
[20001391,"2000-1391","Торц.пл. TOPJOB S 0,7мм 3пр ",100,25,19.93,22,2000,0.5,9.9649999999999999]
[20001392,"2000-1392","Торц.пл. TOPJOB S 0,7мм 3пр ор.",100,25,19.93,22,2000,0.5,9.9649999999999999]
[51221386,"2000-1401","Кл. TOPJOB S 1мм2 4пр ",100,0,46.5,22,2000,0.5,23.25]
[51221387,"2000-1402","Кл. TOPJOB S 1мм2 4пр ор.",100,0,48.31,22,2000,0.5,24.155000000000001]
[51221388,"2000-1403","Кл. TOPJOB S 1мм2 4пр кр.",100,0,48.31,22,2000,0.5,24.155000000000001]
[51221389,"2000-1404","Кл. TOPJOB S 1мм2 4пр с.",100,0,48.31,22,2000,0.5,24.155000000000001]
[51221391,"2000-1405","Кл. TOPJOB S 1мм2 4пр черн.",100,0,48.31,22,2000,0.5,24.155000000000001]
[51221392,"2000-1406","Кл. TOPJOB S 1мм2 4пр жел.",100,0,48.31,22,2000,0.5,24.155000000000001]
[51221393,"2000-1407","Кл. TOPJOB S 1мм2 4пр PE",100,0,166.1,22,2000,0.5,83.05]
[20001491,"2000-1491","Торц.пл. TOPJOB S 0,7мм 4пр ",100,25,20.53,22,2000,0.5,10.265000000000001]
[20001492,"2000-1492","Торц.пл. TOPJOB S 0,7мм 4пр ор.",100,25,20.53,22,2000,0.5,10.265000000000001]
[20002141,"2000-2141","Кл. TOPJOB S 1мм2 4пр 2птц ",50,0,73.069999999999993,22,2000,0.5,36.534999999999997]
[20002195,"2000-2195","Торц.пл. TOPJOB S 0,7мм 4пр ",100,25,21.14,22,2000,0.5,10.57]
[20002196,"2000-2196","Торц.пл. TOPJOB S 0,7мм 4пр ор.",100,25,21.14,22,2000,0.5,10.57]
[51293893,"2000-2201","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,86.96,22,2000,0.5,43.48]
[51226989,"2000-2201/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,103.9,22,2000,0.5,51.95]
[20002202,"2000-2202","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,90.59,22,2000,0.5,45.295000000000002]
[51227013,"2000-2202/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,107.5,22,2000,0.5,53.75]
[20002203,"2000-2203","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,90.59,22,2000,0.5,45.295000000000002]
[51227014,"2000-2203/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,107.5,22,2000,0.5,53.75]
[20002204,"2000-2204","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,90.59,22,2000,0.5,45.295000000000002]
[51227015,"2000-2204/099-000","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,107.5,22,2000,0.5,53.75]
[20002207,"2000-2207","Кл. TOPJOB S 1мм2 4пр 2ур о-РЕ",50,0,227.7,22,2000,0.5,113.85]
[51227017,"2000-2207/099-000","Кл. TOPJOB S 1мм2 4пр 2ур о-РЕ",50,0,245.8,22,2000,0.5,122.9]
[20002208,"2000-2208","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,118.4,22,2000,0.5,59.2]
[51227018,"2000-2208/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,135.9,22,2000,0.5,67.95]
[20002209,"2000-2209","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,121.4,22,2000,0.5,60.7]
[51227019,"2000-2209/099-000","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,138.9,22,2000,0.5,69.45]
[20002217,"2000-2217","Кл. TOPJOB S 1мм2 4пр 2ур ",50,0,184.2,22,2000,0.5,92.1]
[51227020,"2000-2217/099-000","Кл. TOPJOB S 1мм2 4пр 2ур ",50,0,201.7,22,2000,0.5,100.85]
[20002218,"2000-2218","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,184.2,22,2000,0.5,92.1]
[51227021,"2000-2218/099-000","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,201.7,22,2000,0.5,100.85]
[20002227,"2000-2227","Кл. TOPJOB S 1мм2 4пр 2ур ",50,0,184.2,22,2000,0.5,92.1]
[51227022,"2000-2227/099-000","Кл. TOPJOB S 1мм2 4пр 2ур ",50,0,201.7,22,2000,0.5,100.85]
[20002228,"2000-2228","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,184.2,22,2000,0.5,92.1]
[51227023,"2000-2228/099-000","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,201.7,22,2000,0.5,100.85]
[51303123,"2000-2231","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,94.81,22,2000,0.5,47.405000000000001]
[51227024,"2000-2231/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,112.3,22,2000,0.5,56.15]
[20002232,"2000-2232","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,97.83,22,2000,0.5,48.914999999999999]
[51227025,"2000-2232/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,115.3,22,2000,0.5,57.65]
[20002233,"2000-2233","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,97.83,22,2000,0.5,48.914999999999999]
[51227026,"2000-2233/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,115.3,22,2000,0.5,57.65]
[20002234,"2000-2234","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,97.83,22,2000,0.5,48.914999999999999]
[51227027,"2000-2234/099-000","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,115.3,22,2000,0.5,57.65]
[20002237,"2000-2237","Кл. TOPJOB S 1мм2 4пр 2ур о-РЕ",50,0,234.9,22,2000,0.5,117.45]
[51227028,"2000-2237/099-000","Кл. TOPJOB S 1мм2 4пр 2ур о-РЕ",50,0,252.4,22,2000,0.5,126.2]
[20002238,"2000-2238","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,125,22,2000,0.5,62.5]
[51227029,"2000-2238/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,141.9,22,2000,0.5,70.95]
[20002239,"2000-2239","Кл. TOPJOB S 1мм2 4пр 2ур с.",50,0,129.19999999999999,22,2000,0.5,64.599999999999994]
[51227031,"2000-2239/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,146.69999999999999,22,2000,0.5,73.349999999999994]
[20002247,"2000-2247","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,190.8,22,2000,0.5,95.4]
[51227033,"2000-2247/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,207.7,22,2000,0.5,103.85]
[20002248,"2000-2248","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,190.8,22,2000,0.5,95.4]
[51227034,"2000-2248/099-000","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,207.7,22,2000,0.5,103.85]
[20002257,"2000-2257","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,190.8,22,2000,0.5,95.4]
[51227035,"2000-2257/099-000","Кл. TOPJOB S 1мм2 4пр 2ур",50,0,207.7,22,2000,0.5,103.85]
[20002258,"2000-2258","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,190.8,22,2000,0.5,95.4]
[51227036,"2000-2258/099-000","Кл. TOPJOB S 1мм2 4пр 2ур экр",50,0,207.7,22,2000,0.5,103.85]
[20002291,"2000-2291","Торц.пл. TOPJOB S 0,7мм 2ур ",25,0,19.93,22,2000,0.5,9.9649999999999999]
[20002292,"2000-2292","Торц.пл. TOPJOB S 0,7мм 2ур ор.",25,0,19.93,22,2000,0.5,9.9649999999999999]
[20000402,"2000-402","Перемычка TOPJOB S 2конт.",200,25,13.29,22,2000,0.5,6.6449999999999996]
[51292045,"2000-402/000-005","Перемычка TOPJOB S 2конт. кр.",200,25,13.89,22,2000,0.5,6.9450000000000003]
[51292051,"2000-402/000-006","Перемычка TOPJOB S 2конт. с.",200,25,13.89,22,2000,0.5,6.9450000000000003]
[20000403,"2000-403","Перемычка TOPJOB S 3конт.",200,25,23.55,22,2000,0.5,11.775]
[51292046,"2000-403/000-005","Перемычка TOPJOB S 3конт. кр.",200,25,24.16,22,2000,0.5,12.08]
[51292052,"2000-403/000-006","Перемычка TOPJOB S 3конт. с.",200,25,24.16,22,2000,0.5,12.08]
[20000404,"2000-404","Перемычка TOPJOB S 4конт.",200,25,36.840000000000003,22,2000,0.5,18.420000000000002]
[51292047,"2000-404/000-005","Перемычка TOPJOB S 4конт. кр.",200,25,38.65,22,2000,0.5,19.324999999999999]
[51292053,"2000-404/000-006","Перемычка TOPJOB S 4конт. с.",200,25,38.65,22,2000,0.5,19.324999999999999]
[20000405,"2000-405","Перемычка TOPJOB S 5конт.",100,25,48.92,22,2000,0.5,24.46]
[51292048,"2000-405/000-005","Перемычка TOPJOB S 5конт. кр.",100,25,50.12,22,2000,0.5,25.06]
[51292054,"2000-405/000-006","Перемычка TOPJOB S 5конт. с.",100,25,50.12,22,2000,0.5,25.06]
[51219605,"2000-405/011-000","Перемычка TOPJOB S 5конт. 1-3-5",100,25,51.33,22,2000,0.5,25.664999999999999]
[20000406,"2000-406","Перемычка TOPJOB S 6конт.",100,25,61.6,22,2000,0.5,30.8]
[51292087,"2000-406/000-005","Перемычка TOPJOB S 6конт. кр.",100,25,64.010000000000005,22,2000,0.5,32.005000000000003]
[51292091,"2000-406/000-006","Перемычка TOPJOB S 6конт. с.",100,25,64.010000000000005,22,2000,0.5,32.005000000000003]
[51219846,"2000-406/020-000","Дельта-Перемычка TOPJOB S 6конт",100,25,65.22,22,2000,0.5,32.61]
[20000407,"2000-407","Перемычка TOPJOB S 7конт.",100,25,73.680000000000007,22,2000,0.5,36.840000000000003]
[51292088,"2000-407/000-005","Перемычка TOPJOB S 7конт. кр.",100,25,76.7,22,2000,0.5,38.35]
[51292092,"2000-407/000-006","Перемычка TOPJOB S 7конт. с.",100,25,76.7,22,2000,0.5,38.35]
[20000408,"2000-408","Перемычка TOPJOB S 8конт.",100,25,85.15,22,2000,0.5,42.575000000000003]
[51292089,"2000-408/000-005","Перемычка TOPJOB S 8конт. кр.",100,25,87.57,22,2000,0.5,43.784999999999997]
[51292093,"2000-408/000-006","Перемычка TOPJOB S 8конт. с.",100,25,87.57,22,2000,0.5,43.784999999999997]
[20000409,"2000-409","Перемычка TOPJOB S 9конт.",100,25,98.44,22,2000,0.5,49.22]
[51292090,"2000-409/000-005","Перемычка TOPJOB S 9конт. кр.",100,25,102.7,22,2000,0.5,51.35]
[51292094,"2000-409/000-006","Перемычка TOPJOB S 9конт. с.",100,25,102.7,22,2000,0.5,51.35]
[20000410,"2000-410","Перемычка TOPJOB S 4конт.",100,25,111.1,22,2000,0.5,55.55]
[51292049,"2000-410/000-005","Перемычка TOPJOB S 10конт. Кр",100,25,115.3,22,2000,0.5,57.65]
[51292055,"2000-410/000-006","Перемычка TOPJOB S 10конт. с.",100,25,115.3,22,2000,0.5,57.65]
[20000433,"2000-433","Перемычка TOPJOB S 2конт. 1-3",200,25,21.74,22,2000,0.5,10.87]
[51292050,"2000-433/000-005","Перемычка TOPJOB S 2конт. 1-3",200,25,22.95,22,2000,0.5,11.475]
[51292056,"2000-433/000-006","Перемычка TOPJOB S 2конт. 1-3",200,25,22.95,22,2000,0.5,11.475]
[20000434,"2000-434","Перемычка TOPJOB S 2конт. 1-4",200,25,36.840000000000003,22,2000,0.5,18.420000000000002]
[20000435,"2000-435","Перемычка TOPJOB S 2конт. 1-5",100,25,51.33,22,2000,0.5,25.664999999999999]
[20000436,"2000-436","Перемычка TOPJOB S 2конт. 1-6",100,25,65.22,22,2000,0.5,32.61]
[20000437,"2000-437","Перемычка TOPJOB S 2конт. 1-7",100,25,80.319999999999993,22,2000,0.5,40.159999999999997]
[20000438,"2000-438","Перемычка TOPJOB S 2конт. 1-8",100,25,95.42,22,2000,0.5,47.71]
[20000439,"2000-439","Перемычка TOPJOB S 2конт. 1-9",100,25,108.1,22,2000,0.5,54.05]
[20000440,"2000-440","Перемычка TOPJOB S 2конт. 1-10",100,25,122.6,22,2000,0.5,61.3]
[20000492,"2000-492","Перемычка TOPJOB S верт. 2ур",100,25,35.03,22,2000,0.5,17.515000000000001]
[2000110,"200-110","Алюминиевые плоские рельсы",100,0,44.08,10,200,0.45,24.244]
[20010115,"2001-115","Предупр.марк. TOPJOB S 5 марк.",100,25,15.7,22,2001,0.5,7.85]
[20011201,"2001-1201","Кл. TOPJOB S 1,5мм2 2пр ",100,0,32.61,22,2001,0.5,16.305]
[20011202,"2001-1202","Кл. TOPJOB S 1,5мм2 2пр ор.",100,0,33.21,22,2001,0.5,16.605]
[20011203,"2001-1203","Кл. TOPJOB S 1,5мм2 2пр ор.",100,0,33.21,22,2001,0.5,16.605]
[20011204,"2001-1204","Кл. TOPJOB S 1,5мм2 2пр с.",100,0,33.21,22,2001,0.5,16.605]
[20011205,"2001-1205","Кл. TOPJOB S 1,5мм2 2пр черн.",100,0,33.21,22,2001,0.5,16.605]
[20011206,"2001-1206","Кл. TOPJOB S 1,5мм2 2пр жел.",100,0,33.21,22,2001,0.5,16.605]
[20011207,"2001-1207","Кл. TOPJOB S 1,5мм2 2пр РЕ",100,0,131,22,2001,0.5,65.5]
[51190169,"2001-1211/1000-410","Кл. TOPJOB S 1,5мм2 2пр д-д",100,0,157.6,22,2001,0.5,78.8]
[51190170,"2001-1211/1000-411","Кл. TOPJOB S 1,5мм2 2пр д-д",100,0,157.6,22,2001,0.5,78.8]
[20011301,"2001-1301","Кл. TOPJOB S 1,5мм2 3пр ",100,0,39.86,22,2001,0.5,19.93]
[20011302,"2001-1302","Кл. TOPJOB S 1,5мм2 3пр ор.",100,0,41.07,22,2001,0.5,20.535]
[20011303,"2001-1303","Кл. TOPJOB S 1,5мм2 3пр кр.",100,0,41.07,22,2001,0.5,20.535]
[20011304,"2001-1304","Кл. TOPJOB S 1,5мм2 3пр с.",100,0,41.07,22,2001,0.5,20.535]
[20011305,"2001-1305","Кл. TOPJOB S 1,5мм2 3пр черн.",100,0,41.07,22,2001,0.5,20.535]
[20011306,"2001-1306","Кл. TOPJOB S 1,5мм2 3пр жел.",100,0,41.07,22,2001,0.5,20.535]
[20011307,"2001-1307","Кл. TOPJOB S 1,5мм2 3пр PE",100,0,154,22,2001,0.5,77]
[51190172,"2001-1311/1000-410","Кл. TOPJOB S 1,5мм2 3пр д-д",100,0,169.7,22,2001,0.5,84.85]
[51190173,"2001-1311/1000-411","Кл. TOPJOB S 1,5мм2 3пр д-д",100,0,169.7,22,2001,0.5,84.85]
[51190176,"2001-1321/1000-413","Кл. TOPJOB S 1,5мм2 3пр LED",100,0,272.39999999999998,22,2001,0.5,136.19999999999999]
[51190174,"2001-1321/1000-434","Кл. TOPJOB S 1,5мм2 3пр LED",100,0,272.39999999999998,22,2001,0.5,136.19999999999999]
[20011401,"2001-1401","Кл. TOPJOB S 1,5мм2 4пр ",100,0,46.5,22,2001,0.5,23.25]
[20011402,"2001-1402","Кл. TOPJOB S 1,5мм2 4пр ор.",100,0,48.31,22,2001,0.5,24.155000000000001]
[20011403,"2001-1403","Кл. TOPJOB S 1,5мм2 4пр кр.",100,0,48.31,22,2001,0.5,24.155000000000001]
[20011404,"2001-1404","Кл. TOPJOB S 1,5мм2 4пр с.",100,0,48.31,22,2001,0.5,24.155000000000001]
[20011405,"2001-1405","Кл. TOPJOB S 1,5мм2 4пр черн.",100,0,48.31,22,2001,0.5,24.155000000000001]
[20011406,"2001-1406","Кл. TOPJOB S 1,5мм2 4пр жел.",100,0,48.31,22,2001,0.5,24.155000000000001]
[20011407,"2001-1407","Кл. TOPJOB S 1,5мм2 4пр РЕ",100,0,166.1,22,2001,0.5,83.05]
[20011408,"2001-1408","Кл. TOPJOB S 1,5мм2 4пр экр бел.",100,0,166.1,22,2001,0.5,83.05]
[20011411,"2001-1411","Кл. TOPJOB S 1,5мм2 4пр д-д",100,0,82.13,22,2001,0.5,41.064999999999998]
[51190177,"2001-1411/1000-410","Кл. TOPJOB S 1,5мм2 4пр д-д",100,0,175.7,22,2001,0.5,87.85]
[51190178,"2001-1411/1000-411","Кл. TOPJOB S 1,5мм2 4пр д-д",100,0,175.7,22,2001,0.5,87.85]
[51190180,"2001-1421/1000-413","Кл. TOPJOB S 1,5мм2 4пр LED",100,0,283.2,22,2001,0.5,141.6]
[51190179,"2001-1421/1000-434","Кл. TOPJOB S 1,5мм2 4пр LED",100,0,283.2,22,2001,0.5,141.6]
[20011441,"2001-1441","Кл. TOPJOB S 1,5мм2 4пр 2птц",100,0,65.83,22,2001,0.5,32.914999999999999]
[2000116,"200-116","Алюминиевые плоские рельсы",100,0,60.99,10,200,0.45,33.544499999999999]
[20010171,"2001-171","Стопор для изоляции TOPJOB S ",200,25,6.64,22,2001,0.5,3.32]
[20010402,"2001-402","Перемычка TOPJOB S 2конт.",200,25,13.29,22,2001,0.5,6.6449999999999996]
[20010403,"2001-403","Перемычка TOPJOB S 3конт.",200,25,23.55,22,2001,0.5,11.775]
[20010404,"2001-404","Перемычка TOPJOB S 4конт.",200,25,36.840000000000003,22,2001,0.5,18.420000000000002]
[20010405,"2001-405","Перемычка TOPJOB S 5конт.",100,25,48.92,22,2001,0.5,24.46]
[51218363,"2001-405/011-000","Перемычка TOPJOB S 5конт. 1-3-5",100,25,51.33,22,2001,0.5,25.664999999999999]
[20010406,"2001-406","Перемычка TOPJOB S 6конт.",100,25,61.6,22,2001,0.5,30.8]
[51219847,"2001-406/020-000","Перемычка 6конт. 1-2,3-4,5-6",100,25,65.22,22,2001,0.5,32.61]
[20010407,"2001-407","Перемычка TOPJOB S 7конт.",100,25,73.680000000000007,22,2001,0.5,36.840000000000003]
[20010408,"2001-408","Перемычка TOPJOB S 8конт.",100,25,85.15,22,2001,0.5,42.575000000000003]
[20010409,"2001-409","Перемычка TOPJOB S 9конт.",100,25,98.44,22,2001,0.5,49.22]
[20010410,"2001-410","Перемычка TOPJOB S 10конт.",100,25,111.1,22,2001,0.5,55.55]
[20010433,"2001-433","Перемычка TOPJOB S 2конт. 1-3",200,25,21.74,22,2001,0.5,10.87]
[20010434,"2001-434","Перемычка TOPJOB S 2конт. 1-4",200,25,36.840000000000003,22,2001,0.5,18.420000000000002]
[20010435,"2001-435","Перемычка TOPJOB S 2конт. 1-5",100,25,51.33,22,2001,0.5,25.664999999999999]
[20010436,"2001-436","Перемычка TOPJOB S 2конт. 1-6",100,25,65.22,22,2001,0.5,32.61]
[20010437,"2001-437","Перемычка TOPJOB S 2конт. 1-7",100,25,80.319999999999993,22,2001,0.5,40.159999999999997]
[20010438,"2001-438","Перемычка TOPJOB S 2конт. 1-8",100,25,95.42,22,2001,0.5,47.71]
[20010439,"2001-439","Перемычка TOPJOB S 2конт. 1-9",100,25,108.1,22,2001,0.5,54.05]
[20010440,"2001-440","Перемычка TOPJOB S 2конт. 1-10",100,25,122.6,22,2001,0.5,61.3]
[20010501,"2001-501","Отвод TOPJOB S 1,5мм2 1пол.",100,25,84.55,22,2001,0.5,42.274999999999999]
[20010511,"2001-511","Отвод TOPJOB S 1,5мм2 1пол.",100,25,84.55,22,2001,0.5,42.274999999999999]
[20010549,"2001-549","Разделит. отвода TOPJOB S ",100,25,17.510000000000002,22,2001,0.5,8.7550000000000008]
[20010552,"2001-552","Отвод TOPJOB S 1,5мм2 2пол. ",25,0,170.3,22,2001,0.5,85.15]
[20010553,"2001-553","Отвод TOPJOB S 1,5мм2 3пол. ",25,0,254.8,22,2001,0.5,127.4]
[20010554,"2001-554","Отвод TOPJOB S 1,5мм2 4пол. ",25,0,340.6,22,2001,0.5,170.3]
[20010555,"2001-555","Отвод TOPJOB S 1,5мм2 5пол. ",10,0,425.1,22,2001,0.5,212.55]
[20010556,"2001-556","Отвод TOPJOB S 1,5мм2 6пол. ",10,0,510.9,22,2001,0.5,255.45]
[20010557,"2001-557","Отвод TOPJOB S 1,5мм2 7пол. ",10,0,595.4,22,2001,0.5,297.7]
[20010558,"2001-558","Отвод TOPJOB S 1,5мм2 8пол. ",10,0,680.6,22,2001,0.5,340.3]
[20010559,"2001-559","Отвод TOPJOB S 1,5мм2 9пол. ",10,0,765.1,22,2001,0.5,382.55]
[20010560,"2001-560","Отвод TOPJOB S 1,5мм2 10пол. ",10,0,851.5,22,2001,0.5,425.75]
[20021091,"2002-1091","Торц.пл. TOPJOB S 1мм 2ур ",100,25,25.97,22,2002,0.5,12.984999999999999]
[20021092,"2002-1092","Торц.пл. TOPJOB S 1мм 2ур ор.",100,25,25.97,22,2002,0.5,12.984999999999999]
[20020115,"2002-115","Предупр.марк. TOPJOB S 5 марк.",100,25,16.91,22,2002,0.5,8.4550000000000001]
[20020116,"2002-116","Многоцелевой исполнит.инструмент",5,0,70.05,22,2002,0.5,35.024999999999999]
[20021201,"2002-1201","Кл. TOPJOB S 2,5мм2 2пр ",100,0,36.840000000000003,22,2002,0.5,18.420000000000002]
[20021202,"2002-1202","Кл. TOPJOB S 2,5мм2 2пр ор.",100,0,39.25,22,2002,0.5,19.625]
[20021203,"2002-1203","Кл. TOPJOB S 2,5мм2 2пр кр.",100,0,39.25,22,2002,0.5,19.625]
[20021204,"2002-1204","Кл. TOPJOB S 2,5мм2 2пр с.",100,0,39.25,22,2002,0.5,19.625]
[20021205,"2002-1205","Кл. TOPJOB S 2,5мм2 2пр черн.",100,0,39.25,22,2002,0.5,19.625]
[20021206,"2002-1206","Кл. TOPJOB S 2,5мм2 2пр жел.",100,0,39.25,22,2002,0.5,19.625]
[20021207,"2002-1207","Кл. TOPJOB S 2,5мм2 2пр РЕ",100,0,137.69999999999999,22,2002,0.5,68.849999999999994]
[60248635,"2002-1208","Кл. TOPJOB S 2,5мм2 2пр экр бел.",100,0,137.69999999999999,22,2002,0.5,68.849999999999994]
[20020121,"2002-121","Держ.марк. TOPJOB S 2ур",50,25,12.08,22,2002,0.5,6.04]
[51190181,"2002-1211/1000-410","Кл. TOPJOB S 2,5мм2 2пр д-д",100,0,164.9,22,2002,0.5,82.45]
[51190182,"2002-1211/1000-411","Кл. TOPJOB S 2,5мм2 2пр д-д",100,0,164.9,22,2002,0.5,82.45]
[20021291,"2002-1291","Торц.пл. TOPJOB S 0,8мм 2пр ",100,25,19.32,22,2002,0.5,9.66]
[60245955,"2002-1292","Торц.пл. TOPJOB S 0,8мм 2пр ор.",100,25,19.32,22,2002,0.5,9.66]
[20021293,"2002-1293","Раздел.пл. TOPJOB S 2мм 2пр ор.",100,25,20.53,22,2002,0.5,10.265000000000001]
[20021294,"2002-1294","Раздел.пл. TOPJOB S 2мм 2пр ",100,25,20.53,22,2002,0.5,10.265000000000001]
[20021301,"2002-1301","Кл. TOPJOB S 2,5мм2 3пр ",100,0,44.69,22,2002,0.5,22.344999999999999]
[20021302,"2002-1302","Кл. TOPJOB S 2,5мм2 3пр ор.",100,0,47.1,22,2002,0.5,23.55]
[20021303,"2002-1303","Кл. TOPJOB S 2,5мм2 3пр кр.",100,0,47.1,22,2002,0.5,23.55]
[20021304,"2002-1304","Кл. TOPJOB S 2,5мм2 3пр с.",100,0,47.1,22,2002,0.5,23.55]
[20021305,"2002-1305","Кл. TOPJOB S 2,5мм2 3пр черн.",100,0,47.1,22,2002,0.5,23.55]
[20021306,"2002-1306","Кл. TOPJOB S 2,5мм2 3пр жел.",100,0,47.1,22,2002,0.5,23.55]
[20021307,"2002-1307","Кл. TOPJOB S 2,5мм2 3пр РЕ",100,0,166.1,22,2002,0.5,83.05]
[20021308,"2002-1308","Кл. TOPJOB S 2,5мм2 3пр экр бел.",100,0,166.1,22,2002,0.5,83.05]
[20020131,"2002-131","Держ.марк. TOPJOB S 3ур",50,25,12.68,22,2002,0.5,6.34]
[20021311,"2002-1311","Кл. TOPJOB S 2,5мм2 3пр д-д",100,0,81.53,22,2002,0.5,40.765000000000001]
[51190183,"2002-1311/1000-410","Кл. TOPJOB S 2,5мм2 3пр д-д",100,0,174.5,22,2002,0.5,87.25]
[51190184,"2002-1311/1000-411","Кл. TOPJOB S 2,5мм2 3пр д-д",100,0,174.5,22,2002,0.5,87.25]
[20021321,"2002-1321","Кл. TOPJOB S 2,5мм2 3пр LED",100,0,81.53,22,2002,0.5,40.765000000000001]
[51190186,"2002-1321/1000-413","Кл. TOPJOB S 2,5мм2 3пр LED",100,0,278.39999999999998,22,2002,0.5,139.19999999999999]
[51190185,"2002-1321/1000-434","Кл. TOPJOB S 2,5мм2 3пр LED",100,0,278.39999999999998,22,2002,0.5,139.19999999999999]
[20021391,"2002-1391","Торц.пл. TOPJOB S 0,8мм 3пр ",100,25,19.93,22,2002,0.5,9.9649999999999999]
[20021392,"2002-1392","Торц.пл. TOPJOB S 0,8мм 3пр ор.",100,25,19.93,22,2002,0.5,9.9649999999999999]
[20021393,"2002-1393","Раздел.пл. TOPJOB S 2мм 3пр ор.",100,25,21.14,22,2002,0.5,10.57]
[20021394,"2002-1394","Раздел.пл. TOPJOB S 2мм 3пр ",100,25,21.14,22,2002,0.5,10.57]
[20021401,"2002-1401","Кл. TOPJOB S 2,5мм2 4пр ",100,0,60.99,22,2002,0.5,30.495000000000001]
[20021402,"2002-1402","Кл. TOPJOB S 2,5мм2 4пр ор.",100,0,62.81,22,2002,0.5,31.405000000000001]
[20021403,"2002-1403","Кл. TOPJOB S 2,5мм2 4пр кр.",100,0,62.81,22,2002,0.5,31.405000000000001]
[20021404,"2002-1404","Кл. TOPJOB S 2,5мм2 4пр с.",100,0,62.81,22,2002,0.5,31.405000000000001]
[20021405,"2002-1405","Кл. TOPJOB S 2,5мм2 4пр черн.",100,0,62.81,22,2002,0.5,31.405000000000001]
[20021406,"2002-1406","Кл. TOPJOB S 2,5мм2 4пр жел.",100,0,62.81,22,2002,0.5,31.405000000000001]
[20021407,"2002-1407","Кл. TOPJOB S 2,5мм2 4пр РЕ",100,0,188.4,22,2002,0.5,94.2]
[20021408,"2002-1408","Кл. TOPJOB S 2,5мм2 4пр экр бел.",100,0,188.4,22,2002,0.5,94.2]
[20021411,"2002-1411","Кл. TOPJOB S 2,5мм2 4пр д-д",100,0,96.62,22,2002,0.5,48.31]
[51190102,"2002-1411/1000-410","Кл. TOPJOB S 2,5мм2 4пр д-д",100,0,190.2,22,2002,0.5,95.1]
[51190103,"2002-1411/1000-411","Кл. TOPJOB S 2,5мм2 4пр д-д",100,0,190.2,22,2002,0.5,95.1]
[51190189,"2002-1421/1000-413","Кл. TOPJOB S 2,5мм2 4пр LED",100,0,297.7,22,2002,0.5,148.85]
[51190188,"2002-1421/1000-434","Кл. TOPJOB S 2,5мм2 4пр LED",100,0,297.7,22,2002,0.5,148.85]
[20021441,"2002-1441","Кл. TOPJOB S 2,5мм2 4пр 2птц",100,0,88.77,22,2002,0.5,44.384999999999998]
[20021491,"2002-1491","Торц.пл. TOPJOB S 0,8мм 4пр ",100,25,20.53,22,2002,0.5,10.265000000000001]
[60245950,"2002-1492","Торц.пл. TOPJOB S 0,8мм 4пр ор.",100,25,20.53,22,2002,0.5,10.265000000000001]
[20021493,"2002-1493","Раздел.пл. TOPJOB S 2мм 4пр ор.",100,25,21.74,22,2002,0.5,10.87]
[20021494,"2002-1494","Раздел.пл. TOPJOB S 2мм 4пр ",100,25,21.74,22,2002,0.5,10.87]
[20021549,"2002-1549","Кл. TOPJOB S 2,5мм2 2пр",50,0,382.3,22,2002,0.5,191.15]
[20021568,"2002-1568","Кл. TOPJOB S 2,5мм2 2пр 2разм.",50,0,"снят с производства",22,2002,0.5,{"$error":"#VALUE!"}]
[20021591,"2002-1591","Торц.пл. TOPJOB S 0,8мм ",100,25,24.76,22,2002,0.5,12.38]
[20021592,"2002-1592","Торц.пл. TOPJOB S 0,8мм ор.",100,25,24.76,22,2002,0.5,12.38]
[20021593,"2002-1593","Раздел.пл. TOPJOB S 2мм",100,25,24.76,22,2002,0.5,12.38]
[20021594,"2002-1594","Раздел.пл. TOPJOB S 2мм",100,25,24.76,22,2002,0.5,12.38]
[51222006,"2002-1601","Кл. TOPJOB S 2,5мм2 2пр ",50,0,125.6,22,2002,0.5,62.8]
[20021602,"2002-1602","Кл. TOPJOB S 2,5мм2 2пр ор.",50,0,130.4,22,2002,0.5,65.2]
[51222009,"2002-1604","Кл. TOPJOB S 2,5мм2 2пр с.",50,0,130.4,22,2002,0.5,65.2]
[20020161,"2002-161","Держ.марк. TOPJOB S 1ур",100,25,11.47,22,2002,0.5,5.7350000000000003]
[51222016,"2002-1611","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,192.6,22,2002,0.5,96.3]
[51207548,"2002-1611/1000-541","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,541.1,22,2002,0.5,270.55]
[51207553,"2002-1611/1000-542","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,541.1,22,2002,0.5,270.55]
[51207554,"2002-1611/1000-836","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,541.1,22,2002,0.5,270.55]
[51239054,"2002-1611/1000-867","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,541.1,22,2002,0.5,270.55]
[51222020,"2002-1661","Кл. TOPJOB S 2,5мм2 2пр держ.",50,0,119,22,2002,0.5,59.5]
[51243255,"2002-1661/999-991","Кл. TOPJOB S 2,5мм2 2пр держ.",1,0,{"$error":"#N/A"},22,2002,0.5,{"$error":"#N/A"}]
[51222022,"2002-1671","Кл. TOPJOB S 2,5мм2 2пр разм.",50,0,125.6,22,2002,0.5,62.8]
[51210502,"2002-1671/401-000","Кл. TOPJOB S 2,5мм2 2пр разм.",50,0,130.4,22,2002,0.5,65.2]
[51222023,"2002-1672","Кл. TOPJOB S 2,5мм2 2пр разм. ор",50,0,130.4,22,2002,0.5,65.2]
[51210503,"2002-1672/401-000","Кл. TOPJOB S 2,5мм2 2пр разм. ор",50,0,133.5,22,2002,0.5,66.75]
[51222026,"2002-1674","Кл. TOPJOB S 2,5мм2 2пр разм.с",50,0,130.4,22,2002,0.5,65.2]
[51210504,"2002-1674/401-000","Кл. TOPJOB S 2,5мм2 2пр разм.с",50,0,133.5,22,2002,0.5,66.75]
[51222038,"2002-1681","Кл. TOPJOB S 2,5мм2 2пр прдх",50,0,125.6,22,2002,0.5,62.8]
[20021691,"2002-1691","Торц.пл. TOPJOB S 1мм 2пр ",100,25,20.53,22,2002,0.5,10.265000000000001]
[20021692,"2002-1692","Торц.пл. TOPJOB S 1мм 2пр ор.",100,25,20.53,22,2002,0.5,10.265000000000001]
[20021701,"2002-1701","Кл. TOPJOB S 2,5мм2 3пр ",50,0,149.19999999999999,22,2002,0.5,74.599999999999994]
[20021702,"2002-1702","Кл. TOPJOB S 2,5мм2 3пр ор.",50,0,153.4,22,2002,0.5,76.7]
[20021704,"2002-1704","Кл. TOPJOB S 2,5мм2 3пр с.",50,0,153.4,22,2002,0.5,76.7]
[20021707,"2002-1707","Кл. TOPJOB S 2,5мм2 разм. РЕ",50,0,270.5,22,2002,0.5,135.25]
[20020171,"2002-171","Стопор для изоляции TOPJOB S ",200,25,7.25,22,2002,0.5,3.625]
[20021711,"2002-1711","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,228.9,22,2002,0.5,114.45]
[51280022,"2002-1711/1000-541","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,576.70000000000005,22,2002,0.5,288.35000000000002]
[51280023,"2002-1711/1000-542","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,576.70000000000005,22,2002,0.5,288.35000000000002]
[51280024,"2002-1711/1000-836","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,576.70000000000005,22,2002,0.5,288.35000000000002]
[51280025,"2002-1711/1000-867","Кл. TOPJOB S 2,5мм2 разм. Прдх",50,0,576.70000000000005,22,2002,0.5,288.35000000000002]
[20020172,"2002-172","Стопор для изоляции TOPJOB S ",200,25,7.25,22,2002,0.5,3.625]
[20021761,"2002-1761","Кл. TOPJOB S 2,5мм2 3пр  держ.",50,0,137.69999999999999,22,2002,0.5,68.849999999999994]
[20021771,"2002-1771","Кл. TOPJOB S 2,5мм2 3пр разм.",50,0,149.19999999999999,22,2002,0.5,74.599999999999994]
[51280019,"2002-1771/401-000","Кл. TOPJOB S 2,5мм2 3пр разм.",50,0,152.19999999999999,22,2002,0.5,76.099999999999994]
[20021772,"2002-1772","Кл. TOPJOB S 2,5мм2 3пр разм. ор",50,0,153.4,22,2002,0.5,76.7]
[51280020,"2002-1772/401-000","Кл. TOPJOB S 2,5мм2 3пр разм. Ор",50,0,156.4,22,2002,0.5,78.2]
[20021774,"2002-1774","Кл. TOPJOB S 2,5мм2 3пр разм. с.",50,0,153.4,22,2002,0.5,76.7]