{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["лист 1","лист 2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"лист 1","index":0,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
["Наименование ",null,"Вес","Окраска за 1 т."]
["Изготовление и монтаж колонн из: "]
["-двутавр 25К1 по СТО АСЧМ 20-93 С255","т",1,{"$f":"MyF(A4,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":23.8}]
["-швеллер [24У по ГОСТ 8240-93 С245","т",5,{"$f":"MyF(A5,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":35}]
["- уголки L125x8 по ГОСТ 8509-93 C245","т",5.4,{"$f":"MyF(A6,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":33}]
["- уголки L50x5 по ГОСТ 8509-93C235","т",7,{"$f":"MyF(A7,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":52}]
["- t24 по ГОСТ 8200-70 С245","т",1.5,{"$f":"MyF(A8,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":10.6}]
["- t20 по ГОСТ 8200-70 С245","т",0.3,{"$f":"MyF(A9,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":12.7}]
["- t10 по ГОСТ 8200-70 С255","т",1,{"$f":"MyF(A10,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":25.5}]
["- t8 по ГОСТ 8200-70 С235","т",0.5,{"$f":"MyF(A11,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":31.9}]
["Изготовление и монтаж связей по колоннам из: ",null,null,{"$f":"MyF(A12,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":""}]
["- уголки L100x7 по ГОСТ 8509-93 C245","т",1,{"$f":"MyF(A13,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":37}]
["- t8 по ГОСТ 8200-70 С235","т",2,{"$f":"MyF(A14,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":31.9}]
["Изготовление и монтаж балок путей подвесного транспорта из:",null,null,{"$f":"MyF(A15,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":""}]
["-двутавр 30М по СТО АСЧМ 20-93 С255","т",2,{"$f":"MyF(A16,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":22.3}]
["- t10 по ГОСТ 8200-70 С255","т",1,{"$f":"MyF(A17,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":25.5}]
["- t16 по ГОСТ 8200-70 С255","т",0.5,{"$f":"MyF(A18,'лист 2'!$A$3:$A$67,'лист 2'!$C$3:$C$67)","v":15.9}]

{"sheet":"лист 2","index":1,"n_rows":67,"n_cols":3,"rows_kept":67,"cut":false,"hidden":false,"merged":[[0,1,1,1]]}
[null,"Ед. изм."]
["Элемент",null,"Площадь поверхности 1 т элемента, м²"]
["20K1","т",28.7]
["20K2","т",24]
["25К1","т",23.8]
["25K1","т",23.8]
["30K1","т",20.6]
["35K1","т",19.100000000000001]
["12Б1","т",57.5]
["20Б1","т",37.6]
["20Ш1","т",32.9]
["25Ш1","т",27]
["30Ш1","т",24.5]
["18М","т",27.9]
["24М","т",24]
["30М","т",22.3]
["10У","т",44.2]
["12У","т",43.3]
["14У","т",41.5]
["16У","т",40.799999999999997]
["18У","т",39.299999999999997]
["20У","т",38]
["22У","т",36.700000000000003]
["24У","т",35]
["27У","т",33.200000000000003]
["30У","т",31.4]
["100x60x4","т",68.3]
["120x60x5","т",55.1]
["140x60x5","т",54.8]
["100х5","т",27.8]
["120х5","т",27.4]
["140х5","т",27.1]
["160х5","т",26.9]
["L25x3","т",86.5]
["L50x5","т",52]
["L63x5","т",52]
["L75x6","т",44]
["L90x6","т",44]
["L90x7","т",37]
["L100x7","т",37]
["L110x7","т",37]
["L125x8","т",33]
["L140x9","т",29.5]
["L125x80x8","т",33]
["-t4","т",63.7]
["-t6","т",42.5]
["-t8","т",31.9]
["-t10","т",25.5]
["-t12","т",21.2]
["-t14","т",18.2]
["-t16","т",15.9]
["-t20","т",12.7]
["-t24","т",10.6]
["ПВ-506","т",183.82]
["35x3","т",46.43]
["57x3","т",44.82]
["89x5","т",26.99]
["102x5","т",26.79]
["108x5","т",26.71]
["127x5","т",26.52]
["159x5","т",26.31]
["168x5","т",26.26]
["219x6","т",21.83]
["219x8","т",16.53]
["273x6","т",21.71]
["325x6","т",21.63]
["377x6","т",21.57]