{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["УР","Б"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"УР","index":0,"n_rows":35,"n_cols":3,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
[null,"Дата:",{"$f":"C3+C2","v":"2016-02-19"}]
[null,"Рапорт №",2]
[null,"Начало бурения:","2016-02-17"]
[]
["№","Наименование ХР","Расход, кг"]
[1,"Сода каустическая",500]
[2,"Сода кальц-ная"]
[3,"Известь",90]
[4,"Бикарбонат натрия"]
[5,"Кислота лимонная"]
[6,"BENTEX"]
[7,"SABOXAN"]
[8,"SB PAC LV"]
[9,"SB PAC HV"]
[10,"КМК"]
[11,"ФХЛС"]
[12,"КССБ"]
[13,"Праестол 2500"]
[14,"GLIDEX m.3.1"]
[15,"SB DEFOAM",25]
[16,"SB CIDE"]
[17,"SURFEX"]
[18,"SB CARB 60"]
[19,"SB CARB 100"]
[20,"SB ALK"]
[21,"Войлок (кошма)"]
[22,"Волокно кордное"]
[23,"Крошка резинвая"]
[24,"SB LCC"]
[25,"Mixnute"]
[26,"Графит"]
[27,"SB GN"]
[28,"Окись цинка"]
[29,"SB CARB 5 мкм"]
[30,"Слюда КФП-5"]

{"sheet":"Б","index":1,"n_rows":33,"n_cols":17,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,1,2,1],[1,0,2,0],[1,2,1,16]]}
[]
["№","Наименование ХР","Расход, кг"]
[null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[1,"Сода каустическая"]
[2,"Сода кальц-ная"]
[3,"Известь"]
[4,"Бикарбонат натрия"]
[5,"Кислота лимонная"]
[6,"BENTEX"]
[7,"SABOXAN"]
[8,"SB PAC LV"]
[9,"SB PAC HV"]
[10,"КМК"]
[11,"ФХЛС"]
[12,"КССБ"]
[13,"Праестол 2500"]
[14,"GLIDEX m.3.1"]
[15,"SB DEFOAM"]
[16,"SB CIDE"]
[17,"SURFEX"]
[18,"SB CARB 60"]
[19,"SB CARB 100"]
[20,"SB ALK"]
[21,"Войлок (кошма)"]
[22,"Волокно кордное"]
[23,"Крошка резинвая"]
[24,"SB LCC"]
[25,"Mixnute"]
[26,"Графит"]
[27,"SB GN"]
[28,"Окись цинка"]
[29,"SB CARB 5 мкм"]
[30,"Слюда КФП-5"]