{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["какой-то лист"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"какой-то лист","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[[15,0,15,7],[16,0,16,7],[7,0,7,7],[8,0,8,7],[9,0,9,7],[11,0,11,7],[12,0,12,7],[10,0,10,7]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[1,"Сваи из труб ГОСТ 8732-78 из стали 09Г2С 159х8 мм","т",null,null,null,null,null,55758.86,{"$f":"I20*J$17","v":0},{"$f":"J20*D20","v":0}]
[{"$f":"IF($B21=\"\",\"\",MAX($A$20:A20)+1)","v":2},"Трубы для свай ГОСТ 8732-78 из стали 09Г2С 219х8 мм","т",7.97,null,null,null,null,55758.86,{"$f":"I21*J$17","v":0},{"$f":"J21*D21","v":0}]
[{"$f":"IF($B22=\"\",\"\",MAX($A$20:A21)+1)","v":3},"Термостабилизатор грунтов марки ТК 32/12М5 А, ТУ3644-003-54098700-2006","шт",null,null,null,null,null,15596.97,0,0]
[{"$f":"IF($B23=\"\",\"\",MAX($A$20:A22)+1)","v":4},"М/к заглушек из сортовой стали С245","т",null,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B24=\"\",\"\",MAX($A$20:A23)+1)","v":5},"М/к термометрической трубки 57х3,5 мм, сталь В20","т",5.3999999999999999E-2,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B25=\"\",\"\",MAX($A$20:A24)+1)","v":6},"Смотровая труба Д-57х3,5мм","т",7.3999999999999996E-2,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B26=\"\",\"\",MAX($A$20:A25)+1)","v":7},"Колодец из труб диаметром 159х8, ст.Б20","т",null,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B27=\"\",\"\",MAX($A$20:A26)+1)","v":8},"Крышка колодца из труб диаметром 70х3,5мм ст. Б20","т",1E-3,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B28=\"\",\"\",MAX($A$20:A27)+1)","v":9},"Крышка колодца из труб диаметром 219х8, ст.Б20","т",6.0000000000000001E-3,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B29=\"\",\"\",MAX($A$20:A28)+1)","v":10},"М/к заглушки температурных трубок из листовой стали, сталь С255","т",null,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B30=\"\",\"\",MAX($A$20:A29)+1)","v":11},"М/к крышек из листовой стали, С245","т",3.0000000000000001E-3,null,null,null,null,72064.39,0,0]
[{"$f":"IF($B31=\"\",\"\",MAX($A$20:A30)+1)","v":12},"Песок для засыпки пазух скважин","м3",0.74,null,null,null,null,768.05,0,0]
[{"$f":"IF($B32=\"\",\"\",MAX($A$20:A31)+1)","v":13},"Цементно-песчаный раствор марки 150 с применением песка из местных карьеров","м3",null,null,null,null,null,12622.94,0,0]
[{"$f":"IF($B33=\"\",\"\",MAX($A$20:A32)+1)","v":14},"Грунт-эмаль СБЭ-111 \"Унипол\" марки \"Б\" ТУ2312-001-59846005-20036","кг",25,null,null,null,null,144.55000000000001,0,0]
[{"$f":"IF($B34=\"\",\"\",MAX($A$20:A33)+1)","v":15},"Эмаль СБЭ-111 \"Унипол\" марки \"Б\" ТУ2312-001-59846005-20036","кг",3,null,null,null,null,144.55000000000001,0,0]
[{"$f":"IF($B35=\"\",\"\",MAX($A$20:A34)+1)","v":16},"Плиты теплоизоляционные из пенополиуретана","м3",0.01,null,null,null,null,2613.77,0,0]
[{"$f":"IF($B36=\"\",\"\",MAX($A$20:A35)+1)","v":17},"Кислород","м3",4.05]
[{"$f":"IF($B37=\"\",\"\",MAX($A$20:A36)+1)","v":18},"Электроды","кг"]
[{"$f":"IF($B38=\"\",\"\",MAX($A$20:A37)+1)","v":19},"Изделия теплоизоляционные","м3",7.0000000000000007E-2]
[{"$f":"IF($B39=\"\",\"\",MAX($A$20:A38)+1)","v":20},"Растворитель","т"]
[{"$f":"IF($B40=\"\",\"\",MAX($A$20:A39)+1)","v":21},"Раствор готовый кладочный цементный, марка 200 (М150)","м3"]
[{"$f":"IF($B41=\"\",\"\",MAX($A$20:A40)+1)","v":22},"Щебень","м3",1.89]