{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["data","result"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"data","index":0,"n_rows":178,"n_cols":7,"rows_kept":178,"cut":false,"hidden":false,"merged":[]}
["Report",null,"xxxxx",null,"xxxx",null,"Осталось 0"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[null,1438,null,null,null,"RING RETAINER","RING RETAINER; RING RETAINER; RING RETAINER; "]
[null,null,null,null,null,"RING SPACER,   .620/.615 OD X.260/.265"]
[null,null,null,null,null,"ID X .188 THK."]
[null,18770,null,null,null,"RING SEAL","RING SEAL; RING SEAL; "]
[null,null,null,null,null,"RING SEAL"]
[null,53384,null,null,null,"GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE","GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE; GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE; "]
[null,null,null,null,null,"GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE"]
[null,54220,null,null,null,"REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC","REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC; REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC; REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC; "]
[null,null,null,null,null,"REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC"]
[null,null,null,null,null,"BOP PUMP"]
[null,60951,null,null,null,"BEARING,ROLLER THRUST,1.752IN ID,2.49IN","BEARING,ROLLER THRUST,1.752IN ID,2.49IN; BEARING,ROLLER THRUST,1.752IN ID,2.49IN; BEARING,ROLLER THRUST,1.752IN ID,2.49IN; BEARING,ROLLER THRUST,1.752IN ID,2.49IN; BEARING,ROLLER THRUST,1.752IN ID,2.49IN; "]
[null,null,null,null,null,"BEARING,ROLLER THRUST:1.752IN ID,2.49IN"]
[null,null,null,null,null,"OD,0.78IN T MODIFIED 1012 STEEL"]
[]
[]
[null,65199,null,null,null,"VALVE,DRAIN,1/4IN NPT M,10000,SS,2064101","VALVE,DRAIN,1/4IN NPT M,10000,SS,2064101; VALVE,DRAIN,1/4IN NPT M,10000,SS,2064101; VALVE,DRAIN,1/4IN NPT M,10000,SS,2064101; "]
[null,null,null,null,null,"VALVE,BLEED,1/4\" NPT MALE,10000psig"]
[null,null,null,null,null,",STAINLESS STEEL"]
[null,65559,null,null,null,"O-RING,12.475ID,0.275W90D,MS-1078,NITR","O-RING,12.475ID,0.275W90D,MS-1078,NITR; O-RING,12.475ID,0.275W90D,MS-1078,NITR; O-RING,12.475ID,0.275W90D,MS-1078,NITR; O-RING,12.475ID,0.275W90D,MS-1078,NITR; "]
[null,null,null,null,null,"O-RING 12.475IN ID,0.275IN W 90D"]
[null,null,null,null,null,"/MS-1078    NITRILE PKG AND QUAL /CIW"]
[null,null,null,null,null,"702645 CROSS SECTION"]
[null,70651,null,null,null,"GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED","GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED; GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED; GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED; GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED; GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED; "]
[null,null,null,null,null,"GLOVES,LEATHER,LIGHT DUTY,PR,SIZE MED"]
[null,null,null,null,null,",MATL GOATSKIN,MFR MEMPHIS,MFR NO"]
[null,null,null,null,null,"3611M."]
[]
[null,70960,null,null,null,"ROPE,MANILLA FIBRE,3/8 X 100 FEET","ROPE,MANILLA FIBRE,3/8 X 100 FEET; ROPE,MANILLA FIBRE,3/8 X 100 FEET; ROPE,MANILLA FIBRE,3/8 X 100 FEET; "]
[null,null,null,null,null," ROPE, MANILLA FIBRE, 3/18, 100 FEET PER"]
[null,null,null,null,null,"ROLL, MFR GUARDIAN"]
[null,71425,null,null,null,"TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479","TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479; TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479; TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479; TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479; "]
[null,null,null,null,null,"TAPE,DUCT,SILVER,2\" ROLL"]
[null,null,null,null,null,"PN: 208479"]
[null,null,null,null,null,"MFR: SHURTAPE"]
[null,84042,null,null,null,"XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB","XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB; "]
[null,null,null,null,null,"CROSSOVER, 20.000 BY 13.375 INCH OUTSIDE"]
[null,null,null,null,null,"DIAMETER, 166.40 BY 68.00"]
[null,null,null,null,null,"POUNDS PER FOOT, GRADE N-80, SEAMLESS,"]
[null,null,null,null,null,"VETCO RL-4S BY BUTTRESS (TORQUE"]
[null,null,null,null,null,"POSITION SPECIFICATIONS, TIN PLATED),"]
[null,null,null,null,null,"BOX BY BOX, 0.812 BY 0.480 INCH"]
[null,null,null,null,null,"WALL THICKNESS, API SPECIFICATION 5L AND"]
[null,null,null,null,null,"5CT."]
[null,84179,null,null,null,"SET,FITTING,RIG UP,HALLIBURTON,101300553","SET,FITTING,RIG UP,HALLIBURTON,101300553; SET,FITTING,RIG UP,HALLIBURTON,101300553; SET,FITTING,RIG UP,HALLIBURTON,101300553; SET,FITTING,RIG UP,HALLIBURTON,101300553; SET,FITTING,RIG UP,HALLIBURTON,101300553; SET,FITTING,RIG UP,HALLIBURTON,101300553; "]
[null,null,null,null,null,"SET, FITTING, RIG UP, MANUFACTURER NOVA,"]
[null,null,null,null,null,"PART NUMBER RUF1, SOLD BY"]
[null,null,null,null,null,"HALLIBURTON AS PART NUMBER 101300553,"]
[null,null,null,null,null,"316LSS FITTINGS FOR SHIPPING,"]
[null,null,null,null,null,"TESTING, AND RIGGING UP CONTROL LINES."]
[null,84282,null,null,null,"CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC","CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC; "]
[null,null,null,null,null,"COUPLING,CASING,7\",29PPF,VAM TOP HC BOX"]
[]
["Report",null,"xxxxx",null,"xxxxx"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"1CR-80,SEAMLESS"]
[null,84367,null,null,null,"BSG,WEAR,11,CAMERON,2206525-01,IC-2-L","BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; BSG,WEAR,11,CAMERON,2206525-01,IC-2-L; "]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206525-"]
[null,null,null,null,null,"01, 6.545 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TYPE IC-2-L BOWL PROFILE, FOR"]
[null,null,null,null,null,"CUTTINGS WELLHEAD PROTECTION."]
[null,84368,null,null,null,"BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL","BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL; "]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206527-"]
[null,null,null,null,null,"01, 9.000 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TYPE IC-2 BOWL PROFILE, FOR"]
[null,null,null,null,null,"CUTTINGS WELLHEAD PROTECTION."]
[null,84369,null,null,null,"BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL","BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL; "]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206527-"]
[null,null,null,null,null,"01, 8.785 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TUBING SPOOL, FOR ERD"]
[null,null,null,null,null,"WELLHEAD PROTECTION."]
[null,84417,null,null,null,"TBG,COILED,1/4,HALLIBURTON,101300458","TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; TBG,COILED,1/4,HALLIBURTON,101300458; "]
[null,null,null,null,null,"TUBING, COILED, 0.250 INCH, MANUFACTURER"]
[null,null,null,null,null,"HALLIBURTON, PART NUMBER 101300458,"]
[null,null,null,null,null,"GRADE INCONEL 825, CONDUCTOR,"]
[null,null,null,null,null,"ENCAPSULATED WITH 80 MILS OF CP-1, 0.049"]
[null,null,null,null,null,"INCH WALL THICKNESS, INCLUDES SPOOL TO"]
[null,null,null,null,null,"HOLD LENGTH OF CONTROL LINE."]
[null,84439,null,null,null,"CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3","CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3; "]
[null,null,null,null,null,"CASING, 13.375 INCH OUTSIDE DIAMETER,"]
[null,null,null,null,null,"68.00 POUNDS PER FOOT, GRADE L-80,"]
[null,null,null,null,null," SEAMLESS, BUTTRESS THREADED AND"]
[null,null,null,null,null,"COUPLED, BOX BY PIN, RANGE 3, 0.480"]
[null,null,null,null,null,"INCH WALL THICKNESS, API SPECIFICATION"]
[null,null,null,null,null,"5CT."]
[null,92341,null,null,null,"NUT,HEAVY HEX,1IN -8,GR 2H,ZN PLATED","NUT,HEAVY HEX,1IN -8,GR 2H,ZN PLATED; NUT,HEAVY HEX,1IN -8,GR 2H,ZN PLATED; NUT,HEAVY HEX,1IN -8,GR 2H,ZN PLATED; "]
[null,null,null,null,null,"NUT,HEAVY HEXAGONAL,1\"-8,GRADE 2H.ZINC"]
[null,null,null,null,null,"PLATED"]
[null,123343,null,null,null,"PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"","PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"; PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"; PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"; PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"; PIN,DOWEL,021812-14,CAMERON,0.434x2.375\"; "]
[null,null,null,null,null,"PIN,DOWEL,021812-14,CAMERON,0.434x2.375\""]
[null,null,null,null,null,"Block & Gate Valve"]
[null,null,null,null,null,"ANGOLA STOCK \"ZZ-OBSOLETE-SEE IPES"]
[null,null,null,null,null,"60145\""]
[null,123384,null,null,null,"O-RING,676936-13,CAMERON","O-RING,676936-13,CAMERON; O-RING,676936-13,CAMERON; "]
[null,129710,null,null,null,"PIN,SPIRAL,689623-02,CAMERON,0.156x2\"","PIN,SPIRAL,689623-02,CAMERON,0.156x2\"; "]
[null,150856,null,null,null,"HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM","HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM; "]
[null,null,null,null,null,"HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM,"]
[null,null,null,null,null,"MFR HAYS CHEMICAL, MUST BE ACCOMPANIED"]
[null,null,null,null,null,"WITH CURRENT MSDS SHEET TO BE ACCEPTED"]
[]
[]
[null,164924,null,null,null,"VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø","VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø; "]
[null,null,null,null,null,"OVERALL HEIGHT : 1200mm"]
[]
["Report",null,"xxxxx",null,"xxxx"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"WEIGHT         : 20 KGS"]
[]
[null,169689,null,null,null,"TOOL,INSERTING,BPV,040800-01,CAMERON","TOOL,INSERTING,BPV,040800-01,CAMERON; TOOL,INSERTING,BPV,040800-01,CAMERON; TOOL,INSERTING,BPV,040800-01,CAMERON; TOOL,INSERTING,BPV,040800-01,CAMERON; TOOL,INSERTING,BPV,040800-01,CAMERON; TOOL,INSERTING,BPV,040800-01,CAMERON; "]
[null,null,null,null,null,"TOOL FOR 2\" AND LARGER BPV'S-STANDARD"]
[null,null,null,null,null,"SERVICE FOR LUBR.TYPE \"S-10\""]
[null,null,null,null,null,"WITH 1 1/8\" POLISHED ROD FOR USE WITH"]
[null,null,null,null,null,"BACK PRESS.VALVES."]
[]
[null,169792,null,null,null,"GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#","GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#; GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#; GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#; GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#; "]
[null,null,null,null,null,"CASE MATERIAL : STAINLESS STEEL"]
[null,null,null,null,null,"CONNECTION    : 1/4\" LBM"]
[null,null,null,null,null,"FILL FLUID    : GLYCERINE"]
[null,173054,null,null,null,"TRUVIS, 25KG SACK","TRUVIS, 25KG SACK; TRUVIS, 25KG SACK; "]
[null,null,null,null,null,"TRUVIS, 25KG SACK"]
[null,173158,null,null,null,"SCREW,DRIVE,2034002-06,CAMERON","SCREW,DRIVE,2034002-06,CAMERON; SCREW,DRIVE,2034002-06,CAMERON; SCREW,DRIVE,2034002-06,CAMERON; SCREW,DRIVE,2034002-06,CAMERON; "]
[null,null,null,null,null,"MATERIAL : AISI 4340 OR 4140"]
[]
[]
[null,177164,null,null,null,"BIT,DRILL,174 MGSSH+C,SMI.INT,17 1/2\"","BIT,DRILL,174 MGSSH+C,SMI.INT,17 1/2\"; BIT,DRILL,174 MGSSH+C,SMI.INT,17 1/2\"; "]
[null,179313,null,null,null,"COLLAR,STOP,18-5/8","COLLAR,STOP,18-5/8; "]
[null,179391,null,null,null,"KEY, VERTICAL ANTI-ROTATION, (SHORT)","KEY, VERTICAL ANTI-ROTATION, (SHORT); KEY, VERTICAL ANTI-ROTATION, (SHORT); KEY, VERTICAL ANTI-ROTATION, (SHORT); KEY, VERTICAL ANTI-ROTATION, (SHORT); KEY, VERTICAL ANTI-ROTATION, (SHORT); "]
[null,null,null,null,null,"KEY, VERTICAL ANTI-ROTATION, (SHORT),FOR"]
[null,null,null,null,null,"20\" S - 60/MT CONNECTORS"]
[]
[]
[null,216590,null,null,null,"M-DTE 832 DRUM-M 208L","M-DTE 832 DRUM-M 208L; M-DTE 832 DRUM-M 208L; "]
[null,null,null,null,null,"M-DTE 832 DRUM-M 208L"]
[null,217058,null,null,null,"CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD","CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD; "]
[null,null,null,null,null,"CENTRALIZER, 9-5/8\", LO-DRAG, ROLLER,"]
[null,null,null,null,null,"12.030\" OD."]
[null,null,null,null,null,"(MECHANICAL FRICTION & WEAR REDUCTION"]
[null,null,null,null,null,"CENTRALIZER SYSTEM FOR"]
[null,null,null,null,null,"FOR 12-1/4\" HOLE)"]
[null,218085,null,null,null,"DRILLBIT, 8.1/2\"","DRILLBIT, 8.1/2\"; DRILLBIT, 8.1/2\"; DRILLBIT, 8.1/2\"; DRILLBIT, 8.1/2\"; "]
[null,null,null,null,null,"DRILLBIT, 8.1/2\""]
[]
[]
[null,219968,null,null,null,"VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S","VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S; "]
[null,null,null,null,null,"MANOMETERABSPERRVENTIL"]
[null,null,null,null,null,"Typ           : PN700"]
[null,null,null,null,null,"Werkstoff     : AUSFUEHRUNG FUER H2S"]
[null,null,null,null,null,"GEMAESS NACE MR-01-75"]
[]
[null,null,null,null,null,"Chemische und physikalische"]
[null,null,null,null,null,"Werkstoffanalysen, Härteprüfung und"]
[null,null,null,null,null,"hydrostatischer Drucktest sind gemäß der"]
[null,null,null,null,null,"zutreffenden Hersteller-Spezifikationen"]
[null,null,null,null,null,"durchzuführen und mit"]
[null,null,null,null,null,"Abnahmeprüfzeugnissen nach  EN 10204/3.1"]
[null,null,null,null,null,"zu belegen."]

{"sheet":"result","index":1,"n_rows":178,"n_cols":7,"rows_kept":178,"cut":false,"hidden":false,"merged":[]}
["Report",null,"xxxxx",null,"xxxx"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[null,1438,null,null,null,"RING RETAINER","RING SPACER,   .620/.615 OD X.260/.265; ID X .188 THK."]
[]
[]
[null,18770,null,null,null,"RING SEAL","RING SEAL"]
[]
[null,53384,null,null,null,"GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE","GRUBSCREW, 1/4\"UNC x 1/4\", H2S SERVICE"]
[]
[null,54220,null,null,null,"REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC","REGULATOR, AIR f/ AIR DRIVEN HYDRAULIC; BOP PUMP"]
[]
[]
[null,60951,null,null,null,"BEARING,ROLLER THRUST,1.752IN ID,2.49IN"]
[null,null,null,null,null,"BEARING,ROLLER THRUST:1.752IN ID,2.49IN"]
[null,null,null,null,null,"OD,0.78IN T MODIFIED 1012 STEEL"]
[]
[]
[null,65199,null,null,null,"VALVE,DRAIN,1/4IN NPT M,10000,SS,2064101"]
[null,null,null,null,null,"VALVE,BLEED,1/4\" NPT MALE,10000psig"]
[null,null,null,null,null,",STAINLESS STEEL"]
[null,65559,null,null,null,"O-RING,12.475ID,0.275W90D,MS-1078,NITR"]
[null,null,null,null,null,"O-RING 12.475IN ID,0.275IN W 90D"]
[null,null,null,null,null,"/MS-1078    NITRILE PKG AND QUAL /CIW"]
[null,null,null,null,null,"702645 CROSS SECTION"]
[null,70651,null,null,null,"GLOVE,LEATHER,LIGHTWEIGHT,GOATSKIN.MED"]
[null,null,null,null,null,"GLOVES,LEATHER,LIGHT DUTY,PR,SIZE MED"]
[null,null,null,null,null,",MATL GOATSKIN,MFR MEMPHIS,MFR NO"]
[null,null,null,null,null,"3611M."]
[]
[null,70960,null,null,null,"ROPE,MANILLA FIBRE,3/8 X 100 FEET"]
[null,null,null,null,null," ROPE, MANILLA FIBRE, 3/18, 100 FEET PER"]
[null,null,null,null,null,"ROLL, MFR GUARDIAN"]
[null,71425,null,null,null,"TAPE,DUCT,2IN WIDE,SILVER,ROLL,208479"]
[null,null,null,null,null,"TAPE,DUCT,SILVER,2\" ROLL"]
[null,null,null,null,null,"PN: 208479"]
[null,null,null,null,null,"MFR: SHURTAPE"]
[null,84042,null,null,null,"XO,20X13-3/8,166.4X68,N80,RL4SXBTCTP,BXB"]
[null,null,null,null,null,"CROSSOVER, 20.000 BY 13.375 INCH OUTSIDE"]
[null,null,null,null,null,"DIAMETER, 166.40 BY 68.00"]
[null,null,null,null,null,"POUNDS PER FOOT, GRADE N-80, SEAMLESS,"]
[null,null,null,null,null,"VETCO RL-4S BY BUTTRESS (TORQUE"]
[null,null,null,null,null,"POSITION SPECIFICATIONS, TIN PLATED),"]
[null,null,null,null,null,"BOX BY BOX, 0.812 BY 0.480 INCH"]
[null,null,null,null,null,"WALL THICKNESS, API SPECIFICATION 5L AND"]
[null,null,null,null,null,"5CT."]
[null,84179,null,null,null,"SET,FITTING,RIG UP,HALLIBURTON,101300553"]
[null,null,null,null,null,"SET, FITTING, RIG UP, MANUFACTURER NOVA,"]
[null,null,null,null,null,"PART NUMBER RUF1, SOLD BY"]
[null,null,null,null,null,"HALLIBURTON AS PART NUMBER 101300553,"]
[null,null,null,null,null,"316LSS FITTINGS FOR SHIPPING,"]
[null,null,null,null,null,"TESTING, AND RIGGING UP CONTROL LINES."]
[null,84282,null,null,null,"CPLG,7IN,29PPF,1CR-80,SMLS,VAMTOPHC","COUPLING,CASING,7\",29PPF,VAM TOP HC BOX; 1CR-80,SEAMLESS"]
[]
[]
["Report",null,"xxxxx",null,"xxxxx"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[]
[null,84367,null,null,null,"BSG,WEAR,11,CAMERON,2206525-01,IC-2-L"]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206525-"]
[null,null,null,null,null,"01, 6.545 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TYPE IC-2-L BOWL PROFILE, FOR"]
[null,null,null,null,null,"CUTTINGS WELLHEAD PROTECTION."]
[null,84368,null,null,null,"BSG,WEAR,11,CAMERON,2206527-01,IC-2 BOWL"]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206527-"]
[null,null,null,null,null,"01, 9.000 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TYPE IC-2 BOWL PROFILE, FOR"]
[null,null,null,null,null,"CUTTINGS WELLHEAD PROTECTION."]
[null,84369,null,null,null,"BSG,WEAR,11,CAMERON,2206531-01,TBG SPOOL"]
[null,null,null,null,null,"BUSHING, WEAR, 11.000 INCH, MANUFACTURER"]
[null,null,null,null,null,"CAMERON, PART NUMBER 2206527-"]
[null,null,null,null,null,"01, 8.785 INCH MINIMUM BORE, FOR USE"]
[null,null,null,null,null,"WITH TUBING SPOOL, FOR ERD"]
[null,null,null,null,null,"WELLHEAD PROTECTION."]
[null,84417,null,null,null,"TBG,COILED,1/4,HALLIBURTON,101300458"]
[null,null,null,null,null,"TUBING, COILED, 0.250 INCH, MANUFACTURER"]
[null,null,null,null,null,"HALLIBURTON, PART NUMBER 101300458,"]
[null,null,null,null,null,"GRADE INCONEL 825, CONDUCTOR,"]
[null,null,null,null,null,"ENCAPSULATED WITH 80 MILS OF CP-1, 0.049"]
[null,null,null,null,null,"INCH WALL THICKNESS, INCLUDES SPOOL TO"]
[null,null,null,null,null,"HOLD LENGTH OF CONTROL LINE."]
[null,84439,null,null,null,"CSG,13-3/8IN,68PPF,L80,SMLS,BTC,BxP,R3"]
[null,null,null,null,null,"CASING, 13.375 INCH OUTSIDE DIAMETER,"]
[null,null,null,null,null,"68.00 POUNDS PER FOOT, GRADE L-80,"]
[null,null,null,null,null," SEAMLESS, BUTTRESS THREADED AND"]
[null,null,null,null,null,"COUPLED, BOX BY PIN, RANGE 3, 0.480"]
[null,null,null,null,null,"INCH WALL THICKNESS, API SPECIFICATION"]
[null,null,null,null,null,"5CT."]
[null,92341,null,null,null,"NUT,HEAVY HEX,1IN -8,GR 2H,ZN PLATED"]
[null,null,null,null,null,"NUT,HEAVY HEXAGONAL,1\"-8,GRADE 2H.ZINC"]
[null,null,null,null,null,"PLATED"]
[null,123343,null,null,null,"PIN,DOWEL,021812-14,CAMERON,0.434x2.375\""]
[null,null,null,null,null,"PIN,DOWEL,021812-14,CAMERON,0.434x2.375\""]
[null,null,null,null,null,"Block & Gate Valve"]
[null,null,null,null,null,"ANGOLA STOCK \"ZZ-OBSOLETE-SEE IPES"]
[null,null,null,null,null,"60145\""]
[null,123384,null,null,null,"O-RING,676936-13,CAMERON"]
[null,129710,null,null,null,"PIN,SPIRAL,689623-02,CAMERON,0.156x2\""]
[null,150856,null,null,null,"HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM"]
[null,null,null,null,null,"HYPOCHLORITE, SODIUM, 10-15%, 5L DRUM,"]
[null,null,null,null,null,"MFR HAYS CHEMICAL, MUST BE ACCOMPANIED"]
[null,null,null,null,null,"WITH CURRENT MSDS SHEET TO BE ACCEPTED"]
[]
[]
[null,164924,null,null,null,"VICE,PIPE,1456-0106,LUNA,MAX.PIPE 5\"Ø"]
[null,null,null,null,null,"OVERALL HEIGHT : 1200mm"]
[]
["Report",null,"xxxxx",null,"xxxx"]
["User",null,"xxxxx"]
["Date",null,"2016-12-27","22:34:00"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"WEIGHT         : 20 KGS"]
[]
[null,169689,null,null,null,"TOOL,INSERTING,BPV,040800-01,CAMERON"]
[null,null,null,null,null,"TOOL FOR 2\" AND LARGER BPV'S-STANDARD"]
[null,null,null,null,null,"SERVICE FOR LUBR.TYPE \"S-10\""]
[null,null,null,null,null,"WITH 1 1/8\" POLISHED ROD FOR USE WITH"]
[null,null,null,null,null,"BACK PRESS.VALVES."]
[]
[null,169792,null,null,null,"GAUGE,PRESSURE,ENPB-G,McD.CON,4\",0-3000#"]
[null,null,null,null,null,"CASE MATERIAL : STAINLESS STEEL"]
[null,null,null,null,null,"CONNECTION    : 1/4\" LBM"]
[null,null,null,null,null,"FILL FLUID    : GLYCERINE"]
[null,173054,null,null,null,"TRUVIS, 25KG SACK"]
[null,null,null,null,null,"TRUVIS, 25KG SACK"]
[null,173158,null,null,null,"SCREW,DRIVE,2034002-06,CAMERON"]
[null,null,null,null,null,"MATERIAL : AISI 4340 OR 4140"]
[]
[]
[null,177164,null,null,null,"BIT,DRILL,174 MGSSH+C,SMI.INT,17 1/2\""]
[null,179313,null,null,null,"COLLAR,STOP,18-5/8"]
[null,179391,null,null,null,"KEY, VERTICAL ANTI-ROTATION, (SHORT)"]
[null,null,null,null,null,"KEY, VERTICAL ANTI-ROTATION, (SHORT),FOR"]
[null,null,null,null,null,"20\" S - 60/MT CONNECTORS"]
[]
[]
[null,216590,null,null,null,"M-DTE 832 DRUM-M 208L"]
[null,null,null,null,null,"M-DTE 832 DRUM-M 208L"]
[null,217058,null,null,null,"CENTRALIZER,9-5/8,LO-DRAG,12.030IN OD"]
[null,null,null,null,null,"CENTRALIZER, 9-5/8\", LO-DRAG, ROLLER,"]
[null,null,null,null,null,"12.030\" OD."]
[null,null,null,null,null,"(MECHANICAL FRICTION & WEAR REDUCTION"]
[null,null,null,null,null,"CENTRALIZER SYSTEM FOR"]
[null,null,null,null,null,"FOR 12-1/4\" HOLE)"]
[null,218085,null,null,null,"DRILLBIT, 8.1/2\""]
[null,null,null,null,null,"DRILLBIT, 8.1/2\""]
[]
[]
[null,219968,null,null,null,"VENT-MANO_1/2NPT-FEMX1/2NPT_PN700_H2S"]
[null,null,null,null,null,"MANOMETERABSPERRVENTIL"]
[null,null,null,null,null,"Typ           : PN700"]
[null,null,null,null,null,"Werkstoff     : AUSFUEHRUNG FUER H2S"]
[null,null,null,null,null,"GEMAESS NACE MR-01-75"]
[]
[null,null,null,null,null,"Chemische und physikalische"]
[null,null,null,null,null,"Werkstoffanalysen, Härteprüfung und"]
[null,null,null,null,null,"hydrostatischer Drucktest sind gemäß der"]
[null,null,null,null,null,"zutreffenden Hersteller-Spezifikationen"]
[null,null,null,null,null,"durchzuführen und mit"]
[null,null,null,null,null,"Abnahmeprüfzeugnissen nach  EN 10204/3.1"]
[null,null,null,null,null,"zu belegen."]