{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["выборка","Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"выборка","index":0,"n_rows":268,"n_cols":16,"rows_kept":268,"cut":false,"hidden":false,"merged":[]}
[]
["надо, чтобы не проставлять самому диаметры по фланцам, чтобы формулой в тексте находить 1\" , 10\" 16\" 18\"  1/2\"и рядом в ячейке писалось 1 , 10 16 18 0,5 где есть 1/2 чтоб было в другой ячеке стало 0,5\nИ также чтоб можно было и по классам сделать тесть Class 150 Class 1500 Class 900 Class 600 Class 2500 и на против в другой ячейке проставлялись просто цифры без какого либо текста\n",null,null,"Здесь Диаметр Фланца \"","Здесь класс"]
["Названия строк","Сумма по полю Кол-во",null,null,null,null,null,null,{"$f":"COUNTA(D4:D268)","v":265},{"$f":"COUNTA(E4:E268)","v":265}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 1500, RJ, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",2,1,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A4),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":1},{"$f":"--class($A4)","v":1500},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A4),{150,300,600,900,1500,2500})","v":1500},null,null,{"$f":"COUNT(D4:D268)","v":264},{"$f":"COUNT(E4:E268)","v":262}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket ,stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",7,2,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A5),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":1},{"$f":"--class($A5)","v":150},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A5),{150,300,600,900,1500,2500})","v":150},null,null,{"$f":"I4/I3","v":0.99622641509433962},{"$f":"J4/J3","v":0.98867924528301887}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 1500, RJ, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,3,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A6),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 1500, RJ, pipe con. 33.4x9.09, in complete with gasket,  stud  bolts, hex.  nuts,  A105",5,4,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A7),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 900, RJ, pipe con. 33.4x9.09, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",1,5,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A8),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 1\" with companion flange, WN, Class 900, RJ, pipe con. 33.4x9.09, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",5,6,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A9),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 10\", with companion flange, WN, Class 150, RF, pipe con. 273x6.35, in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR 0175 / ISO 15156",1,7,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A10),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 10\", with companion flange, WN, Class 150, RF, pipe con. 273x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",6,8,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A11),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 10\", with companion flange, WN, Class 150, RF, pipe con. 273x6.35,in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,9,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A12),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 10\",with companion flange, WN, Class 150, RF, pipe con. 273x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,10,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A13),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 16\" with companion flange, WN, Class 150, RF, pipe con. 406.4x7.92, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,11,16,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A14),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1/2\", WN, Class 1500 Lbs RJ pipe con. 21.3x3.73, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,93,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A15),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1/2\",with companion flange, WN, Class 150, RF, pipe con. 21.3x4.78, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175/ISO 15156",1,94,0.5,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A16),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1/2'', with companion flange, WN, Class 1500, RJ, pipe con. 21.3x4.78, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,95,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A17),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1/2'', with companion flange, WN, pipe con. 21.3x7.47, Class 1500, RJ, in complete with gaskets, stud bolt,hex. nut, A105",1,96,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A18),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1/2'', with companion flange, WN, pipe con. 21.3x7.47, Class 1500, RJ, in complete with gaskets, stud bolt,hex. nut, A105",11,97,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A19),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,17,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A20),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket, stud bolts, hex. nuts, A105, NACE MR 0175 / ISO 15156",1,18,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A21),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",5,19,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A22),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 150, RJ, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",15,20,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A23),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 1500, RJ, pipe con. 60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,21,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A24),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 1500, RJ, pipe con. 60.3x8.74, in complete with gasket, stud bolts, hex. nuts, A105",5,22,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A25),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 2500, RJ, pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,   A 694 grade F60",3,23,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A26),{150,300,600,900,1500,2500})","v":2500}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 2500, RJ, pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,  A 694 grade F60",1,24,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A27),{150,300,600,900,1500,2500})","v":2500}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 900, RJ, pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2 , NACE MR0175/ISO 15156",1,25,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A28),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 900, RJ, pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR0175/ISO 15156",1,26,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A29),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 900, RJ, pipe con. 60.3x11.07,in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR0175/ISO 15156",2,27,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A30),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 900, RJ, pipe con. 60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,28,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A31),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 2\" with companion flange, WN, Class 900, RJ, pipe con. 60.3x8.74, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",10,29,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A32),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x3.91, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,30,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A33),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x3.91, in complete with gaskets, stud bolt, hex. nut, A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",2,31,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A34),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,32,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A35),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 20'' with companion flange, WN, Class 900, RJ, pipe con. 509.0x32.54, in complete with gasket,  stud  bolts, hex.  nuts, A350 LF2, NACE MR 0175/ISO 15156. ",1,33,20,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A36),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 20'', with companion flange, WN, Class 900, RJ, pipe con. 509.0x32.54, in complete with gaskets, stud bolt, hex nuts, A350 LF2, NACE MR 0175/ISO 15156. ",1,34,20,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A37),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, pipe con. 88.9x3.05, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L, (Dual Grade Certified) NACE MR 0175 / ISO 15156",2,35,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A38),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with  gasket, stud bolts,  hex. nuts,  A105, NACE MR0175/ISO 15156",1,36,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A39),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,37,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A40),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with  gasket, stud bolts,  hex. nuts,  A105, NACE MR0175/ISO 15156",1,38,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A41),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, RJ, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",4,39,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A42),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 150, RJ, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",3,40,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A43),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 600, RJ, pipe con.88.9x7.62, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,41,3,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A44),{150,300,600,900,1500,2500})","v":600}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 600, RJ, pipe con.88.9x7.62, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,42,3,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A45),{150,300,600,900,1500,2500})","v":600}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 900, RJ, pipe con. 88.9x11.13 in complete with gasket , stud bolts, hex. nuts, A350 LF2, NACE MR0175/ISO 15156",1,43,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A46),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 900, RJ, pipe con. 88.9x11.13 in complete with gasket , stud bolts, hex. nuts, A350 LF2, NACE MR0175/ISO 15156",1,44,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A47),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 900, RJ, pipe con. 88.9x11.13 in complete with gasket , stud bolts, hex. nuts, A350 LF2, NACE MR0175/ISO 15156",2,45,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A48),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 900, RJ, pipe con. 88.9x15.24, in complete with gasket, studbolts, hex. nuts, A350 LF2, NACE MR0175/ISO 15156",1,46,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A49),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\" with companion flange, WN, Class 900, RJ, pipe con. 88.9x15.24, in complete with gasket, studbolts, hex. nuts, A350 LF2, NACE MR0175/ISO 15156",1,47,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A50),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3\",with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105",7,48,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A51),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3\",with companion flange, WN, Class 900, RJ, pipe con. 88.9x7.62, in complete with gasket,  stud  bolts, hex.  nuts,  A105",9,49,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A52),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 3/4 \"with 1/2\" internal tapered pipe thread,B10,  Class of pressure ANSI 150. Material:  A105 Galvanized to A153",3,50,0.75,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A53),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 3/4'', with companion flange, WN, Class 1500, RJ, pipe con.26.7x5.56, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",2,51,0.75,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A54),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 3”, Class 900, RJ, A350 LF2, 150",2,52,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A55),{150,300,600,900,1500,2500})","v":900}]
["Blind Flange (Фланец глухой) 4\" with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,53,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A56),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 4\" with companion flange, WN, Class 150, RF, pipe con. 114.3х11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,54,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A57),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 4\" with companion flange, WN, Class 150, RF, pipe con. 114.3х11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,55,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A58),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 6\" with companion flange, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",5,56,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A59),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 6\" with companion flange, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket, stud bolts, hex. nuts, A350 LF2, NACE MR 0175 / ISO 15156",2,57,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A60),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 6\" with companion flange, WN, Class 1500, RJ, pipe con. 168.3х21.95, in complete with gasket,  stud  bolts, hex.  nuts,  А350 LF2, NACE MR 0175 / ISO 15156",1,58,6,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A61),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 6\" with companion flange, WN, Class 1500, RJ, pipe con. 168.3х21.95, in complete with gasket,  stud  bolts, hex.  nuts,  А350 LF2, NACE MR 0175 / ISO 15156",1,59,6,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A62),{150,300,600,900,1500,2500})","v":1500}]
["Blind Flange (Фланец глухой) 8\" with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,60,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A63),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,61,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A64),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) 8\",with companion flange, WN, Class 300, RF, pipe con. 219.1x8.18, in complete with gasket,  stud  bolts, hex.  nuts,  A105",3,62,8,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A65),{150,300,600,900,1500,2500})","v":300}]
["Blind Flange (Фланец глухой) DN 3/4\", pressure class ANSI 150, complete with fasteners and spiral-type gaskets, graphite filler 4 mm thick, 3.2 mm thick inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material A350LF2",2,63,0.75,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A66),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) DN 4\", pressure class ANSI 150, complete with fasteners and spiral-type gaskets, graphite filler 4 mm thick, 3.2 mm thick inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material  A105",2,64,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A67),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) DN 4\", pressure class ANSI 150, complete with fasteners and spiral-type gaskets, graphite filler 4 mm thick, 3.2 mm thick inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material A150",1,65,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A68),{150,300,600,900,1500,2500})","v":150}]
["Blind Flange (Фланец глухой) DN1\" ANSI 900, RTJ, ASME B16.5, G23SС, material ASTM A350 LF2, complete with a gasket: Elliptic ring type coupling, mild steel as per ASME B16.20-90 HB max., 1 piece; bolt connections: Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated, 1 package.",2,66,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A69),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":1},{"$f":"--class($A69)","v":900},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A69),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange (Фланец) 1 1/2\", Class 2500, RJ, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,67,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A70),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 1 1/2\", with companion flange, WN, Class 150, RF, pipe con. 48.3x5.08, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,68,1.5,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A71),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1 1/2\", with companion flange, WN, Class 150, RF, pipe con. 48.3x5.08, in complete with gasket, stud bolt, hex. nut, A182 F316L",8,69,1.5,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A72),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1 1/2\", with companion flange, WN, Class 150, RF, pipe con. 48.3x7.14, in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR 0175 / ISO 15156",1,70,1.5,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A73),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1 1/4\", with companion flange, ST NPTF,  Class  300 , RF pipe con. 42.2x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",1,71,1.25,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A74),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 1 1/4\", with companion flange, ST NPTF, Class 150, RF pipe con. 42.2x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",1,72,1.25,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A75),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, ST NPTF, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",1,73,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A76),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, WN, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,74,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A77),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, WN, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,75,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A78),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, WN, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",10,76,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A79),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, WN, Class 150, RF, pipe con. 33.4x6.35, in complete with gasket, stud bolt,hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",25,77,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A80),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\", with companion flange, WN, Class 150, RF, pipe con. 33.4x9.09, in complete with gasket, stud bolt, hex. nuts, А350 LF2, NACE MR 0175/ISO 15156",1,78,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A81),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1\",with companion flange, WN , Class 300 Lbs RF pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105 ",1,79,1,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A82),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 1'', with companion flange, WN, Class 150, RF, pipe con. 33.4x4.55, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,80,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A83),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 1'', with companion flange, WN, Class 300, RF, pipe con. 33.4x4.55, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,81,1,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A84),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 1'', with companion flange, WN, Class 300, RF, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,82,1,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A85),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 1'', with companion flange, WN, Class 600, RJ, pipe con. 33.4x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,83,1,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A86),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 1'', with companion flange, WN, Class 900, RJ pipe con. 33.4x9.09, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",1,84,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A87),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 1'', with companion flange, WN, Class 900, RJ pipe con. 33.4x9.09, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",4,85,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A88),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x6.35, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A182 F316L",2,86,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A89),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x6.35, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A182 F316L",5,87,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A90),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x9.09, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A105",1,88,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A91),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x9.09, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A105",2,89,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A92),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x9.09, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A 694 grade F60",1,90,1,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A93),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x9.09, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A 694 grade F60",3,91,1,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A94),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 1'', with companion flange, WN, pipe con. 33.4x9.09, Class 900, RJ, in complete with gaskets, stud. bolts,hex. nuts, A350 LF2, NACE MR 0175/ISO 15156",1,92,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A95),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 10\",  with companion flange, and  spectacle blind, WN, Class 150, RF, pipe con. 273.0x9.27, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,98,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A96),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 10\", with companion flange, WN, Class 150, RF, pipe con. 273x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,99,10,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A97),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 10'', with companion flange, WN, Class 1500, RJ, pipe con. 273x25.4, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L (Dual Grade Certified), NACE MR 0175 / ISO 15156)",1,100,10,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A98),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 10'', with companion flange, WN, Class 600, RJ, pipe con. 273x15.09, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,101,10,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A99),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 10'', with companion flange, WN, pipe con. 273x25.4, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",2,102,10,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A100),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 12\", with companion flange, WN, Class 150, RF, pipe con. 323.8x8.38, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,103,12,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A101),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 12'', with companion flange, WN, Class 900, RJ pipe con. 323.8x25.4, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",2,104,12,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A102),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 12'', with companion flange, WN, Class 900, RJ pipe con. 323.8x25.4, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",2,105,12,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A103),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 14'', with companion flange, WN, Class 900, RJ pipe con. 355.6x31.75, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,106,14,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A104),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 16\", with companion flange, WN, Class 150, RF, pipe con. 406.4x7.92, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",1,107,16,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A105),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 16\", with companion flange, WN, Class 150, RF, pipe con. 406.4x7.92, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",9,108,16,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A106),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 16'', with companion flange, WN, Class 600, RJ, pipe con. 406.5x21.44, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,109,16,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A107),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 16'', with companion flange, WN, Class 900, RJ pipe con. 406.4x36.53, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,110,16,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A108),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 18\", with companion flange, WN, Class 150, RF, pipe con.18\"x7.92, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,111,18,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A109),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\",  with companion flange, WN, Class 150, RF, pipe con. 60.3x3.91, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,112,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A110),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", ST NPTF, Class 150, RF pipe con. 60.3x5.54, in complete with gasket, stud bolt, hex. nut, A105 Galvanized to A153",6,113,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A111),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, NPTF, Class 300, RF pipe con.60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",1,114,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A112),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 2\", with companion flange, ST NPTF, Class 150, RF pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105 Galvanized to A153",1,115,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A113),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, ST NPTF, Class 150, RF pipe con. 60.3x5.54, in complete with gaskets, stud bolt, hex. nut, A105 Galvanized to A153",10,116,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A114),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF pipe con. 60.3x5.54, in complete with gaskets, stud bolt, hex. nut, A105 Galvanized to A153",3,117,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A115),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x3.91, in complete with gasket, stud bolt, hex nuts, A182 F316/316L (Dual Grade Certified), NACE MR\n0175 / ISO 15156",1,118,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A116),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,119,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A117),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,120,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A118),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,121,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A119),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  in complete with gaskets, stud bolt, hex. Nut,A105",1,122,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A120),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket, stud bolt, hex. nut, A105, NACE MR 0175 / ISO 15156",17,123,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A121),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",33,124,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A122),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con.60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,125,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A123),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, pipe con.60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,126,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A124),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 150, RF, with Spectacle blind, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,127,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A125),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", with companion flange, WN, Class 300 Lbs RF pipe con. 60.3x2.77, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,128,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A126),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 2\", with companion flange, WN, Class 600, RF, pipe con. 60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2 A105, NACE MR 0175 / ISO 15156",1,129,2,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A127),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 2\", with spectacle blind, WN, Class 150, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,130,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A128),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\", WN, Class 150, RF, pipe con. 60.3x3.91, in complete with gasket, stud bolt, hex. nut, A182 F316L",5,131,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A129),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 2\",with companion flange, WN , Class 300 Lbs RF pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105 ",1,132,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A130),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 2'', with companion flange, WN, Class 300, RF, pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,133,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A131),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 2'', with companion flange, WN, Class 600, RJ, pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,134,2,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A132),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x11.07, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,135,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A133),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":2},{"$f":"--class($A133)","v":900},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A133),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x11.07, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",3,136,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A134),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,137,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A135),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x5.54, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",12,138,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A136),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,139,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A137),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con. 60.3x8.74, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",9,140,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A138),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con.60.3x5.54, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,141,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A139),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ pipe con.60.3x8.74, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,142,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A140),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ, pipe con. 60.3x3.91, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L (Dual Grade Certified) NACE MR 0175 / ISO 15156",1,143,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A141),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, Class 900, RJ, pipe con. 60.3x3.91, in complete with gasket, stud bolt, hex. nut, A182 F316/316L (Dual Grade Certified)  NACE MR 0175 / ISO 15156",6,144,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A142),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x11.07, Class 1500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,145,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A143),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x11.07, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",3,146,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A144),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x11.07, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A 694 grade F60",3,147,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A145),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x11.07, Class 2500, RJ,in complete with gasket,  stud  bolts, hex.  nuts,   A 694 grade F60",1,148,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A146),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x17.4, Class 2500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,149,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A147),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x17.4, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",13,150,2,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A148),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x5.54, Class 1500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,151,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A149),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x5.54, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",4,152,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A150),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 2'', with companion flange, WN, pipe con. 60.3x8.74, Class 1500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,153,2,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A151),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 20\",with companion flange, WN, Class 150, RF, pipe con. 508x9.53, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175/ISO 15156",1,154,20,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A152),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 20'', with companion flange, WN, Class 900, RJ pipe con. 508x32.54, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,155,20,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A153),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 114.3x3.05, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,156,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A154),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,157,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A155),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x3.05, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,158,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A156),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105",4,159,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A157),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,160,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A158),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,161,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A159),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket, stud bolt, hex. nut, A105, NACE MR 0175 / ISO 15156",19,162,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A160),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",24,163,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A161),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", with companion flange, WN, Class 150, RF, with Spectacle blind, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,164,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A162),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\", WN, Class 150, RF, pipe con. 88.9x5.49, in complete with gasket, stud bolt, hex. nut, A105",2,165,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A163),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3\",with companion flange, with spectacle blind, WN, Class 150, RF, pipe con. 88.9x5.49, in in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR 0175 / ISO 15156",1,166,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A164),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3'', Class 900, WN,   blind flange, gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",1,167,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A165),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3'', with companion flange, WN, Class 300, RF, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,168,3,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A166),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 3'', with companion flange, WN, Class 300, RF, pipe con.88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,169,3,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A167),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 3'', with companion flange, WN, Class 600, RJ, pipe con. 88.9x11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,170,3,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A168),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 3'', with companion flange, WN, Class 600, RJ, pipe con.88.9x7.62, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,171,3,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A169),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 3'', with companion flange, WN, Class 900, RJ pipe con. 88.9x11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,172,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A170),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3'', with companion flange, WN, Class 900, RJ pipe con. 88.9x15.24, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,173,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A171),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3'', with companion flange, WN, Class 900, RJ pipe con. 88.9x15.24, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",2,174,3,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A172),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3'', with companion flange, WN, pipe con. 88.9x22.2, Class 2500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,175,3,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A173),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 3'', with companion flange, WN, pipe con. 88.9x22.2, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",3,176,3,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A174),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 3/4\", with companion flange, WN, Class 150, RF, pipe con. 26.7x5.56, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,177,0.75,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A175),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 3/4\", with companion flange, WN, Class 150, RF, pipe con. 26.7x5.56, in complete with gasket, stud bolt,hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",10,178,0.75,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A176),{150,300,600,900,1500,2500})","v":150},null,null,null,null,null,null,null,null,null,{"$f":"MID($I$176,COLUMN(I176),1)","v":""}]
["Flange (Фланец) 3/4\", with companion flange, WN, Class 600, RJ, pipe con. 26.7x5.56, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,179,0.75,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A177),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 3/4'', with companion flange, WN, Class 1500, RJ, pipe con. 26.7x5.56, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,180,0.75,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A178),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 3/4'', with companion flange, WN, Class 2500, RJ, pipe con. 26.7x7.82, in complete with gasket,  stud  bolts, hex.  nuts,  ASTM A 694 grade F60",1,181,0.75,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A179),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 3/4'', with companion flange, WN, Class 900, RJ pipe con. 26.7x3.91, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,182,0.75,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A180),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3/4'', with companion flange, WN, Class 900, RJ pipe con. 26.7x7.82, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,183,0.75,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A181),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3/4'', with companion flange, WN, Class 900, RJ pipe con. 26.7x7.82, in complete with gasket, stud bolt, hex.nut, A350 LF2, NACE MR 0175 / ISO 15156",2,184,0.75,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A182),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 3/4'', with companion flange, WN, pipe con. 26.7x5.56, Class 1500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316L",1,185,0.75,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A183),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 3/4'', with companion flange, WN, pipe con. 26.7x5.56, Class 1500, RJ, in complete with gaskets, stud bolt,hex. nut, A182 F316L",5,186,0.75,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A184),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,187,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A185),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A105",2,188,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A186),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,189,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A187),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,190,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A188),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket, stud bolt, hex. nut, A105, NACE MR 0175 / ISO 15156",5,191,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A189),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4\", with companion flange, WN, Class 150, RF, pipe con. 114.3x6.02, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",5,192,4,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A190),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 4'', with companion flange, WN, Class 300, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,193,4,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A191),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 4'', with companion flange, WN, Class 300, RF, pipe con. 114.3x6.02, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,194,4,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A192),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 4'', with companion flange, WN, Class 600, RJ, pipe con. 114.3x13.49, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,195,4,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A193),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 4'', with companion flange, WN, Class 600, RJ, pipe con. 114.3x8.56, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,196,4,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A194),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 4'', with companion flange, WN, Class 900, RJ pipe con. 114.3x11.13, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,197,4,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A195),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 4'', with companion flange, WN, Class 900, RJ pipe con. 114.3x11.13, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",7,198,4,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A196),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 4'', with companion flange, WN, Class 900, RJ pipe con. 114.3x17.12, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,199,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A197),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":4},{"$f":"--class($A197)","v":900},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A197),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 4'', with companion flange, WN, Class 900, RJ pipe con. 114.3x17.12, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",9,200,4,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A198),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 4'', with companion flange, WN, pipe con. 114.3x11.13, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",2,201,4,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A199),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 4'', with companion flange, WN, pipe con. 114.3x17.12, Class 1500, RJ, in complete with gasket,  stud  bolts, hex.  nuts,   A350 LF2, NACE MR 0175 / ISO 15156",1,202,4,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A200),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 4'', with companion flange, WN, pipe con. 114.3x17.12, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",2,203,4,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A201),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 4'', with companion flange, WN, pipe con. 114.3x25.4, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",10,204,4,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A202),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 6\",  with companion flange, spectacle blind, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,205,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A203),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange,   WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,206,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A204),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 150, RF, pipe con. 168.3x10.97, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,207,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A205),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,208,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A206),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,209,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A207),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 150, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,210,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A208),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 150, RF, with Spectacle blind, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,211,6,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A209),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 6\", with companion flange, WN, Class 300, RF,pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,212,6,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A210),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 6\", with companion flange, WN, Class 600, RJ, pipe con. 168.3x10.97, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,213,6,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A211),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 6\",with companion flange, WN , Class 300 Lbs RF pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105 ",1,214,6,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A212),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 6'', with companion flange, WN, Class 300, RF, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,215,6,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A213),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 6'', with companion flange, WN, Class 600, RJ, pipe con. 168.3x10.97, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,216,6,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A214),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 6'', with companion flange, WN, Class 600, RJ, pipe con. 168.3x14.27, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,217,6,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A215),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 6'', with companion flange, WN, Class 600, RJ, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A403 WP 316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,218,6,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A216),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 6'', with companion flange, WN, Class 900, RJ pipe con. 168.3x10.97, in complete with gasket,  stud  bolts, hex.  nuts,   A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,219,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A217),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 6'', with companion flange, WN, Class 900, RJ pipe con. 168.3x14.27, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,220,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A218),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 6'', with companion flange, WN, Class 900, RJ pipe con. 168.3x14.27, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",1,221,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A219),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 6'', with companion flange, WN, Class 900, RJ pipe con. 168.3x18.26, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,222,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A220),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 6'', with companion flange, WN, Class 900, RJ pipe con. 168.3x18.26, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",3,223,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A221),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 6'', with companion flange, WN, pipe con. 168.3x10.97, Class 600, RJ, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175",1,224,6,600,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A222),{150,300,600,900,1500,2500})","v":600}]
["Flange (Фланец) 6'', with companion flange, WN, pipe con. 168.3x21.95, Class 1500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",12,225,6,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A223),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 6'', with companion flange, WN, pipe con. 168.3x33.3, Class 2500, RJ, in complete with gaskets, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",7,226,6,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A224),{150,300,600,900,1500,2500})","v":2500}]
["Flange (Фланец) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,227,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A225),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105, NACE MR 0175 / ISO 15156",1,228,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A226),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,229,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A227),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket, stud bolt, hex. nut, A105, NACE MR 0175 / ISO 15156",5,230,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A228),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8\", with companion flange, WN, Class 150, RF, pipe con. 219.1х6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,231,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A229),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8\",with companion flange, WN, Class 150, RF, pipe con. 219.1x6.35, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,232,8,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A230),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) 8'', with companion flange, with spectacle blind, WN, pipe con. 168.3x18.26, Class 900, RJ, in complete with gaskets, stud.bolts, hex. nuts, A350 LF2, NACE MR 0175/ISO 15156",1,233,8,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A231),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 8'', with companion flange, WN, Class 1500, RJ, pipe con. 219.1x20.62, in complete with gasket,  stud  bolts, hex.  nuts,  A182 F316/316L (Dual Grade Certified), NACE MR 0175 / ISO 15156",1,234,8,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A232),{150,300,600,900,1500,2500})","v":1500}]
["Flange (Фланец) 8'', with companion flange, WN, Class 300, RF, pipe con. 219.1x8.18, in complete with gasket,  stud  bolts, hex.  nuts,  A105",1,235,8,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A233),{150,300,600,900,1500,2500})","v":300}]
["Flange (Фланец) 8'', with companion flange, WN, Class 900, RJ pipe con. 219.1x20.62, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",1,236,8,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A234),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) 8'', with companion flange, WN, Class 900, RJ pipe con. 219.1x20.62, in complete with gasket, stud bolt, hex. nut, A350 LF2, NACE MR 0175 / ISO 15156",3,237,8,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A235),{150,300,600,900,1500,2500})","v":900}]
["Flange (Фланец) DN 2\",B10, pressure class ANSI 150, complete with blind flange, fasteners and spiral-type gaskets, graphite filler 4 mm thick, 3.2 mm thick inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material A105 Galvanized to A153 Operating medium is Instrumentation air.\nParameters of connected pipe – 60.3х5.54mm (DN 50(2\")), Рop=0.04 MPa, material as per API 5L grade B. ",1,238,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A236),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) DN 3\" pressure class ANSI 150, complete with blind flange, fasteners and spiral-type gaskets, graphite filler 4 mm thick, 3.2 mm thick inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material A105\nOperating medium is Instrumentation air.\nParameters of connected pipe – 60.3х5.54mm (DN 50(2\")),  Рр=1,96 МПа MPa, material as per API 5L grade B.",1,239,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A237),{150,300,600,900,1500,2500})","v":150}]
["Flange (Фланец) ВТ 18\",G23SC,  pressure class ANSI 900, complete with fasteners and spiral-type gaskets of oval-type, soft steel according to ASME B16.20 - 90 HB max inner and outer centering rings made of stainless steel of 304L mark in accordance with ASME B16.20/API 601. Studs A320 L7M, Hh nuts A194 7M, zinc-coated /bichromate-treated ( flange: WN as per ASME В16.5, gasket: , body Material A350 LF2. Operating medium is raw gas.\nParameters of connected pipe – 18\"х29,36mm (DN 300(12\")),  Рop=9.2 MPa,  material as per ASTM A 333 grade 6.",1,240,18,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A238),{150,300,600,900,1500,2500})","v":900}]
["Flange complete with Blind Flange (Фланец глухой) 2\", in complete with gasket,  stud  bolts, hex.  nuts,  material as per A350 LF2,NACE MR 0175 / ISO 15156 ",1,241,2,{"$error":"#VALUE!"},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A239),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange complete with Blind Flange (Фланец глухой) 2\", in complete with gaskets, stud bolt, hex. nut,material as per  600# RJ   A350 LF2,NACE MR 0175 / ISO 15156",1,242,2,{"$error":"#VALUE!"},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A240),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1\", pressure class ANSI 900, complete with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ according to ASME В16.5 material A350 LF2, Gasket/ прокладка/ прокладка: oval ring cou-pling, soft steel according to ASME В16.20 -90 НВ max. - 1 pcs/ шт., fastening: Studs/ шпилька as per ASME В16.5, A320 L7М – 4 pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated – 8  pcs/ шт.)\nParameters of connecting pipe  - 33.40х11.07 mm",1,243,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A241),{150,300,600,900,1500,2500})","v":900}]
["Flange/ Фланец DN 1\", Pressure rating ANSI 150, in package with fastening and Gasket/ прокладка/ прокладка (Flange/ Фланец: RF as per ASME В16.5 material A105, Gasket/ прокладка/ прокладкаs: spiral type, graphite filler, as per ASME В16.20/ API 601, fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7, nuts as per ASME В18.2.2,  Hh,  A194 7, galva-nized/bichromate-treated)\nParameters of the connected pipe – 33.4х6.35 mm",1,244,1,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A242),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1\", Pressure rating ANSI 1500, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ as per ASME В16.5 material A105, Gasket/ прокладка/ прокладкаs: oval ring connection, soft steel, as per ASME В16.20 – 90 НВ max., fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7, nuts as per ASME В18.2.2,  Hh,  A194 7, galva-nized/bichromate-treated)\nParameters of the connected pipe – 33.40х9.09 mm (DN 25 (1\")),  Рoр=17,7МPA,  API 5 L  X42  PSL2.",1,245,1,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A243),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1\", Pressure rating ANSI 300, in package with fastening and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RF as per ASME В16.5 material A105, Gasket/ прокладка/ прокладкаs: spiral type with graph-ite filler as per ASME В16.20/API601, fastening: Studs/ шпилька A320 L7М по ASME В16.5, nuts Hh,  A194 7M as per ASME В18.2.2, galvanized/bichromate-treated)\nParameters of the connected pipe – 33.4х6.35 mm",1,246,1,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A244),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1\", Pressure rating ANSI 900, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ as per ASME В16.5, oval ring Gasket/ прокладка/ прокладка soft steel as per ASME B16.20 - HB90 max. Studs/ шпилька as per ASME В16.5, ASTM A320 L7М, nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated)\nParameters of the connected pipe – 33.4х9.09 mm",5,247,1,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A245),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1/2\", pressure class ANSI 1500, complete with fasteners and gas-ket (Flange/ Фланец: RJ according to ASME В16.5, material A105, Gasket/ прокладка/ прокладка: oval ring coupling, soft steel according to ASME В16.20 -90 НВ max. - 1 pcs/ шт.,, fas-tening: Studs/ шпилька as per ASME В16.5, A320 L7 – 4  pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7, galvanized/bichromate-treated - 8 pcs/ шт.)\nConnected pipe parameters – 21.30х7,47 mm",1,248,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A246),{150,300,600,900,1500,2500})","v":1500}]
["Flange/ Фланец DN 1/2\", pressure class ANSI 1500, complete with fasteners and gas-ket (Flange/ Фланец: RJ according to ASME В16.5, material A182 F316L, Gasket/ прокладка/ прокладка: oval ring coupling, stainless steel of grade ТР 316 L, according to ASME В16.20 -135 НВ max. – 1 pcs/ шт., fastening : Studs/ шпилька ASTM A320 B8M according to ASME В16.5 – 4 pcs/ шт., nuts according to ASME A194 8M according to ASME B18.2.2, Hh, galvanized/ bichromate-treated – 8  pcs/ шт.\nConnected pipe parameters – 21.30х4.78 mm",1,249,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A247),{150,300,600,900,1500,2500})","v":1500}]
["Flange/ Фланец DN 1/2\", Pressure rating ANSI 1500, in package with Flange/ Фланец blind, fasteners and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RJ as per ASME В16.5, Gasket/ прокладка/ прокладкаs: stainless steel grade ТР 316 L, as per as per ASME В16.20 -135НВ max, fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 В8М, nuts as per ASME В18.2.2,  Hh, ASTM A194 8M, galvanized/bichromate-treated)\nParameters of the connected pipe – 21.3х9.09 mm (DN 15(1/2»)),  Рoр=16,1 MPa,  ASTM A 312 TP 316L",1,250,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A248),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1/2\", Pressure rating ANSI 1500, in package with Flange/ Фланец blind, fasteners and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RJ as per ASME В16.5, oval ring Gasket/ прокладка/ прокладкаs as per ASME В16.20, soft steel 135НВ max, fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 B&M, nuts as per ASME В18.2.2,  Hh, ASTM A194 8M, galvanized/bichromate-treated)\nParameters of the connected pipe – 21.3х9.09 mm (DN 15(1/2»)),  Рoр=16,1 MPa,  API 5L X42 PSL2.",4,251,0.5,1500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A249),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 1/2\", Pressure rating ANSI 900, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ as per ASME В16.5, oval ring Gasket/ прокладка/ прокладка, soft steel as per ASME B16.20 - HB90 max. Studs/ шпилька as per ASME В16.5, ASTM A320 L7М, nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate treated)\nParameters of the connected pipe – 21.3х4.78 mm",2,252,0.5,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A250),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 2\", pressure class ANSI 900, complete with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ as per ASME В16.5 material A350 LF2; Gasket/ прокладка/ прокладка: oval ring coupling, soft steel according to ASME В16.20-90 НВ max. – 1 pcs/ шт., fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М - 8 pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated -16  pcs/ шт.), body material as per Technical Requirements 8009-0090-LUOC-00-000-MEC-TRQ-0000001-A1-ER.\nThe operating medium is gas.\nParameters of connecting pipe  - 60.30х11.07 mm (DN 50 (2\")),  Рop=11.6MPa, ASTM A 333 grade 6, G26S.",1,253,2,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A251),{150,300,600,900,1500,2500})","v":900}]
["Flange/ Фланец DN 2\", Pressure rating  ANSI 300, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RF as per ASME В16.5 material A105, Gasket/ прокладка/ прокладкаs: spiral type, graphite filler, as per  ASME В16.20/API601, fastening: Studs/ шпилька A320 L7М as per ASME В16.5, nuts,  Hh, ASTM A194 7M as per  ASME В18.2.2, galva-nized/bichromate-treated)\nParameters of the connected pipe – 60.30х5.54 mm  (DN 50 (2\")),  Pop=0,7 MPa,  API 5L grade В.",1,254,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A252),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 2\", Pressure rating  ANSI 300,RF,A350 LF2",2,255,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A253),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 2\", Pressure rating ANSI 150, in package with Flange/ Фланец blind, fasteners and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RF as per ASME В16.5,Gasket/ прокладка/ прокладкаs: spiral-wound graphite-filled as per ASME В16.20/API601, fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М, nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated)\nParameters of the connected pipe – 60.3х5.54 mm (DN 50(2”)).",4,256,2,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A254),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 2\", Pressure rating ANSI 300, in package with fasteners and Gasket/ прокладка/ прокладка  (Flange/ Фланец  RF as per ASME В16.5 material  A105, Gasket/ прокладка/ прокладкаs: spiral type, graphite filler as per ASME В16.20/API601, fastening: Studs/ шпилька A320 L7 as per ASME В16.5, nuts Hh,  A194 7 as per ASME В18.2.2, galvanized/bichromate-treated)\nParameters of the connected pipe – 60.3х5.54 mm (DN 50 (2\",)), Pop=1,5 MPa,  API 5L grade В galvanized up A53 grade В.",1,257,2,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A255),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 3\", Pressure rating  ANSI 150, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RF as per ASME В16.5 material  A350 LF2, Gasket/ прокладка/ прокладкаs: spiral type, graphite filler  as per ASME В16.20/API601, fastening: Studs/ шпилька  A320 L7М as per ASME В16.5, nuts Hh,  A194 7M as per ASME В18.2.2, galvanized/bichromate-treated)\nParameters of the connected pipe – 88.9х5.49 mm",1,258,3,150,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A256),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 3\", Pressure rating ANSI 300, in package with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RF as per ASME В16.5 material A105, Gasket/ прокладка/ прокладкаs: spiral type, graphite filler, as per ASME В16.20/ API 601, fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М, nuts as per ASME В18.2.2,  Hh,  A194 7М, galva-nized/bichromate-treated)\nParameters of the connected pipe – 60.30х5.54 mm, Рoр=0.15-0,3 МPA A333 grade 6.",1,259,3,300,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A257),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Flange/ Фланец DN 4\", pressure class ANSI 900, complete with fasteners and Gasket/ прокладка/ прокладка (Flange/ Фланец: RJ as per ASME В16.5 material A350 LF2; Gasket/ прокладка/ прокладка: oval ring coupling, soft steel according to ASME В16.20-90 НВ max. - 1 pcs/ шт., fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М – 8 pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated – 16 pcs/ шт.), body material as per Technical Requirements 8009-0090-LUOC-00-000-MEC-TRQ-0000001-A1-ER.\nOperating medium is drainage.\nParameters of connected pipe - 114.3х17.12 mm (DN 100 (4\")),  Рop=11.6\nMPa, ASTM A 333 grade 6, G26S.",1,260,4,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A258),{150,300,600,900,1500,2500})","v":900}]
["Flange/ Фланец DN 6\", pressure class ANSI 900, complete with fasteners and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RJ as per ASME В16.5 material A350 LF2; Gasket/ прокладка/ прокладка: oval ring coupling, soft steel according to ASME В16.20 -90 НВ max. – 1 pcs/ шт., fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М -12 pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated - 24 pcs/ шт.)\nParameters of connected pipe - 168.3х18.26 mm (DN 150 (6\")),  Рop=11.6MPa, ASTM A 333 grade 6, G26S.",1,261,6,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A259),{150,300,600,900,1500,2500})","v":900}]
["Flange/ Фланец DN 8\", pressure class ANSI 900, complete with fasteners and Gasket/ прокладка/ прокладкаs (Flange/ Фланец: RJ as per ASME В16.5 material A350 LF2; Gasket/ прокладка/ прокладка: oval ring coupling, soft steel according to ASME В16.20 -90 НВ max. – 1 pcs/ шт., fastening: Studs/ шпилька as per ASME В16.5, ASTM A320 L7М – 12 pcs/ шт., nuts as per ASME В18.2.2, Hh, ASTM A194 7M, galvanized/bichromate-treated -24 pcs/ шт.)\nConnected pipe parameters – 219.10 х 20.62 mm (DN 200 (8\")), Рop=11.6 MPa, ASTM A 333 grade 6, G26S",1,262,8,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A260),{150,300,600,900,1500,2500})","v":900}]
["RJ flange (Фланец RJ), complete with flange blind, fasteners and gaskets, material А350 LF2 ",1,263,{"$f":"--SUBSTITUTE(SUBSTITUTE(diam($A261),\" 1/2\",\",5\"),\" 3/4\",\",75\")","v":{"$error":"#VALUE!"}},{"$f":"--class($A261)","v":{"$error":"#VALUE!"}},{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A261),{150,300,600,900,1500,2500})","v":{"$error":"#N/A"}}]
["Spectacle blind (blind spacer plate + open spacer plate) DN 8\", pressure class ANSI 900, for Flange/ Фланецs with sealing surface RJ as per ASME B 16.5, material as per ASTM A 516 grade 70",1,264,8,900,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A262),{150,300,600,900,1500,2500})","v":900}]
["WeldoFlange (Велдофланец) (Велдофланец) 1 1/2\", Class 2500, RJ, pipe con. 323.9x25.4, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,265,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A263),{150,300,600,900,1500,2500})","v":2500}]
["WeldoFlange (Велдофланец) 1 1/2\", Class 2500, RJ, pipe con. 168.3x18.26, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,266,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A264),{150,300,600,900,1500,2500})","v":2500}]
["WeldoFlange (Велдофланец) 1 1/2\", Class 2500, RJ, pipe con. 168.3x7.11, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",2,267,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A265),{150,300,600,900,1500,2500})","v":2500}]
["WeldoFlange (Велдофланец) 1 1/2\", Class 2500, RJ, pipe con. 323.9x25.4, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",3,268,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A266),{150,300,600,900,1500,2500})","v":2500}]
["WeldoFlange (Велдофланец) 1 1/2\", Class 2500, RJ, pipe con. 88.9x5.49, in complete with gasket,  stud  bolts, hex.  nuts,  A350 LF2, NACE MR 0175 / ISO 15156",3,269,1.5,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A267),{150,300,600,900,1500,2500})","v":2500}]
["WeldoFlange (Велдофланец) 18\"x 1 1/2\", Class 2500, RJ, pipe con. 457x29.36-60.3x8.74 in complete with gasket,  stud  bolts, hex.  nuts,  A105/А350 LF2,  NACE MR 0175 /ISO 5156",2,270,18,2500,{"$f":"LOOKUP(,-1/SEARCH(\"Class*\"&{150,300,600,900,1500,2500},A268),{150,300,600,900,1500,2500})","v":2500}]

{"sheet":"Лист1","index":1,"n_rows":6,"n_cols":1,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[150]
[300]
[600]
[900]
[1500]
[2500]