{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":11,"n_cols":13,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,1,{"$f":"D3+1","v":2},{"$f":"E3+1","v":3},4,5,6,7,8,9,10]
[null,null,1,"7-25-2","Маш и мех","200-0001","Автомобили бортовые, грузо­подъемность до 3 т","авто","м-ч",0.14000000000000001,"авто[0,14 м-ч]",{"$f":"H4&\"[\"&J4&\" \"&I4&\"]\"","v":"авто[0,14 м-ч]"}]
[null,null,{"$f":"C4+1","v":2},"7-25-2","Маш и мех","270-0014","Подъемники мачтовые строи­тельные, грузоподъемность 0,5т","подм","м-ч",0.32,"подм[0,32 м-ч]",{"$f":"H5&\"[\"&J5&\" \"&I5&\"]\"","v":"подм[0,32 м-ч]"}]
[null,null,{"$f":"C5+1","v":3},"7-25-2","Маш и мех","270-0090","Пила дисковая электрическая","пила","м-ч",5.21,"пила[5,21 м-ч]","пила[5,21 м-ч]"]
[null,null,4,"7-25-2","Маш и мех","270-122","Машины паркетно-строгальные","мапс","м-ч",17.47,"мапс[17,47 м-ч]","мапс[17,47 м-ч]"]
[null,null,5,"7-25-2","Маш и мех","270-241","Машина паркетно-шлифовальная","мапш","м-ч",14.66,"мапш[14,66 м-ч]","мапш[14,66 м-ч]"]
[null,null,6,"7-25-2","Материалы","111-0609","Мастика клеящая каучуковая КН-2","макк","кг",192,"макк[192 кг]","макк[192 кг]"]
[null,null,7,"7-25-2","Материалы","111-1604","Бумага шлифовальная","бума","м2",20,"бума[20 м2]","бума[20 м2]"]
[null,null,8,"7-25-2","Материалы","П","Паркет штучный","пашт","м2",102,"пашт[102 м2]","пашт[102 м2]"]