{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["MaterialsNorms","Лист 2","Справочник"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MaterialsNorms","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,"Наименование","кол-во"," Труба PE-RT"]
[null,null,null,"диаметр, мм",null,"толщина "]
[null,"ГПИ-труба 25/90 (32х4,4-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 32/110 (40х5,5-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 40/110 (50х6,9-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 50/125 (63х8,6-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 63/140 (75х10,3-SDR 7,4) ",1,75,"х"]
[null,"ГПИ-труба 75/160 (90х12,3-SDR 7,4) ",1,90,"х"]
[null,"ГПИ-труба 90/180 (110х15,1-SDR 7,4) ",1,110,"х"]
[null,"ГПИ-труба 110/200 (125х17,1-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 125/225 (140х19,2-SDR 7,4) ",1,null,"х"]
[null,"ГПИ-труба 140/250 (160х21,9-SDR 7,4) ",1,160,"х"]
[null,"ГПИ-труба 160/250 (180х24,6-SDR 7,4) ",1,null,"х"]

{"sheet":"Лист 2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Справочник","index":2,"n_rows":12,"n_cols":2,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["jD1 Диаметр нап. трубы","jS1 толщ стенки нап. трубы"]
[32,4.4000000000000004]
[40,5.5]
[50,6.9]
[63,8.6]
[75,10.3]
[90,12.3]
[110,15.1]
[125,17.100000000000001]
[140,19.2]
[160,21.9]
[180,24.6]