{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["месяц.гр"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"месяц.гр","index":0,"n_rows":4,"n_cols":12,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[1,2,null,null,null,null,null,null,null,null,"1 слово","3 слово"]
[1,"4KPC22AP001 Электродвигатель  АД132S4А3У3 N=7,5кВт","4KPC22AP001","Электродвигатель ",0,"АД132S4А3У3 N=7,5кВт","АД132S4А3У3 7,5 кВт,1450об/мин.","1UKS 91 273",0,"ХЦ"]
[2,"4KPC25AP001, Электродвигатель,  АД132S4А3У3, N=7,5кВт","4KPC25AP001","Электродвигатель ",0,"АД132S4А3У3 N=7,5кВт","АД132S4А3У3 7,5 кВт,1450об/мин.","1UKS 91 273",0,"ХЦ"]
[3,"4KPC10AP001,    Электродвигатель ,  АД132S4А3У3  , N=7,5кВт","4KPC10AP001","Электродвигатель ",0,"АД132S4А3У3 N=7,5кВт","АД132S4А3У3 7,5 кВт,1450об/мин.","1UKS 91 371","ЗКД","ХЦ"]