{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["КП","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"КП","index":0,"n_rows":4,"n_cols":4,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["Устройство","Производитель","Технический характеристики","Артикул"]
["Купольная внутренняя HD-TVI-видеокамера\n1 Mpx","Hiwatch","Купольная внутренняя HD-TVI-видеокамера. \nРазрешение 1 Мп 1296х732 пикселей\n1/4 CMOS матрица. \nИК-подсветка до 20 м. \nОбъектив  3.6мм (2.8мм, 6мм опционально), \nУгол обзора 70.9°(3.6мм), 82°(2.8мм), 56.7°(6мм)\nРабочая температура -20°С — 45°С\nГабариты 98 × 65.4 мм","DS-T101"]
["Купольная внутренняя HD-TVI-видеокамера\n1 Mpx","Hiwatch","Купольная внутренняя HD-TVI-видеокамера. \nРазрешение 1 Мп 1280х720 пикселей\n1/4 CMOS матрица. \nИК-подсветка до 30 м. \nОбъектив  2.8 – 12мм @ F1.4, вариообъектив, \nУгол обзора  71.8° – 23.4°\nРабочая температура -20°С — 45°С\nГабариты 136 х 102мм","DS-T107"]
["Купольная внутренняя IP-видеокамера\n1 Mpx","Hiwatch","Купольная внутренняя IP-видеокамера. Разрешение 1 Мп 1280×720 пикселей\n 1/4 Progressive Scan CMOS матрица. \nИК-подсветка до 10 м. \nОбъектив  2.8мм @F2.0 (4мм, 6мм опция), \nУгол обзора  92.5° (2.8мм), 73.1° (4мм), 46° (6мм)\nРабочая температура -20°С — 45°С\nГабариты 110x80.9мм","DS-I113"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}