{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Исходная","Результат"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Исходная","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Поз.","Наименование и техническая характеристика","Тип, марка, обозначение документа, опросного листа","Код продукции","Поставщик","Ед. измерения","Кол.","Масса 1 ед., кг","Примечание"]
[null,null," "," "," "," "," "," "," "]
[null,"Болт с шестигранной головкой","M8x16","CM020816HDZ","АО \"ДКС\"","шт.",50," "," "]
[null,"Болт с шестигранной головкой","M8x16","CM020816HDZ","АО \"ДКС\"","шт.",4," "," "]
[null,"Винт для крепления к профилю M10x30"," ","CM0401030","АО \"ДКС\"","шт.",68]
[null,"Винт для крепления к профилю M10x30"," ","CM0401030","АО \"ДКС\"","шт.",96]
[" ","Винт для обеспечения электрического контакта крышек, гальванически оцинкованная сталь","М5х8","CM030508","АО \"ДКС\"","шт.",40," "," "]
[" ","Винт для обеспечения электрического контакта крышек, гальванически оцинкованная сталь","М5х8","CM030508","АО \"ДКС\"","шт.",19," "," "]
[" ","Винт для обеспечения электрического контакта крышек, гальванически оцинкованная сталь","М5х8","CM030508","АО \"ДКС\"","шт.",75," "," "]
[" ","Винт с гладкой головкой и квадратным подголовником M6x20, гальванически оцинкованная сталь","М6х20","CM010620","АО \"ДКС\"","шт.",8," "," "]
[null,"Винт с гладкой головкой и квадратным подголовником M6x20, гальванически оцинкованная сталь","М6х20","CM010620","АО \"ДКС\"","шт.",68]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",436," "," "]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",300," "," "]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",138," "," "]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",585," "," "]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",192," "," "]

{"sheet":"Результат","index":1,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Поз.","Наименование и техническая характеристика","Тип, марка, обозначение документа, опросного листа","Код продукции","Поставщик","Ед. измерения","Кол.","Масса 1 ед., кг","Примечание"]
[null,null," "," "," "," "," "," "," "]
[null,"Болт с шестигранной головкой","M8x16","CM020816HDZ","АО \"ДКС\"","шт.",54,null," "]
[null,"Винт для крепления к профилю M10x30"," ","CM0401030","АО \"ДКС\"","шт.",164]
[" ","Винт для обеспечения электрического контакта крышек, гальванически оцинкованная сталь","М5х8","CM030508","АО \"ДКС\"","шт.",134,null," "]
[" ","Винт с гладкой головкой и квадратным подголовником M6x20, гальванически оцинкованная сталь","М6х20","CM010620","АО \"ДКС\"","шт.",76,null," "]
[" ","Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",1651,null," "]
[]
[]
[]
[]
["Поз.","Наименование и техническая характеристика","Тип, марка, обозначение документа, опросного листа","Код продукции","Поставщик","Ед. измерения","Кол. ","Масса 1 ед., кг","Примечание"]
[null,"Болт с шестигранной головкой","M8x16","CM020816HDZ","АО \"ДКС\"","шт.",54]
[null,"Винт для крепления к профилю M10x30"," ","CM0401030","АО \"ДКС\"","шт.",164]
[null,"Винт для обеспечения электрического контакта крышек, гальванически оцинкованная сталь","М5х8","CM030508","АО \"ДКС\"","шт.",134]
[null,"Винт с гладкой головкой и квадратным подголовником M6x20, гальванически оцинкованная сталь","М6х20","CM010620","АО \"ДКС\"","шт.",76]
[null,"Винт с квадратным подголовником M6x10, гальванически оцинкованная сталь","М6х10","CM010610","АО \"ДКС\"","шт.",1651]