{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["СВОР_Сопряжение"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"СВОР_Сопряжение","index":0,"n_rows":4,"n_cols":20,"rows_kept":4,"cut":false,"hidden":false,"merged":[[2,13,3,13],[1,5,1,9],[2,11,3,11]]}
[null,8,6,42,7,8,1.5,8,1.5,8,16,16,16]
[null,null,"№ п/п","Наименование работ","Ед. изм.","Объем работ",null,null,null,null,"Формула расчета объемов работ и расхода материалов","Ссылка на чертежи, спецификации в ПД","Доп.инф."]
[null,null,null,"Заполнение битумно-полимерной мастикой БРИТ-БР(БП)-ДШ-85:",null,null,null,null,null,null,null,"Том 3.2\nчертеж \"Деформацоинный шов\""]
[null,null,null," - Пространство между переходными плитами и шкафной стенкой","м3/кг",{"$f":"P4*R4*T4","v":8.0360000000000001E-2},null,"/",null,{"$f":"1100*F4","v":88.396000000000001},{"$f":"u_2(F4)","v":"V = Площадь сечения, м2 (0,004018) * Длина заполнения, м (10) * Кол-во опор, шт (2) "},null,"расход  1100кг/м3",null,"Площадь сечения, м2",4.0179999999999999E-3,"Длина заполнения, м",10,"Кол-во опор, шт",2]