{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":4,"n_cols":6,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["К75-10 1,0МК 250В 10%",{"$f":"емкость(A1)","v":1},{"$f":"вольтаж(A1)","v":250},{"$f":"проценты(A1)","v":10},null,"http://www.excelworld.ru/forum/2-8941-1#81456"]
["К75-10 0,1М 500В конденсатор ",{"$f":"емкость(A2)","v":0.1},{"$f":"вольтаж(A2)","v":500},{"$f":"проценты(A2)","v":""}]
["К42-У2 250В 0,33МКФ - 10% комбинированный",{"$f":"емкость(A3)","v":0.33},{"$f":"вольтаж(A3)","v":250},{"$f":"проценты(A3)","v":10}]
["МБГО 250В 0,33МКФ - 20% напряжометр",{"$f":"емкость(A4)","v":0.33},{"$f":"вольтаж(A4)","v":250},{"$f":"проценты(A4)","v":20}]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}