{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,0,0,5],[1,0,1,5]]}
["Объект: С"]
["Здание: Корпус №"]
["№\nп/п","Автомат - Щит","Марка\nавтомата","Номинал\nавтомата,\nА","Фаза","Кабель","Длина кабеля"]
[null,"Объект1"]
[1,"QF1 ","EZC250N",25,"A, B, C","АВВГнг-LS 5х185"]
[2,"QF2 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[3,"QF3 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[4,"QF4 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[5,"QF5 ","EZC100N",60,"A, B, C","ВВГнг-LS 5х16"]
[6,"QF6 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[7,"QF7 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[8,"QF8 ","EZC100N",60,"A, B, C","ВВГнг-LS 5х16"]
[9,"QF9 ","EZC100N",50,"A, B, C","ВВГнг-LS 5х10"]
[10,"QF10 ","EZC100N",63,"A, B, C","ВВГнг-LS 5х35"]
[11,"QF11 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х16"]
[12,"QF12 ","EZC100N",80,"A, B, C","ВВГнг-LS 5х25"]
[13,"QF13 ","EZC100N",80,"A, B, C","ВВГнг-LS 5х25"]
[14,"QF14 ","EZC100N",50,"A, B, C","ВВГнг-LS 5х10"]
[15,"QF15 ","EZC100N",100,"A, B, C","ВВГнг-LS 5х25"]
[16,"QF16 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[17,"QF17 ","EZC100N",40,"A, B, C","ВВГнг-LS 5х6"]
[19,"QF19 ","EZC250F",250,"A, B, C"]
[20,"QF20 ","EZC250F",250,"A, B, C"]
[21,"QF21 ","EZC250F",250,"A, B, C"]
[22,"QF22 ","EZC100N",40,"A, B, C"]
[23,"QF23 ","EZC100N",63,"A, B, C"]
[24,"QF24 ","EZC100N",80,"A, B, C"]
[25,"QF25 ","EZC100N",40,"A, B, C"]
[26,"QF26 ","EZC100N",40,"A, B, C"]
[null,"Объект2"]
[1,"QF1 -WL_EPS","C60N","B10","A","ВВГнг-FRLS 3х1,5"]
[2,"QF2 -WL.1С","PL7","B32","A, B, C","ВВГнг-FRLS 5х6"]
[3,"QF3 -WL_EPS2","PL7","B10","B","ВВГнг-FRLS 3х2,5"]
[4,"QF4 Управление","PL7","B6","C"]
[5,"QF5 -WL_Ma","PL7","B10","A, B, C","ВВГнг-FRLS 5х2,5"]
[null,"Объект3"]
[1,"QW101 УЗО","INS63",63]
[2,"QF102 -WL_MX_G1 ","C60H","B20","A, B, C","ВВГнг-LS 5х4"]
[3,"QF103 -WL_MX_G2","C60H","B20","A, B, C","ВВГнг-LS 5х4"]
[4,"QF104 -WL_MX_G3","C60H","B20","A, B, C","ВВГнг-LS 5х4"]