{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист4"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист4","index":0,"n_rows":162,"n_cols":5,"rows_kept":162,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["Имеется:"]
["№ п/п","Name","Country","Remark","Модели ВЭУ"]
[1,"AAER","Canada","Acquired (2010)","A1000S (1000 kW, 54 m diameter) (old model)\nA1000 (1000 kW, 58 m diameter) (old model)\nA1500-70 (1500 kW, 70 m diameter) (old model)\nA1500-77 (1500 kW, 77 m diameter) (old model)\nA1650 -70 (1650 kW, 70 m diameter) (old model)\nA1650 -77 (1650 kW, 77 m diameter) (old model)\nA1650 -80 (1650 kW, 80 m diameter) (old model)\nA2000-71 (2000 kW, 71 m diameter) (old model)\nA2000-80 (2000 kW, 80 m diameter) (old model)\nA2000-84 (2000 kW, 84 m diameter) (old model)"]
[2,"Acciona","Spain",null,"AW-1500/70 (1500 kW, 70 m diameter) (under production)\nAW-1500/77 (1500 kW, 77 m diameter) (under production)\nAW-1500/82 (1500 kW, 82 m diameter) (under production)\nAW-3000/100 (3000 kW, 100 m diameter) (under production)\nAW-3000/109 (3000 kW, 109 m diameter) (under production)\nAW-3000/116 (3000 kW, 116 m diameter) (under production)\nAW-3000/125 (3000 kW, 125 m diameter) (under production)\nAW-3000/132 (3000 kW, 125 m diameter) (under development)"]
[3,"ACSA","Spain",null,"A27/225 (225 kW, 27 m diameter) (under production)\nA29/225 (225 kW, 29 m diameter) (old model)"]
[4,"Adler","Germany","No longer exists","25 (165 kW, 25 m diameter) (old model)"]
[5,"Adwen","Germany",null,"AD 5-132/128 (5000 kW, 128 m diameter) (under production)\nAD 5-132 (5000 kW, 132 m diameter) (under production)\nAD 5-135 (5000 kW, 135 m diameter) (under production)\nAD 8-180 (8000 kW, 180 m diameter) (under development)"]
[6,"Aerodyn","Germany",null,"aM 1.0/77 DD (1000 kW, 77 m diameter) (under development)\naM 1.5/77 (1500 kW, 77 m diameter) (under production)\naM 1.5/83 (1500 kW, 83 m diameter) (under production)\naM 1.5/87 (1500 kW, 87 m diameter) (under production)\naM 1.5/92 (1500 kW, 92 m diameter) (under production)\naM 2.0/80 (2000 kW, 80 m diameter) (under development)\naM 2.0/87 (2000 kW, 87 m diameter) (under development)\naM 2.0/93 (2000 kW, 93 m diameter) (under development)\naM 2.0/120 XL (2000 kW, 120 m diameter) (under development)\naM 2.5/96 (2500 kW, 97 m diameter) (under production)\naM 2.5/103 (2500 kW, 103 m diameter) (under production)\naM 2.5/110 (2500 kW, 110 m diameter) (under production)\naM 2.5/118 (2500 kW, 118 m diameter) (under production)\naM 3.0/118 (3000 kW, 118 m diameter) (under development)\naM 3.0/134 (3000 kW, 118 m diameter) (under production)\naM 3.2/110 (3200 kW, 120 m diameter) (under development)\naM 5.0/130 (5000 kW, 130 m diameter) (under production)\naM 5.0/139 (5000 kW, 139 m diameter) (under production)\n8.0 MW-168 (8000 kW, 168 m diameter) (under development)"]
[7,"Aeronautica Windpower","USA",null,"29-225 (225 kW, 29 m diameter) (old model)\n33-225 (225 kW, 33 m diameter) (old model)\n30-250 (250 kW, 30 m diameter) (under production)\n47-500 (500 kW, 47 m diameter) (under production)\n47-750 (750 kW, 47 m diameter) (under production)\n54-750 (750 kW, 54 m diameter) (under production)"]
[8,"Alizeo","France",null,"Alizeo 1000/56 (1000 kW, 56 m diameter) (under production)\nAlizeo 1000/60 (1000 kW, 60 m diameter) (under production)\nAlizeo 1000/64 (1000 kW, 64 m diameter) (under production)\nAlizeo 1000/60 Softwind (1000 kW, 64 m diameter) (under production)\nAlizeo 1000/64 Softwind (1000 kW, 64 m diameter) (under production)"]
[9,"Alstom Power","France",null,"80 (1670 kW, 80 m diameter) (old model)\n86 (1670 kW, 85.5 m diameter) (old model)\n122 (2700 kW, 122 m diameter) (under production)\n100 (3000 kW, 100.8 m diameter) (under production)\n110 (3000 kW, 109.8 m diameter) (under production)\n122/3000 (3000 kW, 109.8 m diameter) (under production)\nHaliade 150 (6000 kW, 150 m diameter) (under production)"]
[10,"Areva","France","No longer exists (2015)","M5000-116 (5000 kW, 116 m diameter) (old model)\nM5000-135 (5000 kW, 135 m diameter) (old model)"]
[11,"ATB Riva Calzoni SpA","Italy",null,"ATB500 (500 kW, 54 m diameter) (under production)"]
[12,"Autoflug","Germany","No longer exists","A1200 (1200 kW, 61 m diameter) (old model)"]
[13,"Avantis","Germany",null,"AV 1010 (2300 kW, 100.6 m diameter) (old model)\nAV 928 (2500 kW, 93.2 m diameter) (under production)"]
[14,"AVIC Huide","China",null,"HD1000 (1000 kW, 55.4 m diameter) (under production)\nHD1100 (1100 kW, 55 m diameter) (old model)\nHD2000 (2000 kW, 93.2 m diameter) (under production)"]
[15,"AWE","Canada",null,"52-750 (750 kW, 52 m diameter) (under production)\n52-900 (900 kW, 52 m diameter) (under production)\n54-900 (900 kW, 54 m diameter) (under production)"]
[16,"Bard","Germany",null,"VM (5000 kW, 122 m diameter) (under production)"]
[17,"Blaaster","Norway",null,"3000 (3000 kW, 100 m diameter) (under development)"]
[18,"Bonus","Germany","Acquired (2004)","B30/100 (100 kW, 30 m diameter) (old model)\nB19/120 (120 kW, 19.4 m diameter) (old model)\nB23/150 (150 kW, 23 m diameter) (old model)\nB24/150 (150 kW, 24 m diameter) (old model)\nB30/150 (150 kW, 30 m diameter) (old model)\nB31/300 (300 kW, 31 m diameter) (old model)\nB33/300 (300 kW, 33 m diameter) (old model)\nB35/450 (450 kW, 35 m diameter) (old model)\nB37/450 (450 kW, 37 m diameter) (old model)\nB41/600 (600 kW, 41 m diameter) (old model)\nB44/600 (600 kW, 44 m diameter) (old model)\nB52/1000 (1000 kW, 52 m diameter) (old model)\nB54/1000 (1000 kW, 54.1 m diameter) (old model)\nB62/1300 (1300 kW, 62 m diameter) (old model)\nB76/2000 (2000 kW, 76 m diameter) (old model)\nB82/2300 (2300 kW, 82 m diameter) (old model)"]
[19,"China Creative Wind Energy","China",null,"WD59-1250 (1250 kW, 59 m diameter) (old model)\nCCWE-1500/70.DF (1500 kW, 70.5 m diameter) (under production)\nCCWE-1500/77.D (1500 kW, 77.5 m diameter) (under production)\nCCWE-1500/77.DF (1500 kW, 77.5 m diameter) (under production)\nCCWE-1500/82.D (1500 kW, 82 m diameter) (under production)\nCCWE-1500/82.DF (1500 kW, 82 m diameter) (old model)\nCCWE-1500/87.DF (1500 kW, 87 m diameter) (under production)\nCCWE-3000/100.DF (3000 kW, 100 m diameter) (under production)\nCCWE-3000/100.D (3000 kW, 103.4 m diameter) (under production)\nCCWE-3600/115.D (3600 kW, 115 m diameter) (under production)\nCCWE-5000/126.D (5000 kW, 126 m diameter) (under development)"]
[20,"Clipper","USA","No longer exists (2012)","Liberty C89 (2500 kW, 89 m diameter) (old model)\nLiberty C93 (2500 kW, 93 m diameter) (old model)\nLiberty C96 (2500 kW, 96 m diameter) (old model)\nLiberty C99 (2500 kW, 99 m diameter) (old model)\nLiberty C100 (2500 kW, 100 m diameter) (old model)"]
[21,"CNYD","China",null,"YDF-1500-70 (1500 kW, 70 m diameter) (under production)\nYDF-1500-77 (1500 kW, 77 m diameter) (under production)\nYDF-1500-82 (1500 kW, 82 m diameter) (under production)\nYDF-1500-87 (1500 kW, 87 m diameter) (under production)"]
[22,"CWEL","India",null,"C-30/250 (250 kW, 29.6 m diameter) (under production)"]
[23,"Danregn","Germany","Acquired (1983)","150 (150 kW, 23.8 m diameter) (old model)\n300 (300 kW, 31 m diameter) (old model)"]
[24,"Danwin","Denmark","Acquired","20/110 (110 kW, 19.6 m diameter) (old model)\n20/140 (140 kW, 19.6 m diameter) (old model)\n24/150 (150 kW, 24 m diameter) (old model)\n23/160 (160 kW, 23 m diameter) (old model)\n23/180 (180 kW, 23 m diameter) (old model)\n24/200 (200 kW, 24 m diameter) (old model)\n27/225 (225 kW, 27 m diameter) (old model)"]
[25,"Darwind","Netherlands","Acquired (2009)","Darwind (5000 kW, 115 m diameter) (old model)"]
[26,"DCNS","France",null,"Winflo (1000 kW, 60 m diameter) (under development)"]
[27,"DDIS","France",null,"DDIS60 (800 kW, 60 m diameter) (under production)"]
[28,"DEC","China",null,"FD70-1500 (1500 kW, 70 m diameter) (old model)\nFD77-1500 (1500 kW, 77 m diameter) (old model)\nFD93-1500 (1500 kW, 93 m diameter) (under production)\n5.5MW prototype (5500 kW, 140 m diameter) (under development)"]
[29,"Dencon","Denmark","No longer exists","Tornado 200/26 (200 kW, 26 m diameter) (old model)\nTornado 250/26 (250 kW, 26 m diameter) (old model)"]
[30,"DESA","Spain","No longer exists","A300 (300 kW, 30 m diameter) (old model)"]
[31,"Dewind (DewindCo)","USA","Acquired (2009)","D4-500 (500 kW, 41 m diameter) (old model)\nD4 (600 kW, 48 m diameter) (under production)\nD6-1000 (1000 kW, 62 m diameter) (old model)\nD6 (1250 kW, 64 m diameter) (under production)\nD8.0 (2000 kW, 80 m diameter) (under production)\nD8.2 (2000 kW, 80 m diameter) (under production)\nD9 (2000 kW, 93 m diameter) (under production)"]
[32,"Doosan","South Korea",null,"WinDS3000 (3000 kW, 91.3 m diameter) (under production)"]
[33,"DWP","Denmark","No longer exists","D150/22 (150 kW, 22.2 m diameter) (old model)\nD150/24 (150 kW, 23.6 m diameter) (old model)\nD175/24 (175 kW, 23.6 m diameter) (old model)"]
[34,"e.n.o. energy","Germany",null,"82 (2000 kW, 82.4 m diameter) (old model)\n82/2050 (2050 kW, 82.4 m diameter) (under production)\n92 (2200 kW, 92.8 m diameter) (under production)\n100 (2200 kW, 100.5 m diameter) (under production)\n114 (3500 kW, 114 m diameter) (under production)\n126 (3500 kW, 126 m diameter) (under production)"]
[35,"Ebara","Japan",null,"EPW1570 (1500 kW, 70 m diameter) (under production)"]
[36,"Ecotecnia","France","Acquired (2007)","20 (150 kW, 20 m diameter) (old model)\n28 (225 kW, 28 m diameter) (old model)\n44 (600 kW, 44 m diameter) (old model)\n48 (750 kW, 48 m diameter) (old model)\n62 (1300 kW, 62 m diameter) (old model)\n74 (1670 kW, 74 m diameter) (old model)\n80 1.6 (1670 kW, 80 m diameter) (old model)\n86 (1670 kW, 86 m diameter) (old model)\n80 2.0 (2000 kW, 80 m diameter) (old model)\n100 (3000 kW, 100 m diameter) (old model)\n110 (3000 kW, 110 m diameter) (old model)"]
[37,"Elecon Engineering","India",null,"T600-48DS (600 kW, 48 m diameter) (old model)"]
[38,"Elsewedy","Egypt",null,"TWT 1.65/70 (1650 kW, 70 m diameter) (under production)\nTWT 1.65/77 (1650 kW, 77 m diameter) (under production)\nTWT 1.65/82 (1650 kW, 82 m diameter) (under production)"]
[39,"Enercon","Germany",null,"E30/300 (300 kW, 30 m diameter) (old model)\nE32/300 (300 kW, 32 m diameter) (old model)\nE33/330 (330 kW, 33.4 m diameter) (old model)\nE40/500 (500 kW, 40 m diameter) (old model)\nE40/600 (600 kW, 40 m diameter) (old model)\nE44/600 (600 kW, 44 m diameter) (old model)\nE48/600 (600 kW, 48 m diameter) (old model)\nE48/800 (800 kW, 48 m diameter) (under production)\nE53/800 (800 kW, 52.9 m diameter) (under production)\nE44/900 (900 kW, 44 m diameter) (under production)\nE58/1000 (1000 kW, 58 m diameter) (old model)\nE66/1500 (1500 kW, 66 m diameter) (old model)\nE66/1800 (1800 kW, 66 m diameter) (old model)\nE82/1800 (1800 kW, 82 m diameter) (old model)\nE66/2000 (2000 kW, 66 m diameter) (old model)\nE70/2000 (2000 kW, 70 m diameter) (old model)\nE70/E4 (2000 kW, 70 m diameter) (old model)\nE82/2000 (2000 kW, 82 m diameter) (under production)\nE82/2050 (2050 kW, 82 m diameter) (old model)\nE70/2300 (2300 kW, 71 m diameter) (under production)\nE82/2300 (2300 kW, 82 m diameter) (under production)\nE82/2350 (2350 kW, 82 m diameter) (under production)\nE92/2350 (2350 kW, 92 m diameter) (under production)\nE115/2500 (2500 kW, 115 m diameter) (old model)\nE82/3000 (3000 kW, 82 m diameter) (under production)\nE101/3000 (3000 kW, 101 m diameter) (old model)\nE115/3000 (3000 kW, 115 m diameter) (under production)\nE101/3050 (3050 kW, 101 m diameter) (under production)\nE126/4000 (4000 kW, 127 m diameter) (under development)\nE126/4200 (4200 kW, 127 m diameter) (under production)\nE112/4500 (4500 kW, 114 m diameter) (old model)\nE112/6000 (6000 kW, 114 m diameter) (old model)\nE126/6000 (6000 kW, 127 m diameter) (old model)\nE126/7000 (7000 kW, 127 m diameter) (old model)\nE126/7500 (7500 kW, 127 m diameter) (old model)\nE126/7580 (7580 kW, 127 m diameter) (under production)"]
[40,"Enron","USA","Acquired (2002)","900s (1000 kW, 54 m diameter) (old model)\n1.5s (1500 kW, 70 m diameter) (old model)\n1.5sl (1500 kW, 77 m diameter) (old model)"]
[41,"Envision","China",null,"E70 (1500 kW, 70.6 m diameter) (old model)\nE77 (1500 kW, 77.5 m diameter) (old model)\nE82 (1500 kW, 82.5 m diameter) (old model)\nE87 (1500 kW, 87 m diameter) (old model)\n1.5-93 (1500 kW, 93 m diameter) (under production)\n1.8-106 (1800 kW, 106 m diameter) (under production)\n2.1-110 (2100 kW, 110 m diameter) (under production)\n2.2-110 (2200 kW, 110 m diameter) (under production)\n2.3-110 (2300 kW, 110 m diameter) (under production)\n2.3-115 (2300 kW, 115 m diameter) (under production)\n3.0-120 (3000 kW, 120 m diameter) (under production)\nE128 (3600 kW, 128 m diameter) (under development)\n4.0-130 (4000 kW, 130 m diameter) (under production)\n4.3-136 (4000 kW, 136 m diameter) (under production)"]
[42,"Euroturbine","Netherlands","No longer exists","ET 500/36 (500 kW, 37 m diameter) (old model)\nET 550/41 (550 kW, 41 m diameter) (old model)"]
[43,"Eviag","Germany","No longer exists (2012)","ev2.93 (2050 kW, 93.2 m diameter) (old model)\nev90 (2500 kW, 90 m diameter) (old model)\nev100 (2500 kW, 100 m diameter) (old model)"]
[44,"EWT","Netherlands",null,"Directwind 250/52 (250 kW, 51.5 m diameter) (under production)\nDirectwind 250/54 (250 kW, 54 m diameter) (under production)\nDirectwind 500/52 (500 kW, 51.5 m diameter) (under production)\nDirectwind 500/54 (500 kW, 54 m diameter) (under production)\nDirectwind 52/750 (750 kW, 51.5 m diameter) (old model)\nDirectwind 54/750 (750 kW, 54 m diameter) (old model)\nDirectwind 900/52 (900 kW, 51.5 m diameter) (under production)\nDirectwind 900/54 (900 kW, 54 m diameter) (under production)\nDirectwind 2000/90 (2000 kW, 90.5 m diameter) (old model)\nDirectwind 2000/96 (2000 kW, 96 m diameter) (old model)"]
[45,"Fuhrländer","Germany","No longer exists (2013)","FL 100/21 (100 kW, 21 m diameter) (old model)\nFL 250/30 (250 kW, 29.5 m diameter) (old model)\nFL 600/50 (600 kW, 50 m diameter) (old model)\nFL 850/56 (850 kW, 56 m diameter) (old model)\nFL 1000/54 (1000 kW, 54 m diameter) (old model)\nFL 1250/62 (1250 kW, 62 m diameter) (old model)\nFL MD/70 (1500 kW, 70 m diameter) (old model)\nFL 1500/70 (1500 kW, 70 m diameter) (old model)\nFL MD/77 (1500 kW, 77 m diameter) (old model)\nFL 1500/77 (1500 kW, 77 m diameter) (old model)\nFL 2000/93 (2000 kW, 93 m diameter) (old model)\nFL 2500/80 (2500 kW, 80 m diameter) (old model)\nFL 2500/90 (2500 kW, 90 m diameter) (old model)\nFL 2500/100 (2500 kW, 100 m diameter) (old model)\nFL 2500/104 (2500 kW, 104 m diameter) (old model)\nFL 3000/120 (3000 kW, 120 m diameter) (old model)"]
[46,"FWT","Germany",null,"FWT2000/93 (2000 kW, 93 m diameter) (under production)\nFWT2000/100 (2000 kW, 100 m diameter) (under production)\nFWT2500/90 (2500 kW, 90 m diameter) (under production)\nFWT2500/100 (2500 kW, 100 m diameter) (under production)\nFWT2500/104 (2500 kW, 104 m diameter) (under production)\nFWT3000/120 (3000 kW, 120 m diameter) (under production)"]
[47,"Gamesa","Spain",null,"G42/600 (600 kW, 42 m diameter) (old model)\nG44/600 (600 kW, 44 m diameter) (old model)\nG47/660 (660 kW, 47 m diameter) (old model)\nG48/660 (660 kW, 48 m diameter) (old model)\nG52/850 (850 kW, 52 m diameter) (under production)\nG58/850 (850 kW, 58 m diameter) (under production)\nG66/1600 (1600 kW, 66 m diameter) (old model)\nG80/2000 (2000 kW, 80 m diameter) (under production)\nG83/2000 (2000 kW, 83 m diameter) (old model)\nG87/2000 (2000 kW, 87 m diameter) (under production)\nG90/2000 (2000 kW, 90 m diameter) (under production)\nG97/2000 (2000 kW, 97 m diameter) (under production)\nG114/2000 (2000 kW, 114 m diameter) (under production)\nG106/2500 (2500 kW, 106 m diameter) (under production)\nG114/2500 (2500 kW, 114 m diameter) (under development)\nG128/4500 (4500 kW, 128 m diameter) (under production)\nG128/5000 (5000 kW, 128 m diameter) (under production)\nG132/5000 (5000 kW, 132 m diameter) (under development)\nG14X/7000 (7000 kW, 145 m diameter) (under development)"]
[48,"Garuda","India",null,"700.54 (700 kW, 54 m diameter) (under production)\n1700.84 (1700 kW, 84 m diameter) (under production)"]
[49,"GC China Turbine Corp","China",null,"GC54 (1000 kW, 54 m diameter) (under production)\nGC57 (1000 kW, 57 m diameter) (under production)\nGC59 (1000 kW, 59 m diameter) (under production)"]
[50,"GE Energy","USA",null,"1.5s (1500 kW, 70.5 m diameter) (old model)\n1.5se (1500 kW, 70.5 m diameter) (old model)\n1.6sle (1500 kW, 77 m diameter) (old model)\n1.5sl (1500 kW, 77 m diameter) (old model)\n1.5sle (1500 kW, 77 m diameter) (old model)\n1.5-77 (1500 kW, 77 m diameter) (old model)\n1.5xle (1500 kW, 82.5 m diameter) (old model)\n1.6-82.5 (1600 kW, 82.5 m diameter) (old model)\n1.6xle (1600 kW, 82.5 m diameter) (old model)\n1.6-100 (1600 kW, 100 m diameter) (under production)\n1.62-87 (1620 kW, 87 m diameter) (old model)\n1.7-100 (1700 kW, 100 m diameter) (under production)\n1.85-82.5 (1850 kW, 82.5 m diameter) (under production)\n1.85-87 (1850 kW, 87 m diameter) (under production)\n2.3 (2300 kW, 94 m diameter) (old model)\n2.3-107 (2300 kW, 107 m diameter) (under production)\n2.5xl (2500 kW, 100 m diameter) (old model)\n2.5-100 (2500 kW, 100 m diameter) (old model)\n2.5-120 (2500 kW, 120 m diameter) (old model)\n2.75-100 (2750 kW, 100 m diameter) (old model)\n2.75-103 (2750 kW, 103 m diameter) (old model)\n2.75-120 (2750 kW, 120 m diameter) (under production)\n2.85-100 (2850 kW, 100 m diameter) (under production)\n2.85-100 (2850 kW, 100 m diameter) (old model)\n2.85-103 (2850 kW, 103 m diameter) (under production)\n3.0s (3000 kW, 90 m diameter) (old model)\n3.0sl (3000 kW, 94 m diameter) (old model)\nGE 3000 (3000 kW, 104 m diameter) (old model)\n3.2-103 (3200 kW, 103 m diameter) (under production)\n3.6sl (3600 kW, 111 m diameter) (old model)\n4.0-110 (4000 kW, 110 m diameter) (old model)\n4.1-113 (4100 kW, 113 m diameter) (under production)"]
[51,"Genesys","Germany","No longer exists","600 (600 kW, 46 m diameter) (old model)"]
[52,"GGS","Switzerland",null,"Falcon 1250 (1250 kW, 64 m diameter) (under production)\nAltanus 1.5 MW (1500 kW, 64 m diameter) (old model)"]
[53,"Ghodawat","India",null,"G1650 (1650 kW, 78 m diameter) (under production)"]
[54,"Global Wind Power","Denmark",null,"GWP47-750 (750 kW, 47 m diameter) (old model)\nGWP82-2000 (2000 kW, 82.5 m diameter) (old model)"]
[55,"Goldwind","China",null,"S43/600 (600 kW, 43 m diameter) (old model)\nS43/750 (750 kW, 43 m diameter) (old model)\nS48/750 (750 kW, 48 m diameter) (old model)\nGW50/750 (750 kW, 50 m diameter) (old model)\nS50/750 (750 kW, 50 m diameter) (old model)\nGW62/1200 (1200 kW, 62 m diameter) (old model)\nS62/1200 (1200 kW, 62 m diameter) (old model)\nS70/1500 (1500 kW, 70 m diameter) (old model)\nGW70/1500 (1500 kW, 70 m diameter) (under production)\nGW77/1500 (1500 kW, 77 m diameter) (under production)\nGW82/1500 (1500 kW, 82 m diameter) (under production)\nGW87/1500 (1500 kW, 87 m diameter) (under production)\nGW93/1500 (1500 kW, 93 m diameter) (under production)\nGW108/2000 (2000 kW, 108 m diameter) (under production)\nGW115/2000 (2000 kW, 115 m diameter) (under production)\nGW90/2500 (2500 kW, 90 m diameter) (under production)\nGW100/2500 (2500 kW, 100 m diameter) (under production)\nGW103/2500 (2500 kW, 103 m diameter) (old model)\nGW106/2500 (2500 kW, 106 m diameter) (under production)\nGW109/2500 (2500 kW, 109 m diameter) (under production)\nGW121/2500 (2500 kW, 121 m diameter) (under production)"]
[56,"Guangdong Mingyang","China",null,"MY1.5s (1500 kW, 77.1 m diameter) (old model)\nMY1.5su//77 (1500 kW, 77.1 m diameter) (under production)\nMY1.5su/83 (1500 kW, 82.6 m diameter) (under production)\nMY1.5se (1500 kW, 82.6 m diameter) (old model)\nMY1.5sh (1500 kW, 82.6 m diameter) (under production)\nSCD2500/92 (2500 kW, 92 m diameter) (under production)\nSCD2500/100 (2500 kW, 100 m diameter) (under production)\nSCD2500/108 (2500 kW, 108 m diameter) (under production)\nSCD2750 (2750 kW, 100 m diameter) (old model)\nSCD3000/92 (3000 kW, 92 m diameter) (under production)\nSCD3000/100 (3000 kW, 100 m diameter) (under production)\nSCD3000/108 (3000 kW, 108 m diameter) (under production)\n6.0 MW SCD (6000 kW, 140 m diameter) (under development)\n6.5 MW SCD (6500 kW, 150 m diameter) (under development)"]
[57,"Guodian","China",null,"UP77-IIa+ (1500 kW, 77.36 m diameter) (under production)\nUP77 (1500 kW, 77.36 m diameter) (under production)\nUP82-IIa+ (1500 kW, 82.76 m diameter) (under production)\nUP82 (1500 kW, 82.76 m diameter) (under production)\nUP86-IVb (1500 kW, 86.086 m diameter) (under production)\nUP86 (1500 kW, 86.086 m diameter) (under production)\nUP97 (1500 kW, 97 m diameter) (under production)\nUP103 (1900 kW, 103 m diameter) (under production)\nUP96 (2000 kW, 96 m diameter) (under production)\nUP103 (2000 kW, 103 m diameter) (under production)\nUP100-DD (3000 kW, 100 m diameter) (under production)\nUP100 (3000 kW, 100 m diameter) (under production)\nUP100/3000 IIA LT (3000 kW, 100 m diameter) (under production)\nUP108 (3000 kW, 108 m diameter) (old model)\nUP120/3000 IIIA (3000 kW, 120 m diameter) (under production)\nUP136 (6000 kW, 136 m diameter) (under production)\nUP154 (6000 kW, 154 m diameter) (under development)"]
[58,"Hanjin","South Korea",null,"HJWT1500/77 (1500 kW, 77 m diameter) (under production)\nHJWT2000/87 (2000 kW, 87 m diameter) (under production)\nHJWT2000/93 (2000 kW, 93 m diameter) (under production)"]
[59,"Hewind","China",null,"HW43 600 kW (600 kW, 43 m diameter) (old model)\nHW50 780 kW (780 kW, 50 m diameter) (under production)\nHW77 1.5 MW (1500 kW, 77 m diameter) (under production)\nHW82 1.5 MW (1500 kW, 82 m diameter) (old model)\nHW82 1.5 MW (1500 kW, 82 m diameter) (under production)\nHW87 1.5 MW (1500 kW, 87 m diameter) (under production)\nHW92 1.5 MW (1500 kW, 92 m diameter) (under production)\nHW110 2.0 MW (2000 kW, 110 m diameter) (under production)\nHW97 2.5 MW (2500 kW, 97 m diameter) (under production)\nHW103 2.5 MW (2500 kW, 103 m diameter) (under production)\nHW110 2.5 MW (2500 kW, 110 m diameter) (under production)\nHW152 6.0 MW (6000 kW, 152 m diameter) (under production)"]
[60,"Hitachi","Japan",null,"HTW2.0-80 (2000 kW, 80 m diameter) (under production)\nHTW5.0-126 (5000 kW, 126 m diameter) (under development)"]
[61,"HSW","Germany","No longer exists","250 (250 kW, 28 m diameter) (old model)\n750 (750 kW, 46 m diameter) (old model)\n1000 (1000 kW, 54 m diameter) (old model)"]
[62,"Hüllmann","Germany","No longer exists","FHW 100 (100 kW, 20 m diameter) (old model)"]
[63,"Hyosung","South Korea",null,"HS50-750MW (750 kW, 50 m diameter) (under production)\nHS90-2MW (2000 kW, 90.6 m diameter) (under production)"]
[64,"Hyundai","South Korea",null,"HQ1650/77 (1650 kW, 77 m diameter) (under production)\nHQ1650/82 (1650 kW, 82 m diameter) (old model)\nHQ2000/76 (2000 kW, 76 m diameter) (old model)\nHQ2000/86 (2000 kW, 86 m diameter) (under production)\nHQ2000/93 (2000 kW, 93 m diameter) (under production)\nAV928 (2500 kW, 93 m diameter) (old model)\nHQ5500/127 (5500 kW, 127 m diameter) (old model)\nHQ5500/140 (5500 kW, 140 m diameter) (under production)"]
[65,"HZ Windpower","China",null,"H56-850 (850 kW, 56.3 m diameter) (under production)\nH82-2000 (2000 kW, 82.4 m diameter) (under production)\nH87-2000 (2000 kW, 87 m diameter) (under production)\nH93-2000 (2000 kW, 92.8 m diameter) (under production)\nH102-2000 (2000 kW, 102 m diameter) (under production)\nH103-2500 (2500 kW, 103 m diameter) (under production)\nH127-5000 (5000 kW, 127 m diameter) (under development)\nH151-5000 (5000 kW, 151 m diameter) (under development)"]
[66,"IMPSA","Argentina",null,"IWP-70-1500 (1500 kW, 70 m diameter) (under production)\nIWP-V70-1500 (1500 kW, 70 m diameter) (under production)\nIWP-V77-1500 (1500 kW, 77 m diameter) (under production)\nIWP-V82-1500 (1500 kW, 82.3 m diameter) (under production)\nIWP-70-1800 (1800 kW, 70 m diameter) (under production)\nIWP-77-1800 (1800 kW, 77 m diameter) (old model)\nIWP-85-2000 (2000 kW, 85 m diameter) (under production)\nIWP-100-2000 (2000 kW, 100 m diameter) (under development)\nIWP-70-2100 (2100 kW, 70 m diameter) (old model)\nIWP-83-2100 (2100 kW, 83 m diameter) (under production)\nIWP-77-2200 (2200 kW, 77 m diameter) (old model)"]
[67,"India Wind Power","India","No longer exists","IWPL-29/250 (250 kW, 29.7 m diameter) (old model)"]
[68,"Inerjy","USA",null,"EcoVert 300 (250 kW, 15 m diameter) (old model)"]
[69,"Innovative Windpower","Germany","No longer exists","Falcon 1.25 MW-62 (1250 kW, 62 m diameter) (old model)\nFalcon 1.25 MW-64 (1250 kW, 64 m diameter) (old model)\nFalcon 1.25 MW-70 (1250 kW, 70 m diameter) (old model)"]
[70,"Inox Wind","India",null,"DF 93 (2000 kW, 93 m diameter) (under production)\nDF 100 (2000 kW, 100 m diameter) (under production)"]
[71,"ITP","Panama","No longer exists","250 kW (250 kW, 30 m diameter) (old model)\n900 kW - 51.5 (900 kW, 51.5 m diameter) (old model)\n900 kW - 54 (900 kW, 54 m diameter) (old model)"]
[72,"Jacobs","USA",null,"41/500 (500 kW, 41 m diameter) (old model)\n43/500 (500 kW, 43 m diameter) (old model)\n43/600 (600 kW, 43 m diameter) (old model)\n48/600 (600 kW, 48 m diameter) (old model)\n48/750 (750 kW, 48 m diameter) (old model)\nMD70 (1500 kW, 70 m diameter) (old model)\nMD77 (1500 kW, 77 m diameter) (old model)"]
[73,"Jeumont","France","No longer exists (2005)","J48/750 (750 kW, 48 m diameter) (old model)"]
[74,"JSW","Japan",null,"J82 (2000 kW, 83.3 m diameter) (under production)"]
[75,"Kenersys","Germany",null,"K82 (2000 kW, 82 m diameter) (under production)\nK120 (2300 kW, 120 m diameter) (under production)\nK110 (2400 kW, 110 m diameter) (under production)\nK100 (2500 kW, 100 m diameter) (under production)"]
[76,"Kenetech","USA","Acquired (1996)","USW56 (100 kW, 18 m diameter) (old model)\nUSW33 (360 kW, 33 m diameter) (old model)"]
[77,"Koncar","Croatia",null,"KO-VA 57/1 (1000 kW, 57 m diameter) (under production)\nK80 (2500 kW, 91 m diameter) (under production)"]
[78,"Lagerwey","Netherlands",null,"LW250-27 (250 kW, 27 m diameter) (old model)\nLW250-30 (250 kW, 30 m diameter) (old model)\nLW750-52 (750 kW, 52 m diameter) (old model)\nLW93/1500 (1500 kW, 93 m diameter) (under production)\nL100/1500 (1500 kW, 100 m diameter) (under production)\nL82/2000 (2000 kW, 82 m diameter) (under production)\nL90 (2500 kW, 90 m diameter) (old model)\nLW93/2500 (2500 kW, 93 m diameter) (old model)\nLW100/2500 (2500 kW, 100 m diameter) (under production)\nLW90/2600 (2600 kW, 90 m diameter) (old model)\nLW93/2600 (2600 kW, 93 m diameter) (under production)\nLW100/3000 (3000 kW, 100 m diameter) (old model)\nLW136/3600 (3600 kW, 136 m diameter) (under production)\nLW132/3800 (3800 kW, 132 m diameter) (old model)"]
[79,"Leitwind","Italy",null,"LTW77-800 (800 kW, 77 m diameter) (under production)\nLTW77-850 (850 kW, 77 m diameter) (under production)\nLTW80-850 (850 kW, 85 m diameter) (old model)\nLTW77-1000 (1000 kW, 77 m diameter) (under production)\nLTW80-1000 (1000 kW, 80 m diameter) (under production)\nLTW62 (1200 kW, 62 m diameter) (old model)\nLTW77-1350 (1350 kW, 77 m diameter) (old model)\nLTW70-1500 (1500 kW, 70 m diameter) (old model)\nLTW77-1500 (1500 kW, 76.8 m diameter) (under production)\nLTW80-1500 (1500 kW, 80.3 m diameter) (under production)\nLTW86-1500 (1500 kW, 86 m diameter) (under production)\nLTW70-1700 (1700 kW, 70 m diameter) (old model)\nLTW80-1800 (1800 kW, 80.3 m diameter) (under production)\nLTW70-2000 (2000 kW, 70.1 m diameter) (under production)\nLTW101-2000 (2000 kW, 101 m diameter) (under production)\nLTW104-2000 (2000 kW, 104.1 m diameter) (old model)\nLTW106 (2500 kW, 100 m diameter) (old model)\nLTW101-2500 (2500 kW, 101 m diameter) (under production)\nLTW104-2500 (2500 kW, 104.1 m diameter) (old model)\nLTW93 (3000 kW, 92.7 m diameter) (old model)\nLTW101-3000 (3000 kW, 101 m diameter) (under production)"]
[80,"M Torres (MTOI)","Spain",null,"MT TWT 77/1500 (1500 kW, 77 m diameter) (old model)\nMT TWT 70/1650 (1650 kW, 70 m diameter) (old model)\nMT TWT 77/1650 (1650 kW, 77 m diameter) (old model)\nMT TWT 82/1650 (1650 kW, 82 m diameter) (old model)\nMT TWT 90/2500 (2500 kW, 90 m diameter) (old model)\nMT TWT 100/2500 (2500 kW, 100 m diameter) (old model)\nMT TWT 109/2500 (2500 kW, 109 m diameter) (old model)"]
[81,"Made","Spain","Acquired (2003)","AE-20 (150 kW, 20 m diameter) (old model)\nAE-23 (180 kW, 23 m diameter) (old model)\nAE-30 (330 kW, 30 m diameter) (old model)\nAE-32 (330 kW, 32 m diameter) (old model)\nAE-45 (600 kW, 45 m diameter) (old model)\nAE-46/I (660 kW, 46 m diameter) (old model)\nAE-52 (800 kW, 52 m diameter) (old model)\nAE-56 (800 kW, 56 m diameter) (old model)\nAE-59 (800 kW, 59 m diameter) (old model)\nAE-61 (1320 kW, 61 m diameter) (old model)\nAE-90 (2000 kW, 90 m diameter) (old model)"]
[82,"Mapna Group","Iran",null,"Mapna 2.5 MW (2500 kW, 104 m diameter) (under production)"]
[83,"MBB","Germany","No longer exists","Monopteros M30 (200 kW, 33 m diameter) (old model)\nMonopteros M50 (1000 kW, 51 m diameter) (old model)"]
[84,"Mervento","Finland",null,"3.6-118 (3600 kW, 118 m diameter) (under production)"]
[85,"MHI Vestas Offshore","Denmark",null,"V112/3300 (3300 kW, 112 m diameter) (under production)\nV164/8000 (8000 kW, 164 m diameter) (under production)"]
[86,"Mitsubishi","Japan",null,"MWT-275-28 (275 kW, 28 m diameter) (old model)\nMWT-300-29 (300 kW, 29 m diameter) (old model)\nMWT-450-39 (450 kW, 39 m diameter) (old model)\nMHI500 (500 kW, 40 m diameter) (old model)\nMWT-600-45 (600 kW, 45 m diameter) (old model)\nMWT-600-47 (600 kW, 47 m diameter) (old model)\nMWT-1000-57 (1000 kW, 57 m diameter) (old model)\nMWT-1000-61 (1000 kW, 61.4 m diameter) (under production)\nMWT-92-2.3 (2300 kW, 92 m diameter) (old model)\nMWT-92 (2400 kW, 92 m diameter) (under production)\nMWT-95 (2400 kW, 95 m diameter) (under production)\nMWT-100-2.4 (2400 kW, 100 m diameter) (under production)\nMWT-102-2.4 (2400 kW, 102 m diameter) (under production)\nSeaAngel 7/165 (7000 kW, 165 m diameter) (under development)"]
[87,"Moncada Energy Group","Italy",null,"WPR 850/58 (850 kW, 58 m diameter) (under production)"]
[88,"Multibrid","France","Acquired (2007)","M5000 (5000 kW, 116 m diameter) (old model)"]
[89,"Navantia-Siemens","Spain","No longer exists","Bonus Mk-IV (600 kW, 44 m diameter) (old model)\nIzar 55/1300 (1300 kW, 55 m diameter) (old model)\nS-82 (2300 kW, 82 m diameter) (old model)"]
[90,"NedWind","Netherlands","No longer exists (1998)","35/500 (500 kW, 35 m diameter) (old model)\n40/500 (500 kW, 40 m diameter) (old model)\n44/500 (500 kW, 44 m diameter) (old model)\n53/1000 (1000 kW, 53 m diameter) (old model)"]
[91,"Neg Micon","Denmark","Acquired (2004)","M570 (200 kW, 27 m diameter) (old model)\nM700-225 (225 kW, 29.8 m diameter) (old model)\nM250/24 (250 kW, 24 m diameter) (old model)\nM530/24 (250 kW, 24 m diameter) (old model)\nM530 (250 kW, 26 m diameter) (old model)\nM750 (250 kW, 31 m diameter) (old model)\nM750-400/100 (400 kW, 31 m diameter) (old model)\nM400 (400 kW, 36 m diameter) (old model)\nM1500-500 (500 kW, 40 m diameter) (old model)\nNM43/600 (600 kW, 43 m diameter) (old model)\nM1500-600 (600 kW, 43 m diameter) (old model)\nM1800-600/44 (600 kW, 44 m diameter) (old model)\nM1800-600/46 (600 kW, 46 m diameter) (old model)\nNM600/48 (600 kW, 48 m diameter) (old model)\nM1800-600/48 (600 kW, 48 m diameter) (old model)\nM1500-750 (750 kW, 44 m diameter) (old model)\nNM44/750 (750 kW, 44 m diameter) (old model)\nM1500-750/48 (750 kW, 48 m diameter) (old model)\nNM48/750 (750 kW, 48 m diameter) (old model)\nM1800-750/48 (750 kW, 48 m diameter) (old model)\nNM52/900 (900 kW, 52 m diameter) (old model)\nNM950/54 (950 kW, 54 m diameter) (old model)\nNM60/1000 (1000 kW, 60 m diameter) (old model)\nNM64/1500 (1500 kW, 64 m diameter) (old model)\nNM64c/1500 (1500 kW, 64 m diameter) (old model)\nNM72c/1500 (1500 kW, 72 m diameter) (old model)\nNM82/1500 (1500 kW, 82 m diameter) (old model)\nNM72/1650 (1650 kW, 72 m diameter) (old model)\nNM82/1650 (1650 kW, 82 m diameter) (old model)\nNM72/2000 (2000 kW, 72 m diameter) (old model)\nNM72/2100 (2100 kW, 72 m diameter) (old model)\nNM80/2500 (2500 kW, 80 m diameter) (old model)\nNM80/2750 (2750 kW, 80 m diameter) (old model)\nNM92/2750 (2750 kW, 92 m diameter) (old model)\nNM80/2875 (2875 kW, 80 m diameter) (old model)"]
[92,"NEPC","India",null,"200/30 (200 kW, 30 m diameter) (under production)\n225/40 (225 kW, 29.8 m diameter) (under production)\n250/50 (250 kW, 27.6 m diameter) (old model)\n250/31 (250 kW, 31 m diameter) (under production)\n400/100 (400 kW, 31 m diameter) (old model)"]
[93,"Nordex","Germany",null,"N27/150 (150 kW, 27 m diameter) (old model)\nN27/225 (225 kW, 27 m diameter) (old model)\nN27/250 (250 kW, 27 m diameter) (old model)\nN29/250 (250 kW, 29 m diameter) (old model)\nS43 (600 kW, 43 m diameter) (old model)\nN43/600 (600 kW, 43 m diameter) (old model)\nN50/800 (800 kW, 50 m diameter) (old model)\nN52/800 (800 kW, 52 m diameter) (old model)\nN54/1000 (1000 kW, 54 m diameter) (old model)\nN56/1300 (1300 kW, 56 m diameter) (old model)\nN60/1300 (1300 kW, 60 m diameter) (old model)\nS62 (1300 kW, 62 m diameter) (old model)\nN62/1300 (1300 kW, 62 m diameter) (old model)\nS70 (1500 kW, 70 m diameter) (old model)\nS77 (1500 kW, 77 m diameter) (old model)\nN77 (1500 kW, 77 m diameter) (old model)\nN82 (1500 kW, 82 m diameter) (old model)\nS82 (1500 kW, 82 m diameter) (old model)\nN90/2300 (2300 kW, 90 m diameter) (old model)\nN80/2400 (2400 kW, 80 m diameter) (old model)\nN117/2400 (2400 kW, 117 m diameter) (under production)\nN80/2500 (2500 kW, 80 m diameter) (old model)\nN90/2500 Offshore (2500 kW, 90 m diameter) (under production)\nN90/2500 (2500 kW, 90 m diameter) (under production)\nN100/2500 (2500 kW, 100 m diameter) (under production)\nN117/3000 (3000 kW, 116.8 m diameter) (under production)\nN131 (3000 kW, 131 m diameter) (under production)\nN100/3300 (3300 kW, 99.8 m diameter) (under production)\nN150/6000 (6000 kW, 150 m diameter) (under development)"]
[94,"Nordic Windpower","USA","No longer exists","N1000-54 (1000 kW, 54 m diameter) (old model)\nN1000-59 (1000 kW, 59 m diameter) (old model)"]
[95,"Nordtank","Denmark","Acquired (1997)","NTK130/22 (130 kW, 22 m diameter) (old model)\nNTK150/16 (150 kW, 16 m diameter) (old model)\n150XLR (150 kW, 24.6 m diameter) (old model)\nNTK150/25 (150 kW, 25 m diameter) (old model)\nNTK300/31 (300 kW, 31 m diameter) (old model)\nNTK500/37 (500 kW, 37 m diameter) (old model)\nNTK550/41 (550 kW, 41 m diameter) (old model)\nNTK600/43 (600 kW, 43 m diameter) (old model)\nNTK1500/60 (1500 kW, 63 m diameter) (old model)"]
[96,"Nordwind","Germany",null,"NW 22-150 HY-P (150 kW, 22.06 m diameter) (old model)\nNW 44-500 (500 kW, 44 m diameter) (under development)\nNW 47-850 HY-P (850 kW, 47.75 m diameter) (old model)"]
[97,"Northern Power Systems","USA",null,"NPS 100C-21 (100 kW, 20.7 m diameter) (under production)\nNorthern Power 100 (100 kW, 21 m diameter) (old model)\nNorthern Power 100 Artic (100 kW, 21 m diameter) (old model)\nNPS 100C-24 (100 kW, 24.4 m diameter) (under production)\nNorthern Power 2.0/110 (2000 kW, 110 m diameter) (under production)\nNorthern Power 2.2/100 (2200 kW, 100 m diameter) (under production)\nNorthern Power 2.3/93 (2300 kW, 93 m diameter) (under production)"]
[98,"Norwin","Denmark",null,"29-STALL-200 kW (200 kW, 29 m diameter) (under production)\n33-STALL-200 kW (200 kW, 33 m diameter) (old model)\n29-STALL-225 kW (225 kW, 29 m diameter) (under production)\n47-ASR-500 kW (500 kW, 47 m diameter) (under production)\n46-ASR-599 kW (599 kW, 46 m diameter) (old model)\n46-ASR-750 kW (750 kW, 46 m diameter) (old model)\n47-ASR-750 kW (750 kW, 47 m diameter) (under production)\n54-ASR-750 kW (750 kW, 54 m diameter) (under production)"]
[99,"NRG Patagonia","Argentina",null,"NRG 1500 (1500 kW, 60 m diameter) (old model)\nNRGP 64 (1500 kW, 64 m diameter) (under production)\nNRGP 82 (1500 kW, 82 m diameter) (under production)"]
[100,"Palmtree Power","South Africa",null,"Palmtree 300 (300 kW, 32 m diameter) (under production)"]
[101,"Pioneer Power Solutions","USA",null,"P1650 -70 (1650 kW, 70 m diameter) (old model)\nP1650 -77 (1650 kW, 77 m diameter) (old model)\nP1650 -80 (1650 kW, 80 m diameter) (old model)"]
[102,"Pioneer Wincon","India",null,"P250/29 (250 kW, 29 m diameter) (under production)\nP750/49 (750 kW, 49 m diameter) (under production)"]
[103,"Polaris America","USA",null,"100 kW (100 kW, 19.1 m diameter) (old model)\n100 kW/21 (100 kW, 21 m diameter) (under production)"]
[104,"PowerWind","India",null,"500 (500 kW, 56 m diameter) (under production)\n60 (850 kW, 60 m diameter) (under production)\n56 (900 kW, 56 m diameter) (under production)\n90 (2500 kW, 90 m diameter) (under production)\n100 (2500 kW, 100 m diameter) (under production)"]
[105,"Prokon","Germany",null,"P3000/110 (3000 kW, 110 m diameter) (old model)\nP3000/116 (3000 kW, 116 m diameter) (old model)"]
[106,"Regen Powertech","India",null,"Vensys V70 (1500 kW, 70 m diameter) (old model)\nVensys V77 (1500 kW, 77 m diameter) (under production)\nVensys V82 (1500 kW, 82.3 m diameter) (under production)\nVensys V87 (1500 kW, 87 m diameter) (under production)"]
[107,"Repower (Senvion)","Germany","No longer exists (2014)","57/1000 (1000 kW, 57 m diameter) (old model)\nMD70 (1500 kW, 70 m diameter) (old model)\nMD77 (1500 kW, 77 m diameter) (old model)\nMM100/1800 (1800 kW, 100 m diameter) (old model)\nMM70 (2000 kW, 70 m diameter) (old model)\nMM82 (2000 kW, 82 m diameter) (old model)\nMM82 Evo (2000 kW, 82 m diameter) (old model)\nMM92 Evo (2000 kW, 92 m diameter) (old model)\nMM92 (2000 kW, 92 m diameter) (old model)\n5M (5000 kW, 126 m diameter) (old model)"]
[108,"RRB Energy","India",null,"V27-225 (225 kW, 27 m diameter) (under production)\nV39-500 (500 kW, 47 m diameter) (under production)\nPS-600 (600 kW, 47 m diameter) (under production)\nPS-1800 (1800 kW, 82 m diameter) (under production)"]
[109,"Sabaniroo","Iran",null,"S47-660 (660 kW, 47 m diameter) (under production)"]
[110,"Samsung","South Korea",null,"25s (2500 kW, 90 m diameter) (under production)\n25x (2500 kW, 99.8 m diameter) (under production)\n7.0-171 (7000 kW, 171.2 m diameter) (under development)"]
[111,"Sany","China",null,"SE7715 (1500 kW, 77.7 m diameter) (under production)\nSE7715-L (1500 kW, 77.7 m diameter) (under production)\nSE8215 (1500 kW, 83.3 m diameter) (under production)\nSE8215-L (1500 kW, 83.3 m diameter) (under production)\nSE8215-3 (1500 kW, 83.3 m diameter) (old model)\nSE8715-L (1500 kW, 86.7 m diameter) (under production)\nSE8715 (1500 kW, 86.7 m diameter) (under production)\nSE8220III (2000 kW, 82.5 m diameter) (under production)\nSE8720III (2000 kW, 87 m diameter) (under production)\nSE8720IIIE60HZ (2000 kW, 87 m diameter) (under production)\nSE9320III-S3 (2000 kW, 93 m diameter) (under production)\nSE9320III-3 (2000 kW, 93 m diameter) (under production)\nSE11030III-S (3000 kW, 110 m diameter) (under production)"]
[112,"Scanwind","USA","Acquired (2009)","SW-90-3500 DL (3500 kW, 91 m diameter) (old model)\nSW-100-3500 DL (3500 kW, 100 m diameter) (old model)"]
[113,"Schuler Pressen","Germany",null,"SDD 100 (2700 kW, 100 m diameter) (old model)"]
[114,"Senvion","Germany","Acquired (2009)","MM100 (2000 kW, 100 m diameter) (under production)\nMM82/2050 (2050 kW, 82 m diameter) (under production)\nMM92/2050 (2050 kW, 92 m diameter) (under production)\n3.0M122 (3000 kW, 122 m diameter) (under production)\n3.2M114 (3200 kW, 114 m diameter) (under production)\n3.4M104 (3400 kW, 104 m diameter) (under production)\n3.4M114 (3400 kW, 114 m diameter) (under development)\n6M126 (6150 kW, 126 m diameter) (under production)\n6.2M152 (6150 kW, 152 m diameter) (under production)"]
[115,"Shandong Swiss Electric","China",null,"YZ70/1.5 (1500 kW, 70 m diameter) (under production)\nYZ77/1.5 (1500 kW, 77 m diameter) (old model)\nYZ78/1.5 (1500 kW, 78 m diameter) (under production)\nYZ82/1.5 (1500 kW, 82 m diameter) (under production)\nYZ77/2.0 (2000 kW, 77 m diameter) (under production)\nYZ82/2.0 (2000 kW, 82 m diameter) (under production)\nYZ87/2.0 (2000 kW, 87 m diameter) (under production)\nYZ88/2.5 (2500 kW, 88 m diameter) (old model)\nYZ90/2.5 (2500 kW, 90 m diameter) (old model)\nYZ97/2.5 (2500 kW, 97 m diameter) (old model)\nYZ100/3.0 (3000 kW, 100 m diameter) (under production)\nYZ103/3.0 (3000 kW, 103 m diameter) (old model)\nYZ105/3.0 (3000 kW, 105 m diameter) (under production)\nYZ113/3.0 (3000 kW, 113 m diameter) (under production)\nYZ127/6.0 (6000 kW, 127 m diameter) (under development)\nYZ150/10 (10000 kW, 150 m diameter) (under development)"]
[116,"Shanghai Electric","China",null,"W1250/62 (1250 kW, 62.3 m diameter) (under production)\nW1250/64 (1250 kW, 64.3 m diameter) (under production)\nW1250/70 (1250 kW, 70.3 m diameter) (under production)\nW2000/87 (2000 kW, 87 m diameter) (under production)\nW2000/93 (2000 kW, 93 m diameter) (under production)\nW2000/99 (2000 kW, 99 m diameter) (under production)\nW2000/105 (2000 kW, 105 m diameter) (under production)\nW3600/116 (3600 kW, 116 m diameter) (under production)\nW3600/122 (3600 kW, 122 m diameter) (under production)"]
[117,"Shanghai Wande Wind Power","China",null,"WD59-1250 (1250 kW, 59 m diameter) (under production)\nWD71-1500/12 (1500 kW, 71 m diameter) (under production)\nWD77-1500/11 (1500 kW, 77 m diameter) (under production)\nW82-2000 (2000 kW, 82 m diameter) (under production)"]
[118,"Shriram EPC","India","No longer exists","SEPC 250T (250 kW, 28.5 m diameter) (old model)"]
[119,"Siemens","Germany",null,"SWT-1.0-54 (1000 kW, 54 m diameter) (old model)\nSWT-1.3-62 (1300 kW, 62 m diameter) (old model)\nSWT-2.3-82 (2300 kW, 82 m diameter) (old model)\nSWT-2.3-82 VS (2300 kW, 82.4 m diameter) (old model)\nSWT-2.3-93 (2300 kW, 93 m diameter) (old model)\nSWT-2.3-101 DD (2300 kW, 101 m diameter) (old model)\nSWT-2.3-101 (2300 kW, 101 m diameter) (under production)\nSWT-2.3-108 (2300 kW, 108 m diameter) (under production)\nSWT-2.3-113 (2300 kW, 113 m diameter) (old model)\nSWT-2.35-108 (2350 kW, 108 m diameter) (old model)\nSWT-2.5-108 (2500 kW, 108 m diameter) (old model)\nSWT-3.0-101 (3000 kW, 101 m diameter) (under production)\nSWT-3.0-108 (3000 kW, 108 m diameter) (under production)\nSWT-3.0-113 (3000 kW, 113 m diameter) (under production)\nSWT-3.2-101 (3200 kW, 101 m diameter) (under production)\nSWT-3.2-108 (3200 kW, 108 m diameter) (under production)\nSWT-3.2-113 (3200 kW, 113 m diameter) (under production)\nSWT-3.3-130 (3300 kW, 130 m diameter) (under production)\nSWT-3.6-107 (3600 kW, 107 m diameter) (old model)\nSWT-3.6-120 (3600 kW, 120 m diameter) (under production)\nSWT-4.0-120 (4000 kW, 120 m diameter) (under production)\nSWT-4.0-130 (4000 kW, 130 m diameter) (under production)\nSWT-6.0-120 (6000 kW, 120 m diameter) (old model)\nSWT-6.0-154 (6000 kW, 154 m diameter) (under production)\nSWT-7.0-154 (7000 kW, 154 m diameter) (under development)"]
[120,"Sinovel","China",null,"SL 1500/60 (1500 kW, 60 m diameter) (under production)\nFD70B (1500 kW, 70 m diameter) (old model)\nFL1500/70 (1500 kW, 70 m diameter) (old model)\nSL 1500/70 (1500 kW, 70.4 m diameter) (under production)\nGTW 1500KW (1500 kW, 77 m diameter) (old model)\nFL1500/77 (1500 kW, 77 m diameter) (old model)\nSL 1500/77 (1500 kW, 77.4 m diameter) (under production)\nSL 1500/82 (1500 kW, 82.9 m diameter) (under production)\nSL 3000/90 (3000 kW, 90 m diameter) (under production)\nSL 3000/100 (3000 kW, 100 m diameter) (under production)\nSL 3000/105 (3000 kW, 105 m diameter) (under production)\nSL 3000/113 (3000 kW, 113 m diameter) (under production)\nSL 3600/116 (3600 kW, 116 m diameter) (old model)\nSL 5000 (5000 kW, 128 m diameter) (under production)\nSL 6000 (6000 kW, 128 m diameter) (under production)"]
[121,"SIVA","India",null,"100 (100 kW, 29 m diameter) (under production)\n200 (200 kW, 30 m diameter) (under production)\n225/40 (225 kW, 30 m diameter) (under production)\n250/50 (250 kW, 30 m diameter) (under production)"]
[122,"Southern Wind Farms","India",null,"GWL225/40 (225 kW, 29.8 m diameter) (under production)"]
[123,"Soyut Wind","Turkey",null,"Soyut Wind 100 (100 kW, 26 m diameter) (under production)\nSoyut Wind 200 (200 kW, 36.8 m diameter) (under production)\nSoyut Wind 250 (250 kW, 41.2 m diameter) (under production)\nSoyut Wind 300 (300 kW, 41.2 m diameter) (old model)\nSoyut Wind 500 (500 kW, 39.2 m diameter) (under production)\nSoyut Wind 1000 (1000 kW, 55.5 m diameter) (under production)\nSoyut Wind 1650 (1650 kW, 55.5 m diameter) (under production)"]
[124,"SRC Green Power","India",null,"SRC 200/30 (200 kW, 29.8 m diameter) (under production)\nSRC 225/30 (225 kW, 29.8 m diameter) (under production)\nSRC 250/50 (250 kW, 31 m diameter) (under production)"]
[125,"Statoil","Norway",null,"Hywind (2300 kW, 82.4 m diameter) (under development)"]
[126,"STX Windpower","Netherlands",null,"STX72 1.5 MW (1500 kW, 70.65 m diameter) (under production)\nSTX82 1.5 MW (1500 kW, 82.7 m diameter) (old model)\nSTX72 (2000 kW, 70.65 m diameter) (under production)\nSTX82 2.0 MW (2000 kW, 82.7 m diameter) (old model)\nSTX93 2.0 MW (2000 kW, 93.3 m diameter) (under production)"]
[127,"Subaru","Japan","Acquired (#NA)","Subaru 40 (100 kW, 22 m diameter) (old model)\nSubaru 80/2.0 (2000 kW, 80 m diameter) (old model)"]
[128,"Südwind","Germany","No longer exists","S31/250 (250 kW, 31 m diameter) (old model)\nS48/600 (600 kW, 48 m diameter) (old model)\nS70/1500 (1500 kW, 70 m diameter) (old model)\nS77/1500 (1500 kW, 77 m diameter) (old model)"]
[129,"SUREnergy","USA",null,"SURNPS 21-100 (100 kW, 21 m diameter) (under production)\nSURNPS 29-225 (225 kW, 29.1 m diameter) (under production)\nSURNPS 47-600 (600 kW, 47 m diameter) (under production)\nSURNPS 69-750 (750 kW, 51.5 m diameter) (old model)\nSURNPS 54-750 (750 kW, 54 m diameter) (under production)\nSURNPS 57-750 (750 kW, 57 m diameter) (under production)\nSURNPS 54-1000 (1000 kW, 54 m diameter) (under production)\nSURNPS 59-1000 (1000 kW, 59 m diameter) (under production)"]
[130,"Suzlon","India",null,"S33/350 (350 kW, 33 m diameter) (old model)\nS52/600 (600 kW, 52 m diameter) (under production)\nS64/950 (950 kW, 64 m diameter) (old model)\nS60/1000 (1000 kW, 60 m diameter) (old model)\nS62/1000 (1000 kW, 62 m diameter) (old model)\nS64/1250 (1250 kW, 64 m diameter) (old model)\nS66/1250 (1250 kW, 66 m diameter) (under production)\nS70/1250 (1250 kW, 70 m diameter) (old model)\nS82/1500 (1500 kW, 82 m diameter) (under production)\nS88/2100 (2100 kW, 88 m diameter) (under production)\nS95/2100 (2100 kW, 95 m diameter) (old model)\nS97/2100 (2100 kW, 97 m diameter) (under production)\nS111/2100 (2100 kW, 111 m diameter) (under production)\nS88/2250 (2250 kW, 88 m diameter) (old model)"]
[131,"Sway","Norway",null,"10 MW (10000 kW, 145 m diameter) (under development)"]
[132,"Tacke","Germany","No longer exists (1997)","TW-250 (250 kW, 26 m diameter) (old model)\nTW-500 (500 kW, 37 m diameter) (old model)\nTW-600 (600 kW, 43 m diameter) (old model)\n1.5i (1500 kW, 65 m diameter) (old model)\n1.5s (1500 kW, 77 m diameter) (old model)"]
[133,"Turbowinds","Belgium",null,"T300-28 (300 kW, 28 m diameter) (under production)\nT400-34 (400 kW, 34 m diameter) (under production)\nT500-48 (500 kW, 48 m diameter) (under production)\nT600-48 (600 kW, 48 m diameter) (under production)"]
[134,"Unison","South Korea",null,"U50 (750 kW, 50 m diameter) (under production)\nU54 (750 kW, 54 m diameter) (under production)\nU57 (750 kW, 57 m diameter) (under production)\nU88 (2000 kW, 88 m diameter) (under production)\nU93 (2000 kW, 93 m diameter) (under production)"]
[135,"Vensys","Germany","Acquired (2008)","62 (1200 kW, 62 m diameter) (old model)\n64 (1200 kW, 64 m diameter) (old model)\n70 (1500 kW, 70 m diameter) (under production)\n77 (1500 kW, 77 m diameter) (under production)\n82 (1500 kW, 82.3 m diameter) (under production)\n87 (1500 kW, 87 m diameter) (under production)\n90 (2500 kW, 90 m diameter) (old model)\n100 (2500 kW, 99.8 m diameter) (under production)\n109 (2500 kW, 109 m diameter) (under production)\n112 (2500 kW, 112 m diameter) (under production)\n112-3000 (3000 kW, 112 m diameter) (under production)\n120 (3000 kW, 120 m diameter) (under production)"]
[136,"Vergnet","France",null,"GEV 10/15 (15 kW, 10 m diameter) (old model)\nGEV 10/20 (20 kW, 10 m diameter) (old model)\nGEV 15/40 (40 kW, 15 m diameter) (old model)\nGEV 15/60 (60 kW, 15 m diameter) (old model)\nGEV 26/200 (200 kW, 26 m diameter) (old model)\nGEV MP 200/28 (200 kW, 28 m diameter) (old model)\nGEV MP 200/30 (200 kW, 30 m diameter) (under production)\nGEV MP 200/32 (200 kW, 32 m diameter) (under production)\nGEV 26/220 (220 kW, 26 m diameter) (old model)\nGEV MP 250/28 (250 kW, 28 m diameter) (old model)\nGEV MP 250/30 (250 kW, 30 m diameter) (under production)\nGEV MP 250/32 (250 kW, 32 m diameter) (under production)\nGEV MP 275/28 (275 kW, 28 m diameter) (old model)\nGEV MP 275/30 (275 kW, 30 m diameter) (under production)\nGEV MP 275/32 (275 kW, 32 m diameter) (under production)\nGEV HP 1000/55 (1000 kW, 55 m diameter) (under production)\nGEV HP 1000/58 (1000 kW, 58 m diameter) (under production)\nGEV HP 1000/62 (1000 kW, 62 m diameter) (under production)"]
[137,"Vestas","Denmark",null,"V20/100 (100 kW, 20 m diameter) (old model)\nV23/150 (150 kW, 23 m diameter) (old model)\nV23/200 (200 kW, 23 m diameter) (old model)\nV25/200 (200 kW, 25 m diameter) (old model)\nV27/225 (225 kW, 27 m diameter) (old model)\nV29/225 (225 kW, 29 m diameter) (old model)\nV27/270 (270 kW, 27 m diameter) (old model)\nWD34 (400 kW, 34 m diameter) (old model)\nV34/400 (400 kW, 34.8 m diameter) (old model)\nV39/500 (500 kW, 39 m diameter) (old model)\nV42/500 (500 kW, 42 m diameter) (old model)\nV39/600 (600 kW, 39 m diameter) (old model)\nV42/600 (600 kW, 42 m diameter) (old model)\nV44/600 (600 kW, 44 m diameter) (old model)\nV47/660 (660 kW, 47 m diameter) (old model)\nNM44 (750 kW, 44 m diameter) (old model)\nNM48 (750 kW, 48 m diameter) (old model)\nV52/850 (850 kW, 52 m diameter) (old model)\nV60/850 (850 kW, 60 m diameter) (old model)\nV60/850 (850 kW, 60 m diameter) (old model)\nNM52 (900 kW, 52 m diameter) (old model)\nMultipower 52 (900 kW, 52 m diameter) (old model)\nNM60 (1000 kW, 60 m diameter) (old model)\nNM64 (1500 kW, 64 m diameter) (old model)\nM64 Lownoise (1500 kW, 64 m diameter) (old model)\nNM72 (1500 kW, 72 m diameter) (old model)"]
[null,null,null,null,"V82/1500 (1500 kW, 82 m diameter) (old model)\nNM82 (1500 kW, 82 m diameter) (old model)\nV66/1650 (1650 kW, 66 m diameter) (old model)\nV70/1650 (1650 kW, 70 m diameter) (old model)\nNM82/1650 (1650 kW, 82 m diameter) (old model)\nV82/1650 (1650 kW, 82 m diameter) (old model)\nV66/1750 (1750 kW, 66 m diameter) (old model)\nV80/1800 (1800 kW, 80 m diameter) (old model)\nV90/1800 (1800 kW, 90 m diameter) (under production)\nV100/1800 (1800 kW, 100 m diameter) (under production)\nV80/2000 (2000 kW, 80 m diameter) (old model)\nV90/2000 (2000 kW, 90 m diameter) (under production)\nV100/2000 (2000 kW, 100 m diameter) (under production)\nV110/2000 (2000 kW, 110 m diameter) (under production)\nV100/2600 (2600 kW, 100 m diameter) (old model)\nV100/2750 (2750 kW, 100 m diameter) (old model)\nV90/3000 (3000 kW, 90 m diameter) (old model)\nV90/3000 Offshore (3000 kW, 90 m diameter) (old model)\nV100/3000 (3000 kW, 100 m diameter) (old model)\nV112/3000 Offshore (3000 kW, 112 m diameter) (old model)\nV112/3000 (3000 kW, 112 m diameter) (old model)\nV126/3000 (3000 kW, 126 m diameter) (old model)\nV105/3300 (3300 kW, 105 m diameter) (under production)\nV112/3300 (3300 kW, 112 m diameter) (under production)\nV117/3300 (3300 kW, 117 m diameter) (under production)\nV126/3300 (3300 kW, 126 m diameter) (old model)\nV126/3300 (3300 kW, 126 m diameter) (under production)\nV112/3450 (3450 kW, 112 m diameter) (under production)\nV164/7000 (7000 kW, 164 m diameter) (old model)\nV164/8000 (8000 kW, 164 m diameter) (under production)"]
[138,"Vindsyssel","Denmark","No longer exists","VS130/22 (130 kW, 22 m diameter) (old model)\nVS150/22 (150 kW, 22 m diameter) (old model)\nVS270/26 (270 kW, 26 m diameter) (old model)"]
[139,"W2E","Germany",null,"FL1250 (1300 kW, 62 m diameter) (old model)\n2.0 MW/93 (2000 kW, 93 m diameter) (under production)\n2.0 MW/100 (2000 kW, 100 m diameter) (under production)\nHarvester 2.0 MW (2000 kW, 116 m diameter) (under production)\nW2E-93/2.0 (2050 kW, 93.2 m diameter) (old model)\nW2E-100/2.0 (2050 kW, 100 m diameter) (old model)\nW80 (2500 kW, 80 m diameter) (old model)\nW90 (2500 kW, 90 m diameter) (old model)\n2.5 MW/100 (2500 kW, 100 m diameter) (under production)\nW2E-100/2.5 (2500 kW, 100 m diameter) (old model)\nW2E-103/2.5 (2500 kW, 103 m diameter) (old model)\n2.5 MW/103 (2500 kW, 103 m diameter) (under production)\n3.0 MW/120 (3000 kW, 120 m diameter) (under production)\nW2E-120/3fc (3300 kW, 120 m diameter) (old model)\nHarvester 3.3 MW (3300 kW, 130 m diameter) (under production)"]
[140,"WEG","Brazil",null,"AGW 110/2.1 (2100 kW, 110 m diameter) (under production)"]
[141,"WES","Netherlands",null,"WES100 (100 kW, 18 m diameter) (under production)\nWES200 (200 kW, 30 m diameter) (old model)\nWES30 Mk1 (250 kW, 30 m diameter) (under production)"]
[142,"WESPA","Italy",null,"WESPA 200/29 (200 kW, 29 m diameter) (under production)\nWESPA 200/31 (200 kW, 31 m diameter) (under production)\nWESPA 200/33 (200 kW, 33 m diameter) (under production)\nWESPA 225/29 (225 kW, 29 m diameter) (old model)\nWESPA 250/31 (250 kW, 31 m diameter) (under production)\nWESPA 500/47 (500 kW, 47 m diameter) (under production)\nWESPA 750/47 (750 kW, 47 m diameter) (under production)\nWESPA 750/54 (750 kW, 54 m diameter) (under production)"]
[143,"Wikov","Czech Republic",null,"W2000/76 (2000 kW, 76 m diameter) (old model)\nW2000/86 (2000 kW, 86 m diameter) (old model)\nW2000/93 (2000 kW, 93 m diameter) (old model)"]
[144,"Wincon","Denmark","No longer exists","M100/19 (100 kW, 19 m diameter) (old model)\nW200/24 (200 kW, 24 m diameter) (old model)\nW200/26 (200 kW, 26 m diameter) (old model)\nW250/29 (250 kW, 26 m diameter) (old model)\nW600/45 (600 kW, 45 m diameter) (old model)"]
[145,"Wind Energy Group Ltd","United-Kingdom","No longer exists","MS3-300 (300 kW, 33 m diameter) (old model)"]
[146,"Wind Technik Nord","Germany",null,"200/26 (200 kW, 26 m diameter) (old model)\n200/28 (200 kW, 28 m diameter) (under production)\n250/30 (250 kW, 30 m diameter) (under production)\n500 (500 kW, 48 m diameter) (under production)\n646 (600 kW, 46 m diameter) (under production)\n648 (600 kW, 48 m diameter) (under production)"]
[147,"Wind World","Denmark","No longer exists","W120/21 (120 kW, 21 m diameter) (old model)\nW2250/140 (140 kW, 22.5 m diameter) (old model)\nW150/23 (150 kW, 23 m diameter) (old model)\nW2320/150 (150 kW, 23.2 m diameter) (old model)\nW2500/25 (150 kW, 25 m diameter) (old model)\nW150/27 (150 kW, 27 m diameter) (old model)\nW150/28 (150 kW, 28 m diameter) (old model)\nW2320/160 (160 kW, 23.2 m diameter) (old model)\nW2320/180 (180 kW, 23.2 m diameter) (old model)\nW2320/200 (200 kW, 23 m diameter) (old model)\nW2500/220 (220 kW, 25 m diameter) (old model)\nW2530/250 (250 kW, 25.3 m diameter) (old model)\nW250/29 (250 kW, 29 m diameter) (old model)\nW490/37 (490 kW, 37 m diameter) (old model)\nW3700/500 (500 kW, 37 m diameter) (old model)\nW600/42 (600 kW, 42 m diameter) (old model)\nW4800/750 (750 kW, 48 m diameter) (old model)\nW5200/750 (750 kW, 52 m diameter) (old model)"]
[148,"Windey","China",null,"WD25-250kW (250 kW, 25 m diameter) (old model)\nWD48-750 (750 kW, 48 m diameter) (old model)\nWD49-750kW (750 kW, 49 m diameter) (under production)\nWD50-750kW (750 kW, 49 m diameter) (under production)\nWD52-800kW (800 kW, 52 m diameter) (under production)\nWD70-1500 (1500 kW, 70 m diameter) (under production)\nWD77-1500 (1500 kW, 77 m diameter) (under production)\nWD82-1500 (1500 kW, 82 m diameter) (under production)\nWD92-2500 (2500 kW, 92 m diameter) (under production)\nWD100-2500 (2500 kW, 100 m diameter) (under production)\nWD103-2500 (2500 kW, 103 m diameter) (under production)"]
[149,"Windflow","New-Zealand",null,"Windflow 500 (500 kW, 33 m diameter) (under production)"]
[150,"Windmaster","Netherlands","No longer exists","WM22/150 (150 kW, 22 m diameter) (old model)\nWM22/200 (200 kW, 21.8 m diameter) (old model)\nWM28/300 (300 kW, 28 m diameter) (old model)\nWM33/500 (500 kW, 33 m diameter) (old model)\nWM40/750 (750 kW, 40 m diameter) (old model)\nWM43/750 (750 kW, 43 m diameter) (old model)"]
[151,"Windmatic","USA","No longer exists","WM20S (130 kW, 19 m diameter) (old model)\n150 (150 kW, 22 m diameter) (old model)\n180 (180 kW, 22 m diameter) (old model)\n200 (200 kW, 23 m diameter) (old model)"]
[152,"Windstrom Frisia","Germany","No longer exists","F48 (750 kW, 48 m diameter) (old model)\nF56 (850 kW, 56 m diameter) (old model)"]
[153,"Windtec","USA",null,"Floda 500 (500 kW, 36 m diameter) (old model)\nFloda 600 (600 kW, 45 m diameter) (old model)\n646 (600 kW, 46 m diameter) (old model)\n1566 (1500 kW, 66 m diameter) (old model)\n1570 (1500 kW, 70 m diameter) (old model)\nWT1650df/70 (1650 kW, 70 m diameter) (old model)\nWT1650df/77 (1650 kW, 77 m diameter) (under production)\nWT1650df/82 (1650 kW, 82 m diameter) (under production)\nWT2000df/80 (2000 kW, 80 m diameter) (under production)\nWT2000fc/80 (2000 kW, 80 m diameter) (under production)\nWT2000dc/86 (2000 kW, 86 m diameter) (under production)\nWT2000fc/86 (2000 kW, 86 m diameter) (under production)\nWT2000fc/93 (2000 kW, 93 m diameter) (under production)\nWT2000dc/93 (2000 kW, 93 m diameter) (under production)\nWT3000df/91 (3000 kW, 91 m diameter) (under production)\nWT3000fc/91 (3000 kW, 91 m diameter) (under production)\nWT3000fc/113 (3000 kW, 113 m diameter) (under production)\nWT3000fc/116 (3000 kW, 116 m diameter) (under production)\nWT3000df/120 (3000 kW, 120 m diameter) (under production)\nWT3000dd/120 (3000 kW, 120 m diameter) (under production)\nWT3000fc/120 (3000 kW, 120 m diameter) (under production)\nWT3000dd/125 (3000 kW, 125 m diameter) (under production)\nWT5500df/140 (5500 kW, 140 m diameter) (under production)\nWT5500fc/140 (5500 kW, 140 m diameter) (under production)\nWT10000dd/190 SeaTitan (10000 kW, 190 m diameter) (under development)"]
[154,"Winwind","Finland","No longer exists (2014)","WWD-1-56 (1000 kW, 56 m diameter) (old model)\nWWD-1-60 (1000 kW, 60 m diameter) (old model)\nWWD-1-64 (1000 kW, 64 m diameter) (old model)\nWWD-3-90 (3000 kW, 90 m diameter) (old model)\nWWD-3-100 (3000 kW, 100 m diameter) (old model)\nWWD-3-103 (3000 kW, 103 m diameter) (old model)\nWWD-3-109 (3000 kW, 109 m diameter) (old model)\nWinWinD 3 120 (3000 kW, 120 m diameter) (old model)"]
[155,"WKA","Germany","No longer exists","60/1 (1200 kW, 60 m diameter) (old model)\n60/2 (1310 kW, 60 m diameter) (old model)"]
[156,"Wobben","Brazil",null,"E40/500 (500 kW, 40 m diameter) (old model)\nE40/600 (600 kW, 40 m diameter) (old model)\nE48/800 (800 kW, 48 m diameter) (under production)\nE44/900 (900 kW, 44 m diameter) (old model)\nE70/2000 (2000 kW, 70 m diameter) (old model)\nE82/2000 (2000 kW, 82 m diameter) (under production)\nE70/2300 (2300 kW, 71 m diameter) (under production)\nE82/2300 (2300 kW, 82 m diameter) (under production)\nE92/2350 (2350 kW, 92 m diameter) (under production)\nE82/3000 (3000 kW, 82 m diameter) (under production)"]
[157,"Xant","Belgium",null,"XANT-21 (100 kW, 21 m diameter) (under production)"]
[158,"XEMC-Darwind","Netherlands",null,"XE72-2000 (2000 kW, 70.65 m diameter) (old model)\nXE93-2000 (2000 kW, 70.65 m diameter) (under production)\nXE82-2000 (2000 kW, 82.74 m diameter) (old model)\nXE87-2000 (2000 kW, 87.74 m diameter) (old model)\nXE105-2000 (2000 kW, 105 m diameter) (old model)\nXD137-4000 (4000 kW, 137 m diameter) (under production)\nXD115-4500 (4500 kW, 115 m diameter) (under production)\nXE/DD115 (5000 kW, 115 m diameter) (under production)\nXE/DD126 (5000 kW, 126 m diameter) (old model)"]
[159,"Zond","USA","Acquired (1997)","Z-40 (500 kW, 40 m diameter) (old model)\nZ-46 (750 kW, 46 m diameter) (old model)\nZ-48 (750 kW, 48 m diameter) (old model)\nZ-50 (750 kW, 50 m diameter) (old model)"]