{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["расход профиля"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"расход профиля","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6]]}
["Расход профиля по КМД"]
[]
[]
[]
["N п/п","Артикул","Наименование","Цвет RAL","Длина","Кол-во","Ед. изм."]
[null,"Профили"]
[1,"P400/153 ","Стойка 130мм","5 300","RAL 9016",null,"хл"]
[2,"P400/152","Стойка 115мм","5 300","RAL 9016",null,"хл"]
[3,"P400/151","Стойка 100мм","5 300","RAL 9016",null,"хл"]
[4,"P400/153","Стойка 130мм","6 000","RAL 9016",null,"хл"]
[5,"P400/152","Стойка 115мм","6 000","RAL 9016",null,"хл"]
[6,"P400/151","Стойка 100мм","5 800","RAL 9016",null,"хл"]
[7,"P400/27X","Стойка 40 безусая","6 000","RAL 9016",null,"хл"]
[8,"P400/181","Стойка  угловая ","6 000","RAL 9016",null,"хл"]
[9,"P400/181","Стойка  угловая ","5 300","RAL 9016",null,"хл"]
[10,"P400/17X","Ригель (T широкий 70.8х40.2)","6 000","RAL 9016",null,"хл"]
[11,"P400/01X","Стойка/ригель L узкий 39 х 40 мм ","6 000","RAL 9016",null,"хл"]
[12,"P400/07X","Ригель/импост (Т узкий 53.1х40.2)","6 000","RAL 9016",null,"хл"]
[13,"P400/02X","створка","6 000","RAL 9016",null,"хл"]
[14,"P400/102","закладная ригеля","6 000","н/о",null,"хл"]
[15,"P400/104","Закладная стойки","6 000","н/о",null,"хл"]
[16,"P400/176","Адаптер (образователь уса)","6 000","RAL 9016",null,"хл"]
[17,"ЭК-64064","Стойка с замком (одиночная раздвижка)","6 000","RAL 9016",null,"хл"]
[18,"P400/178","Адаптер боковой (притвор)","6 000","RAL 9016",null,"хл"]
[19,"C640/51X","Труба Ф50 мм","6 000","RAL 9016",null,"хл"]
[20,"ЭК-64083","Ригель с полозьями","6 000","RAL 9016",null,"хл"]
[21,"Труба 40х40х2","Труба 40х40х2","6 000","RAL 9016",null,"хл"]
[22,"спейсер","спейсер 20х24",null,"н/о",null,"м.п"]
[23,"ЭК-64031","Штапик (под стекло 10 мм) ","6 000","RAL 9016",null,"хл"]
[24,"P400/31X","Штапик (под стекло 5 мм) ","6 000","RAL 9016",null,"хл"]
[25,"ЭК-64062","Штапик для 1х раздвижки","6 000","RAL 9016",null,"хл"]
[26,"ЭЗУ-215 (ALT0014)","Уплотнитель наружный",null,null,null,"пог.м"]
[27,"ЭЗУ-212 (ALT0015)","Уплотнитель внутренний (штапик)",null,null,null,"пог.м"]
[28,"ТПУ-0064","Уплотнитель раздвижки",null,null,null,"пог.м"]
[29,"PB 69 1000-3P (900-3P) ","фетр раздвижки",null,null,null,"пог.м"]
[30,"9ES/08 ","Закладная  створок Р400/02х",null,null,null,"шт."]
[31,"ТПУ-014 ","Пластина 0.5х16х100мм",null,null,null,"шт."]
[32,"ТПУ-014-01","Пластина  1х16х100мм",null,null,null,"шт."]
[33,"ТПУ-014-04 ","Пластина  3х16х100мм",null,null,null,"шт."]
[34,"ТПУ-026-04 ","Пластина  3х10х100мм",null,null,null,"шт."]
[35,"ТПУ-016 ","Крышка дренажного отв.",null,null,null,"шт."]
[36,"DC791","атмосферостойкий силикон",null,"бел",null,"туб. 310мл"]
[37,"паронит 1мм","в пятку",null,null,null,"рулон 1,5м"]
[38,"C640/10L","Профиль створки боковой ","6 000","RAL 9016",null,"хл"]
[39,"C640/11L","Профиль створки центральный","6 000","RAL 9016",null,"хл"]
[40,"C640/12L","Профиль створки низ-верх","6 000","RAL 9016",null,"хл"]
[41,"ролик","ролик",null,null,null,"шт"]
[42,"Замок-защёлка","Замок-защёлка",null,null,null,"шт"]
[43,"КТ30","Комплект накладок",null,null,null,"шт"]
[44,"DIN 7504P 4,2x32","винт самонарезающий для крепления спейсера к ригелю","А2",null,null,"шт"]
[45,"DIN 7981  5,5x13","саморез для крепления ригельного сухаря ","А2",null,null,"шт"]
[46,"DIN 7504Р  5,5x13","саморез для крепления ригеля к сухарю","А2",null,null,"шт"]
[47,"DIN 7982  4,8х32","саморез для крепления стоичных сухарей к пластине монтажной ","А2",null,null,"шт"]
[48,"DIN 7981 4,8х22 (9VA/33)","шуруп-саморез для крепления КТ/30","А2",null,null,"шт"]
[49,"DIN7504N  3,5x16","саморез для крепления усов и пр.","А2",null,null,"шт"]
[50,"DIN 7504N  4,2x25","винт самонарезающий для угловых соединений и поворотов","А2",null,null,"шт"]
[51,"P400/179","Адаптер боковой (притвор под ус)","6 000","RAL 9016",null,"хл"]