{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["KKS","Хранение"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"KKS","index":0,"n_rows":58,"n_cols":5,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
["KKS","ЦЕХ","вид оборудования","напоминалка","куратор"]
["1NJ10D001","ЦОС","ЭД 0,4 кВ","Вентилятор котла №1","МГО"]
["1NJ30D001","ЦОС","ЭД 0,4 кВ","Дымосос котла №1","МГО"]
["27GHE02AP001","ГОиЧС","ЭД 0,4 кВ","Электродвигатель циркуляционного насоса","МГО"]
["27GHE02AP002","ГОиЧС","ЭД 0,4 кВ","Электродвигатель циркуляционного насоса","МГО"]
["27SAC03AN001","ЦВ","ЭД 0,4 кВ","Электродвигатель","МГО"]
["27SAC05AH001GH01","ЦВ","шкаф САУ","Шкаф САУ","МГО"]
["41BBS10","ЭЦ","токопровод 6кВ",null,"РУ"]
["41BBS30","ЭЦ","токопровод 6кВ",null,"РУ"]
["4BBC","ЭЦ","Секция 6кВ",null,"РУ"]
["4BBD03","ЭЦ","Ячейка 6кВ",null,"РУ"]
["4BBT01","ЭЦ","ТСН",null,"РУ"]
["4BBT02","ЭЦ","ТСН",null,"РУ"]
["4BCT01","ЭЦ","РТСН",null,"РУ"]
["4BCT02","ЭЦ","РТСН",null,"РУ"]
["4BDA","ЭЦ","Секция 6кВ",null,"РУ"]
["4BDG60","ЭЦ","Секция 6кВ",null,"РУ"]
["4BEC","ЭЦ","Секция 6кВ",null,"РУ"]
["4BFA","ЭЦ","НКУ-РУ 0,4кВ",null,"РУ"]
["4BFG","ЭЦ","НКУ-РУ 0,4кВ",null,"РУ"]
["4BFN","ЭЦ","НКУ-РУ 0,4кВ",null,"РУ"]
["4BPE10GU001M02","ЭЦ","ЭД 0,4 кВ","Электродвигатель насоса охлаждения КРЭП 1ГЦН-1","МГО"]
["4BPE10GU001P02","ЭЦ","насос","Насос охлаждения КРЭП 1ГЦН-1","МГО"]
["4FCD04AB001D001","ОЯБиН","ЭД 0,4 кВ","Электродвигатель 4FCD04AB001","МГО"]
["4GCB06","ХЦ","ЭД 0,4 кВ","электродвигатель компрессорной станции","МГО"]
["4GCB20AP002","ХЦ","ЭД 0,4 кВ",null,"МГО"]
["4GMC65AP001","ЦОРО","ЭД 0,4 кВ","Насос откачки трапных вод из приямка","МГО"]
["4JEB10AP001","РЦ-3","ЭД 6 кВ","Электродвигатель 1ГЦН-1","МГО"]
["4JEB10AP003","РЦ-3","ЭД 0,4 кВ","Электродвигатель гидроагрегата обратного клапана 1ГЦН-1","МГО"]
["4KPA1003M02D002","ЦОРО","ЭД 0,4 кВ","Агрегат электронасосный","МГО"]
["4KUK50AN001","ОРБ","ЭД 0,4 кВ","Газодувка","МГО"]
["4KUK60AN001","ОРБ","ЭД 0,4 кВ","Газодувка","МГО"]
["4LAC02AP001","ТЦ-3","ЭД 6 кВ","Предвключенный питательный насос","МГО"]
["4LAC14AP001","ТЦ-3","ЭД 6 кВ","Главный питательный насос","МГО"]
["4LAV11AP001","ТЦ-3","ЭД 0,4 кВ","Маслостанция главного питательного насоса","МГО"]
["4UKS01AB303D001","ОЯБиН","ЭД 0,4 кВ","Электродвигатель 4UKS01AB303D001","МГО"]
["4XJA11HA001","ЭЦ","дизель","Дизель","ДГУ"]
["4XJG11AN004","ЭЦ","вентилятор","Вентилятор охлаждения тосола ДГУ","ДГУ"]
["4XJG11AN004","ЭЦ","автоматика","Вентилятор охлаждения тосола ДГУ","КИП"]
["4XJG11AN004","ЭЦ","кабель","Вентилятор охлаждения тосола ДГУ","КХиО"]
["4XJG11AN004","ЭЦ","ЭД 0,4 кВ","Вентилятор охлаждения тосола ДГУ","МГО"]
["4XJG11AN005","ЭЦ","вентилятор","Вентилятор охлаждения тосола ДГУ","ДГУ"]
["4XJG11AN005","ЭЦ","ЭД 0,4 кВ","Вентилятор охлаждения тосола ДГУ","МГО"]
["4XJG11AN006","ЭЦ","вентилятор","Вентилятор охлаждения тосола ДГУ","ДГУ"]
["4XJG11AN006","ЭЦ","ЭД 0,4 кВ","Вентилятор охлаждения тосола ДГУ","МГО"]
["4XJG11AP007","ЭЦ","насос","Насос горячего резерва","ДГУ"]
["4XJG11AP007","ЭЦ","ЭД 0,4 кВ","Насос горячего резерва","МГО"]
["4XJG11AP008","ЭЦ","насос","Насос горячего резерва","ДГУ"]
["4XJG11AP008","ЭЦ","ЭД 0,4 кВ","Насос горячего резерва","МГО"]
["4XJG11AP009","ЭЦ","насос","Насос заполнения расширительного бака и откачки воды из бака водоподготовки","ДГУ"]
["4XJG11AP009","ЭЦ","ЭД 0,4 кВ","Насос заполнения расширительного бака и откачки воды из бака водоподготовки","МГО"]
["4XJG12AC002","ЭЦ","ЭД 0,4 кВ","Блок охлаждения ДГУ-500","МГО"]
["4XJG12AP005","ЭЦ","насос","Электронасос заполнения и откачки резезвуара воды","ДГУ"]
["4XJG12AP005","ЭЦ","ЭД 0,4 кВ","Электронасос заполнения и откачки резезвуара воды","МГО"]
["BML10/10B","ЭЦ","блок НКУ-РУ 0,4",null,"РУ"]
["BML5/8","ЭЦ","блок НКУ-РУ 0,4",null,"РУ"]
["BML8/4A","ЭЦ","блок НКУ-РУ 0,4",null,"РУ"]
["BML9/3A","ЭЦ","блок НКУ-РУ 0,4",null,"РУ"]

{"sheet":"Хранение","index":1,"n_rows":1,"n_cols":5,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["KKS оборудования","Цех","вид оборудования","Участок (куратор)","исполнитель"]