{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Лист1","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":22,"n_cols":1,"rows_kept":22,"cut":false,"hidden":false,"merged":[[20,0,20,1],[21,0,21,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[0,0,0,1],[1,0,1,1],[2,0,2,1],[3,0,3,1],[4,0,4,1]]}
["1. Вода питьевая"]
["2. Компонент №128"]
["3. Компонент №96"]
[" Раздел 4. Полы Примыкания через демпферную ленту и герметик. Керамическая плитка 1 сорт. Отклонения среднего значения по каждой плитке от рабочего размера 300*300*8 +-0,6%."]
["5. Компонент №181"]
["6. Компонент №5*"]
["7. Компонент №51"]
["8. Компонент №44"]
["9. Компонент №69"]
["10. Компонент №182"]
["Раздел 4.  Полы Примыкания через демпферную ленту и герметик. Керамическая плитка 1 сорт. Отклонения среднего значения по каждой плитке от рабочего размера 300*300*8 +-0,6%."]
["12. Пигмент желтый Bayferrox 920"]
["13. Пигмент красный Bayferrox 130 М, страна происхождения - Германия"]
["14. Пигмент черный Bayferrox 318M, Германия"]
["15. Компонент №237"]
["16. Вода питьевая"]
["17. Компонент №98"]
["18. Компонент №10"]
["19. Компонент №111"]
["20. Компонент №139"]
["Всего загружено"]
["Итого"]

{"sheet":"Лист3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}