{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист3","index":0,"n_rows":637,"n_cols":4,"rows_kept":637,"cut":false,"hidden":false,"merged":[]}
["part","descript"]
["xxxxxx","Description:IBM xxxGB 7.2K 6Gb/s 2.5 HS SAS Hot-Swap Drive with Tray includedFor Storewize V3500 V3700\nPart Number(s)\nIBM Option: ######\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThis 7.2K RPM 6Gb/s 2.5-inch Hot-Swap SAS drive offers the highest performance. It has outstanding reliability that enables operation in RAID environments without compromising application performance or availability.\n\nSpecifications:\nCategoryIBM HardDrive\nSub-Category2.5 SFF\nGenerationHS SAS\nPart Number######\n\n\n\nProducts ID361\nCapacityxxxGB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nHDD Form Factor2.5 inches\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nHot SwapYes",{"$f":"ExtractValues(B2)","v":"\nIBM Option: ######\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThis 7.2K RPM 6Gb/s 2.5-inch Hot-Swap SAS drive offers the highest performance. It has outstanding reliabil"}]
["XS960SE70004","Description:HP 960GB MSA SFF 2.5-inch Serial Attached SCSI(SAS) Read-Intensive (RI) 12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R0Q46A\nSpare Part# P13236-001\nModel# XS960SE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberXS960SE70004\n\n\n\nProducts ID1737648\nTypeSolid State Drive\nStorage Capacity960GB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm FactorInternal\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XS960SE70004 SAS MSA Solid State Drive",{"$f":"ExtractValues(B3)","v":"\nOption Part# R0Q46A\nSpare Part# P13236-001\nModel# XS960SE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all a"},"g"]
["XS800LE70004","Description:HP MSA 800GB 3.5in SAS 12G Mixed Use (MU) SSD\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# P9M80A\nSpare Part# 868232-001\nModel# XS800LE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\n\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberXS800LE70004\n\n\n\nProducts ID737680\nTypeHard Drive - Hot-Plug\nCapacity800GB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XS800LE70004 SAS MSA StorageWorks HardDrive",{"$f":"GetValues(B4)","v":"P9M80A\nSpare Part# 868232-001\nModel# XS800LE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\n\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberXS800LE70004\n\n\n\nProducts ID737680\nTypeHard Drive - Hot-Plug\nCapacity800GB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XS800LE70004 SAS MSA StorageWorks HardDrive"},"g"]
["XS1920SE70004","Description:HP MSA 1.92TB 2.5inch SFF SAS 12Gb/sRead Intensive (RI) Solid State Drive (SSD)Part Number(s)\nOption Part# R0Q37A\nSpare Part# P13012-001\nModel# XS1920SE70004\nModel# VO001920JWTBL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Server Read Intensive (RI) Solid State Drives (SSDs) deliver high performance and endurance for applications requiring high random read IOPs performance. HPE (RI) SSDs typically have an endurance of <1 drive writes per day. All HPE SSDs are backed by over 3.35 million hours of testing and qualification ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to your data by providing the assurance that drive firmware comes from a trusted source. The self-describing icons on the HPE Smart Carrier take the guesswork out of a drive’s status and a \"do not remove\" button prevents data loss from human error. You can also monitor the lifespan of your SSD with HPE SmartSSD Wear Gauge compatibility in management tools allowing you to determine if any drives are at risk of failure.\n\nSpecifications:\nCategoryHP\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberXS1920SE70004\n\n\n\nProducts ID1737592\nCapacity1.92TB\nInterfaceSAS\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeRead Intensive\nData Transfer Rate12 Gb/sec (external)\nInterfaces1 x SAS 12 Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XS1920SE70004 SAS MSA Solid State Drive",{"$f":"GetValues(B5)","v":"R0Q37A\nSpare Part# P13012-001\nModel# XS1920SE70004\nModel# VO001920JWTBL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Server Read Intensive (RI) Solid State Drives (SSDs) deliver high performance and endurance for applications requiring high random read IOPs performance. HPE (RI) SSDs typically have an endurance of <1 drive writes per day. All HPE SSDs are backed by over 3.35 million hours of testing and qualification ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to your data by providing the assurance that drive firmware comes from a trusted source. The self-describing icons on the HPE Smart Carrier take the guesswork out of a drive’s status and a \"do not remove\" button prevents data loss from human error. You can also monitor the lifespan of your SSD with HPE SmartSSD Wear Gauge compatibility in management tools allowing you to determine if any drives are at risk of failure.\n\nSpecifications:\nCategoryHP\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberXS1920SE70004\n\n\n\nProducts ID1737592\nCapacity1.92TB\nInterfaceSAS\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeRead Intensive\nData Transfer Rate12 Gb/sec (external)\nInterfaces1 x SAS 12 Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XS1920SE70004 SAS MSA Solid State Drive"},"g"]
["XK0960GDQPK","Description:HP 960GB 2.5-inch SFF Serial ATA (SATA)\nValue Endurance (VE)   6Gb/s  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 734526-B21\nSmartBuy Part# 734526-S21\nSpare Part# 734567-001\nAssembly Part# 731041-002\nModel# XK0960GDQPK\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberXK0960GDQPK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID507560\nTypeSolid State Drive (SSD)\nCapacity960GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationValue Endurance (VE)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XK0960GDQPK SATA SC SSD Solid State Drive",{"$f":"GetValues(B6)","v":"734526-B21\nSmartBuy Part# 734526-S21\nSpare Part# 734567-001\nAssembly Part# 731041-002\nModel# XK0960GDQPK\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberXK0960GDQPK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID507560\nTypeSolid State Drive (SSD)\nCapacity960GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationValue Endurance (VE)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XK0960GDQPK SATA SC SSD Solid State Drive"},"g"]
["XK0480GDUWE","Description:HP 480GB 3.5-inch LFF SATA Hot-PlugValue Endurance (VE)   6Gb/s  Solid State Drive (SSD)Enterprise Value (EV) Solid State Drive (SSD)2 ½ inch - 3 ½ inch LFF Hybrid Adapter Module\nIn HP 3.5-inch LFF SATA Hot-Plug Solid State Drive tray (as pictured)\nFor HP G1-G7 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Solid State DrivePart Number(s)\nOption Part# 756121-B21\nSmartBuy Part# 756121-S21\nSpare Part# 757229-001\nAssembly Part# 731041-005\nModel# XK0480GDUWE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SSD\nPart NumberXK0480GDUWE\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID504412\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["XK0480GDQPH","Description:HP 480GB 2.5-inch SFF Serial ATA (SATA)\nValue Endurance (VE)   6Gb/s  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 740132-B21\nSmartBuy Part# 740132-S21\nSpare Part# 735501-001\nAssembly Part# 731041-001\nModel# XK0480GDQPH\n\t\t\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberXK0480GDQPH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504380\nTypeSolid State Drive (SSD)\nCapacity480GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationValue Endurance (VE)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XK0480GDQPH SATA SC SSD Solid State Drive",null,"g"]
["XK0480GDPVH","Description:HP G8 G9 480GB 2.5-inch Small Form Factor SFF MLC\nPluggable SATA 3G Solid State Drive (SSD)\nIn 2.5-inch G8 G9 (Gen8 Gen9) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 698297-B21\nSmartBuy Part# 698297-S21\nSpare Part# 698472-001\nAssembly Part# 729847-001\nModel# XK0480GDPVH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberXK0480GDPVH\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID507544\nTypeSolid State Drive\nSmall Form Factor2.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate3G = 3Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XK0480GDPVH SATA SC SSD Solid State Drive",null,"g"]
["XK0240GDSDQ","Description:HP 240GB 2.5-inch SFF Serial ATA (SATA)\nValue Endurance (VE)   6Gb/s  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 734878-B21\nSmartBuy Part# 734878-S21\nSpare Part# 735500-001\nAssembly Part# 731041-003\nModel# XK0240GDSDQ\n\t\t\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberXK0240GDSDQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504396\nTypeSolid State Drive (SSD)\nCapacity240GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationValue Endurance (VE)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# XK0240GDSDQ SATA SC SSD Solid State Drive",null,"g"]
["WD800AAJS-70TDA1","Description:80GB 3.5-inch LFF SATA 1.5G 7.2K\nMidline (MDL) Hard Drive\nIn HP G1-G7 Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349237-B21\nSmartBuy Part#349237-S21\nSpare Part#397551-001\nAssembly Part# 431688-001\nModel# WD800AAJS-70TDA1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. HP SATA 7200 rpm Hard Drives provide entry-level performance and high capacity for select Proliant servers. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD800AAJS-70TDA1\n\n\n\nProducts ID1506188\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity80GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (ATA) plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD800AAJS-70TDA1 SATA 7.2K",null,"g"]
["WD800AAJS-70TDA0","Description:80GB 3.5-inch LFF SATA 1.5G 7.2K\nMidline (MDL) Hard Drive\nIn HP G1-G7 Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349237-B21\nSpare Part# 397551-001\nAssembly Part# 431688-001\nModel# WD800AAJS-70TDA0\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. HP SATA 7200 rpm Hard Drives provide entry-level performance and high capacity for select Proliant servers. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD800AAJS-70TDA0\n\n\n\nProducts ID461869\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity80GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (ATA) plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD800AAJS-70TDA0 SATA 7.2K",null,"g"]
["WD5000YS-70VJB1","Description:500GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch high NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 395473-B21\nSmartBuy Part# 395473-S21\nSpare Part# 395501-002\nAssembly Part# 431689-003\nModel# WD5000YS-70VJB1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD5000YS-70VJB1\n\n\n\nProducts ID461866\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity500GB\nInterface TypeSerial ATA-150\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD5000YS-70VJB1 SATA 7.2K",null,"g"]
["WD5000YS-70MPB1","Description:500GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch high NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 395473-B21\nSmartBuy Part# 395473-S21\nSpare Part# 395501-001\nAssembly Part# 431689-002\nModel# WD5000YS-70MPB1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD5000YS-70MPB1\n\n\n\nProducts ID1506200\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity500GB\nInterface TypeSerial ATA-150\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate1.5G = 1.5Gb/sec (187.5MB/s)\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD5000YS-70MPB1 SATA 7.2K",null,"g"]
["WD5000YS-70MPB0","Description:500GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch high NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 395473-B21\nSpare Part# 395501-001\nAssembly Part# 431689-002\nModel# WD5000YS-70MPB0\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD5000YS-70MPB0\n\n\n\nProducts ID461867\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity500GB\nInterface TypeSerial ATA-150\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD5000YS-70MPB0 SATA 7.2K",null,"g"]
["WD5000AAKX","Description:Western Digital 500GB Hot-Plug SATA LFF Hard Drive 7.2K 3.5-inch form factorPart Number(s)\nModel# WD5000AAKX\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\n\n\nSpecifications:\nCategoryWestern Digital HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD5000AAKX\n\n\n\nProducts ID480115\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity500GB\nSpindle Speed7200RPM",null,"g"]
["WD2500YS-70SHB1","Description:HP 250GB 1.5G 7.2K RPM \n3.5-inch HotPlug SATA DriveFor HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349239-B21\nSmartBuy Part# 349239-S21\nSpare Part# 397553-001\nAssembly Part# 431689-001\nModel# WD2500YS-70SHB1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD2500YS-70SHB1\n\n\n\nProducts ID1506196\nTypeHardDrive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity250GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time10ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD2500YS-70SHB1 SATA 7.2K",null,"g"]
["WD2500YS-70SHB0","Description:HP 250GB 1.5G 7.2K 3.5-inch HotPlug SATA DriveFor HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)Option Part# 349239-B21Spare Part# 397553-001Assembly Part# 352561-001Assembly Part# 353044-001Assembly Part# 391335-002Assembly Part# 391335-004Assembly Part# 397377-004Assembly Part# 407525-003Assembly Part# 431689-001Assembly Part# 432337-001Assembly Part# 454141-001Model# GB0250C8045Model# 6L250S0Model# 7L250S0Model# ST3250624ASModel# ST3250620NSModel# WD2500YS-70SHB0\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD2500YS-70SHB0\n\n\n\nProducts ID1461865\nTypeHardDrive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity250GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time10ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD2500YS-70SHB0 SATA 7.2K",null,"g"]
["WD1600JS-70SGB1","Description:160GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch highIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349238-B21\nSmartBuy Part# 349238-S21\nSpare Part# 397552-001\nAssembly Part# 431688-002\nModel# WD1600JS-70SGB1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD1600JS-70SGB1\n\n\n\nProducts ID506192\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD1600JS-70SGB1 SATA 7.2K",null,"g"]
["WD1600JS-70SGB0","Description:160GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch highIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349238-B21\nSpare Part# 397552-001\nAssembly Part#391334-002\nAssembly Part# 391334-004\nAssembly Part# 440300-002\nAssembly Part# 431688-002\nModel# 6L160M0\nModel# FB160C4081\nModel# ST3160812AS\nModel# WD1600JS-70SGB0\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD1600JS-70SGB0\n\n\n\nProducts ID1461863\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# WD1600JS-70SGB0 SATA 7.2K",null,"g"]
["WD10EZEX","Description:Western Digital 1TB Hot-Plug SATA LFF Hard Drive 7.2K 3.5-inch form factorPart Number(s)\nModel# WD10EZEX\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\n\n\nSpecifications:\nCategoryWestern Digital HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberWD10EZEX\n\n\n\nProducts ID494301\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity1TB\nSpindle Speed7200RPM",null,"g"]
["VT510C2","Description:DEC 15 inch Amber Monitor\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberVT510C2\nProducts ID141456",null,"g"]
["VR000480GWFMD","Description:HP 480GB SATA 6G M.2 Read-Intensive (RI)\nSolid State Drive (SSD) Genuine HPSerial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 875498-B21\nSpare Part# 875855-001\nAssembly Part# 871628-002\nModel# VR000480GWFMD\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.\n\nThese drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA M.2 SSD\nPart NumberVR000480GWFMD\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736426\nCapacity480GB\nInterfaceSATA 6Gbp/s\n\n\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["VO1920JFDGV","Description:HP 1.92TB 2.5-inch SFF Serial Attached SCSI (SAS)\nRead-Intensive (RI) 12Gb/s Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816572-B21\nSmartBuy Part# 816572-S21\nSpare Part# 817051-001\nAssembly Part# 816559-003\nModel# VO1920JFDGV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO1920JFDGV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID499092\nTypeSolid State Drive (SSD)\nCapacity1.92TB\nInterface TypeSerial Attached SCSI (SAS)\nDrive Interface Standard12Gb/s SAS\nBest applicationRead Intensive (RI)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO1920JFDGV SAS SC SSD Solid State Drive",null,"g"]
["VO1920JEUQQ","Description:HP 1.92TB 2.5-inch SFF SAS Read-Intensive (RI)\n12Gb/s Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 802891-B21\nSmartBuy Part# 802891-S21\nSpare Part# 802911-001\nAssembly Part# 799839-001\nModel# VO1920JEUQQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO1920JEUQQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID497420\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO1920JEUQQ SAS SC SSD Solid State Drive",null,"g"]
["VO1600JEABF","Description:HP 1.6TB 3.5-inch LFF SAS 12Gb/s\nValue Endurance (VE) Solid State Drive\nEnterprise Value (EV) Solid State Drive (SSD)\nIn HP G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmware\nPart Number(s)\nOption Part# 762272-B21\nSmartBuy Part# 762272-S21\nSpare Part# 762752-001\nAssembly Part# 750222-003\nModel# VO1600JEABF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO1600JEABF\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID498724\nTypeSolid State Drive\nCapacity1.6TB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nData Transfer Rate1.2GB/s\nInterfaceSerial Attached SCSI 3\nBytes/Sector512\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO1600JEABF SAS SC SSD Solid State Drive",null,"g"]
["VO1200KEFJC","Description:HP 1.2 TB NVMe x4 Lanes PCIe 2.5-inch SFFRead-Intensive (RI) HP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified NVMe SCN SSD (Solid State Drive)Part Number(s)\nOption Part# 764906-B21\nSmartBuy Part# 764906-S21\nSpare Part# 765068-001\nAssembly Part# 764903-002\nModel# VO1200KEFJC\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO1200KEFJC\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID721072\nTypeSolid State Drive\nCapacity1.2TB\nInterface TypeNVMe\n\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO1200KEFJC NVMe SCN SSD Solid State Drive",null,"g"]
["VO0960JFDGU","Description:HP 960GB 2.5-inch SFF Serial Attached SCSI (SAS)\nRead-Intensive (RI) 12Gb/s Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816568-B21\nSmartBuy Part# 816568-S21\nSpare Part# 817049-001\nAssembly Part# 816559-002\nModel# VO0960JFDGU\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO0960JFDGU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1499084\nTypeSolid State Drive (SSD)\nCapacity960GB\nInterface TypeSerial Attached SCSI (SAS)\nDrive Interface Standard12Gb/s SAS\nBest applicationRead Intensive (RI)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0960JFDGU SAS SC SSD Solid State Drive",null,"g"]
["VO0600ECHPP","Description:HP G8 G9 600GB 2.5-inch Small Form Factor SFF MLC\nPluggable SATA 3G Solid State Drive (SSD)\nIn 2.5-inch G8 G9 (Gen8 Gen9) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 692174-B21\nSmartBuy Part# 692174-S21\nSpare Part# 692319-001\nAssembly Part# 667602-005\nModel# VO0600ECHPP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVO0600ECHPP\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID507512\nTypeSolid State Drive\nSmall Form Factor2.5 inches\nCapacity600GB\nInterface TypeSerial ATA\nData Transfer Rate3G = 3Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0600ECHPP SATA SC SSD Solid State Drive",null,"g"]
["VO0480JFDGT","Description:HP 480GB 2.5-inch SFF Serial Attached SCSI (SAS)\nRead-Intensive (RI) 12Gb/s Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816562-B21\nSmartBuy Part# 816562-S21\nSpare Part# 817047-001\nAssembly Part# 816559-001\nModel# VO0480JFDGT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO0480JFDGT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID499076\nTypeSolid State Drive (SSD)\nCapacity480GB\nInterface TypeSerial Attached SCSI (SAS)\nDrive Interface Standard12Gb/s SAS\nBest applicationRead Intensive (RI)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0480JFDGT SAS SC SSD Solid State Drive",null,"g"]
["VO0400KEFJB","Description:HP 400GB NVMe x4 Lanes PCIe 2.5-inch SFFRead-Intensive (RI) HP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 764904-B21\nSmartBuy Part# 764904-S21\nSpare Part# 765067-001\nAssembly Part# 764903-001\nModel# VO0400KEFJB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Read Intensive (RI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance  SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO0400KEFJB\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID721056\nTypeSolid State Drive\nCapacity400GB\nInterface TypeNVMe\n\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0400KEFJB NVMe SCN SSD Solid State Drive",null,"g"]
["VO0300ECHPN","Description:HP G8 G9 300GB 2.5-inch Small Form Factor SFF MLC\nPluggable SATA 3G Solid State Drive (SSD)\nIn 2.5-inch G8 G9 (Gen8 Gen9) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 692171-B21\nSmartBuy Part# 692171-S21\nSpare Part# 692318-001\nAssembly Part# 667602-004\nModel# VO0300ECHPN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVO0300ECHPN\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID503900\nTypeSolid State Drive\nSmall Form Factor2.5 inches\nCapacity300GB\nInterface TypeSerial ATA\nData Transfer Rate3G = 3Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0300ECHPN SATA SC SSD Solid State Drive",null,"g"]
["VO0160ECHPL","Description:HP G8 G9 160GB 2.5-inch Small Form Factor SFF MLC\nPluggable SATA 3G Solid State Drive (SSD)\nIn 2.5-inch G8 G9 (Gen8 Gen9) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 692168-B21\nSmartBuy Part# 692168-S21\nSpare Part# 692317-001\nAssembly Part# 667602-003\nModel# VO0160ECHPL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVO0160ECHPL\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID507496\nTypeSolid State Drive\nSmall Form Factor2.5 inches\nCapacity160GB\nInterface TypeSerial ATA\nData Transfer Rate3G = 3Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0160ECHPL SATA SC SSD Solid State Drive",null,"g"]
["VO015300PXDBV","Description:HP 15.3TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s PM6\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P40474-B21\nSpare Part# P41499-001\nAssembly Part# P41023-001\nModel# VO015300PXDBV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberVO015300PXDBV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726689\nTypeSolid State Drive\nCapacity15.3-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\nProduct FamilyPM6\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO015300PXDBV SAS BC SSD Solid State Drive",null,"g"]
["VO015300JWSSV","Description:HP 15.3TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P06592-B21\nSmartBuy Part# P06592-S21\nSpare Part# P08612-001\nAssembly Part# P02763-005\nModel# VO015300JWSSV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO015300JWSSV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1494664\nTypeSolid State Drive\nCapacity15.3TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO015300JWSSV SAS SC SSD Solid State Drive",null,"g"]
["VO015300JWCNL","Description:HP 15.3TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 870148-B21\nSmartBuy Part# 870148-S21\nSpare Part# 870462-001\nAssembly Part# 867212-002\nModel# VO015300JWCNL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO015300JWCNL\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1499236\nTypeSolid State Drive\nCapacity15.3TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO015300JWCNL SAS SC SSD Solid State Drive",null,"g"]
["VO0080ECHPK","Description:HP 80GB SATA Multi-Level Cell (MLC) 3Gb/s\n2.5-inch Hot-Plug Midline (MDL) Solid State Drive (SSD)\nFor HP G1-G7 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 659529-B21\nSmartBuy Part# 659529-S21\nSpare Part# 659574-001\nAssembly Part# 667602-002\nModel# VO0080ECHPK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant Solid Drive\nSub-CategorySolid State Drive\nGenerationSATA SSD\nPart NumberVO0080ECHPK\n\n\n\nProducts ID503884\nTypeSolid State Drive\nCapacity80GB\nInterface TypeSATA\nForm FactorSmall 2.5 inches (SFF)\nTransfer Rate3GB/s\nLevelMDL\nHot SwapYes\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO0080ECHPK SATA SSD Solid State Drive",null,"g"]
["VO007680PXDBU","Description:HP 7.68TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s PM6\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P40473-B21\nSmartBuy Part# P40473-S21\nSpare Part# P41498-001\nAssembly Part# P41020-001\nModel# VO007680PXDBU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberVO007680PXDBU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1726697\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\nProduct FamilyPM6\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO007680PXDBU SAS BC SSD Solid State Drive",null,"g"]
["VO007680KWVMV","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P10218-B21\nSmartBuy Part# P10218-S21\nSpare Part# P10468-001\nAssembly Part# P09769-003\nModel# VO007680KWVMV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO007680KWVMV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID711084\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO007680KWVMV NVMe SCN SSD Solid State Drive",null,"g"]
["VO007680JWTBP","Description:HP 7.68TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P04523-B21\nSmartBuy Part# P04523-S21\nSpare Part# P06599-001\nAssembly Part# P04172-004\nModel# VO007680JWTBP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO007680JWTBP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID500040\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO007680JWTBP SAS SC SSD Solid State Drive",null,"g"]
["VO007680JWCNK","Description:HP 7.68TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 870144-B21\nSmartBuy Part# 870144-S21\nSpare Part# 870460-001\nAssembly Part# 867212-001\nModel# VO007680JWCNK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO007680JWCNK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1499228\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO007680JWCNK SAS SC SSD Solid State Drive",null,"g"]
["VO004000KWJSH","Description:HP 4TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 877988-B21\nSmartBuy Part# 877988-S21\nSpare Part# 880243-001\nAssembly Part# 877709-003\nModel# VO004000KWJSH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO004000KWJSH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1711204\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity4TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO004000KWJSH NVMe SCN SSD Solid State Drive",null,"g"]
["VO003840RWUFB","Description:HP 3.84TB 2.5-inch SFF Serial Attached SCSI (SAS)\nRead-Intensive (RI) 12Gb/s\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P10444-B21\nSmartBuy Part# P10444-S21\nSpare Part# P10639-001\nAssembly Part# P07305-003\nModel# VO003840RWUFB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO003840RWUFB\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1738316\nTypeSolid State Drive (SSD)\nCapacity3.84TB\nInterface TypeSerial Attached SCSI (SAS)\nDrive Interface Standard12Gb/s SAS\nBest applicationRead Intensive (RI)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO003840RWUFB SAS SC SSD Solid State Drive",null,"g"]
["VO003840PXDBT","Description:HP 3.84TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s PM6\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P40472-B21\nSmartBuy Part# P40472-S21\nSpare Part# P41497-001\nAssembly Part# P41017-001\nModel# VO003840PXDBT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberVO003840PXDBT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726713\nTypeSolid State Drive\nCapacity3.84-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\nProduct FamilyPM6\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO003840PXDBT SAS BC SSD Solid State Drive",null,"g"]
["VO003840KWVMU","Description:HP 3.84 TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P10216-B21\nSmartBuy Part# P10216-S21\nSpare Part# P10467-001\nAssembly Part# P09769-002\nModel# VO003840KWVMU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO003840KWVMU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1711064\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO003840KWVMU NVMe SCN SSD Solid State Drive",null,"g"]
["VO003840JWTBN","Description:HP 3.84TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nPM5 Digitally Signed (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P04521-B21\nSmartBuy Part# P04521-S21\nSpare Part# P06598-001\nAssembly Part# P04172-003\nModel Part# VO003840JWTBN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO003840JWTBN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID494540\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO003840JWTBN SAS SC SSD Solid State Drive",null,"g"]
["VO003840JWDAV","Description:HP 3.84TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 875330-B21\nSmartBuy Part# 875330-S21\nSpare Part# 875686-001\nAssembly Part# 867887-004\nModel#VO003840JWDAV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO003840JWDAV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID499348\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO003840JWDAV SAS SC SSD Solid State Drive",null,"g"]
["VO002000KWJSF","Description:HP 2TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 877986-B21\nSmartBuy Part# 877986-S21\nSpare Part# 880242-001\nAssembly Part# 877709-002\nModel# VO002000KWJSF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO002000KWJSF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1711184\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity2TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO002000KWJSF NVMe SCN SSD Solid State Drive",null,"g"]
["VO001920PXDBR","Description:HP 1.92TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s PM6\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P40471-B21\nSmartBuy Part# P40471-S21\nSpare Part# P41496-001\nAssembly Part# P41014-001\nModel# VO001920PXDBR\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberVO001920PXDBR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726725\nTypeSolid State Drive\nCapacity1.92-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\nProduct FamilyPM6\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO001920PXDBR SAS BC SSD Solid State Drive",null,"g"]
["VO001920KWVMT","Description:HP 1.92 TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P10214-B21\nSmartBuy Part# P10214-S21\nSpare Part# P10466-001\nAssembly Part# P09769-001\nModel# VO001920KWVMT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO001920KWVMT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID711048\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO001920KWVMT NVMe SCN SSD Solid State Drive",null,"g"]
["VO001920JWTBL","Description:HP MSA 1.92TB 2.5inch SFF SAS 12Gb/sRead Intensive (RI) Solid State Drive (SSD)Part Number(s)\nOption Part# R0Q37A\nSpare Part# P13012-001\nModel# XS1920SE70004\nModel# VO001920JWTBL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Server Read Intensive (RI) Solid State Drives (SSDs) deliver high performance and endurance for applications requiring high random read IOPs performance. HPE (RI) SSDs typically have an endurance of <1 drive writes per day. All HPE SSDs are backed by over 3.35 million hours of testing and qualification ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to your data by providing the assurance that drive firmware comes from a trusted source. The self-describing icons on the HPE Smart Carrier take the guesswork out of a drive’s status and a \"do not remove\" button prevents data loss from human error. You can also monitor the lifespan of your SSD with HPE SmartSSD Wear Gauge compatibility in management tools allowing you to determine if any drives are at risk of failure.\n\nSpecifications:\nCategoryHP\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberVO001920JWTBL\n\n\n\nProducts ID737596\nCapacity1.92TB\nInterfaceSAS\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeRead Intensive\nData Transfer Rate12 Gb/sec (external)\nInterfaces1 x SAS 12 Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO001920JWTBL SAS MSA Solid State Drive",null,"g"]
["VO001920JWDAU","Description:HP 1.92TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 875326-B21\nSpare Part# 875684-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO001920JWDAU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID496093\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO001920JWDAU SAS SC SSD Solid State Drive",null,"g"]
["VO001000KWJSE","Description:HP 1TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 877984-B21\nSmartBuy Part# 877984-S21\nSpare Part# 880241-001\nAssembly Part# 877709-001\nModel# VO001000KWJSE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVO001000KWJSE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID711164\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO001000KWJSE NVMe SCN SSD Solid State Drive",null,"g"]
["VO000960PXDBN","Description:HP 960GB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s PM6\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P40470-B21\nSmartBuy Part# P40470-S21\nSpare Part# P41495-001\nAssembly Part# P41011-001\nModel# VO000960PXDBN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberVO000960PXDBN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726745\nTypeSolid State Drive\nCapacity960-GB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\nProduct FamilyPM6\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO000960PXDBN SAS BC SSD Solid State Drive",null,"g"]
["VO000960JWTBK","Description:HP 960GB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nPM5 Digitally Signed (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P04517-B21\nSmartBuy Part# P04517-S21\nSpare Part# P06596-001\nAssembly Part# P04172-001\nModel# VO000960JWTBK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO000960JWTBK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID494564\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO000960JWTBK SAS SC SSD Solid State Drive",null,"g"]
["VO000960JWDAT","Description:HP 960GB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 875313-B21\nSmartBuy Part# 875313-S21\nSpare Part# 875682-001\nAssembly Part# 867887-002\nModel# VO000960JWDAT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO000960JWDAT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1499340\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO000960JWDAT SAS SC SSD Solid State Drive",null,"g"]
["VO000480JWDAR","Description:HP 480GB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 875311-B21\nSmartBuy Part# 875311-S21\nSpare Part# 875681-001\nAssembly Part# 867887-001\nModel# VO000480JWDAR\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVO000480JWDAR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID499332\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VO000480JWDAR SAS SC SSD Solid State Drive",null,"g"]
["VM0500EBQHB","Description:HP 500GB 2.5-inch Serial ATA (SATA) SFF3Gb/s Entry (ETY) 7.2K Non-Hot-Plug (NHP) Hard Drive\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# 628033-B21 \nSmartBuy Part# 628033-S21 \nSpare Part# 628185-001 \nAssembly Part# 628029-002 \nModel# VM0500EBQHB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA drives are designed for the reliability and mass storage demanded by today's entry server and external storage environments. The SATA portfolio is categorized into two categories: Entry (ETY) and Midline (MDL) drives. HP SATA Entry drives are the lowest unit-cost solution for entry-level servers. HP SATA Midline drives are designed with economical reliability and performance for external storage - backups and archival applications.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA NHP HDD\nPart NumberVM0500EBQHB\n\n\n\nProducts ID701820\nConnector TypeSATA 3.0Gbps\nConnectorSerial ATA-300\nTarget UseServer\nForm Factor2.5 inches\nEnclosure TypeInternal\nData Transfer Rate3.0GB/s\nHard Drive Capacity500GB\nSpindle Speed7200RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VM0500EBQHB SATA NHP HDD 7.2K",null,"g"]
["VM0160EASRP","Description:HP 160GB SATA 3Gb/s Midline (MDL) 7200 RPM 2.5-inch SFF Quick Release (QR) Hard Drivein HP Quick Release Hot-Plug drive tray (as pictured)For G1-G7 Proliant QR SATA ServersGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 574893-B21\nSmartBuy Part# 574893-S21\nSpare Part# 575053-001\nAssembly Part# 507749-002\nModel# VM0160EASRP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA QR\nPart NumberVM0160EASRP\n\n\n\nProducts ID700700\nTypeHard Drive - Hot-Swap\nSmall Form Factor2.5 inches\nCapacity160GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate3GB/s\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VM0160EASRP SATA QR 7.2K",null,"g"]
["VK3840GFDKN","Description:HP 3.84TB 3.5-inch 6Gb/s LFF SATA\nRead-Intensive (RI) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816933-B21\nSmart Buy#  816933-S21\nSpare Part# 817092-001\nAssembly Part# 816876-006\nModel# VK3840GFDKN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK3840GFDKN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID704784\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity3.84TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK3840GFDKN SATA SC SSD Solid State Drive",null,"g"]
["VK1920GFLKL","Description:HP 1.92TB 2.5-inch SFF Serial ATA (SATA) Read-Intensive-3 (RI)\nEnterprise   6Gb/s  Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 871770-B21\nSmartBuy Part# 871770-S21\nSpare Part# 872056-001\nAssembly Part# 838403-005\nModel# VK1920GFLKL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK1920GFLKL\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505288\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK1920GFLKL SATA SC SSD Solid State Drive",null,"g"]
["VK1920GFDKL","Description:HP 1.92TB 3.5-inch 6Gb/s LFF SATA\nRead-Intensive (RI) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816923-B21\nSmart Buy#  816923-S21\nSpare Part# 817087-001\nAssembly Part# 816876-005\nModel# VK1920GFDKL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK1920GFDKL\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID704768\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity1.92TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK1920GFDKL SATA SC SSD Solid State Drive",null,"g"]
["VK1600GEYJU","Description:HP 1.6TB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804608-B21\nSmartBuy Part# 804608-S21\nSpare Part# 805376-001\nAssembly Part# 804574-006\nModel# VK1600GEYJU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK1600GEYJU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504852\nTypeHard Drive - Hot Plug - Gen8\nLarge Form Factor3.5 inches\nCapacity1.6TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nConnectivity TechnologySingle-Port\nRead IOPS61500 IOP/s\nWrite IOPS15000 IOP/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK1600GEYJU SATA SC SSD Solid State Drive",null,"g"]
["VK1600GECVP","Description:HP G8 G9 1.6TB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 757342-B21\nSmartBuy Part# 757342-S21\nSpare Part# 757382-001\nAssembly Part# 757338-001\nModel# VK1600GECVP\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK1600GECVP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504544\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity1.6TB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK1600GECVP SATA SC SSD Solid State Drive",null,"g"]
["VK0960GFLKK","Description:HP 960GB 2.5-inch SFF Serial ATA (SATA) Read-Intensive (RI)\nEnterprise   6Gb/s  Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 871768-B21\nSmartBuy Part# 871768-S21\nSpare Part# 872055-001\nAssembly Part# 838403-004\nModel# VK0960GFLKK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0960GFLKK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505280\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS55000\nRandom Write IOPS14000\nAverage Latency155\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0960GFLKK SATA SC SSD Solid State Drive",null,"g"]
["VK0960GFDKK","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 816909-B21\nSmartBuy Part# 816909-S21\nSpare Part# 817080-001\nAssembly# 816876-004\nModel# VK0960GFDKK\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0960GFDKK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID493021\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0960GFDKK SATA SC SSD Solid State Drive",null,"g"]
["VK0960GEPQQ","Description:HP G8 G9 960GB 3.5-inch LFF Hot-Plug SATA Value Endurance (VE)   6Gb/s  Enterprise Boot (EB)Solid State Drive (SSD) in HP G8 G9 Hot-Plug Drive traySmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 789157-B21\nSmartBuy Part# 789157-S21\nSpare Part# 789362-001\nAssembly Part# 789132-003\nModel# VK0960GEPQQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0960GEPQQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1704736\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity960GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0960GEPQQ SATA SC SSD Solid State Drive",null,"g"]
["VK0800JEABE","Description:HP 800GB 3.5-inch LFF SAS 12Gb/s\nValue Endurance (VE) Solid State Drive\nEnterprise Value (EV) Solid State Drive (SSD)\nIn HP G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmware\nPart Number(s)\nOption Part# 762270-B21\nSmartBuy Part# 762270-S21\nSpare Part# 762750-001\nAssembly Part# 750222-002\nModel# VK0800JEABE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK0800JEABE\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID498692\nTypeSolid State Drive\nCapacity800GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nData Transfer Rate1.2GB/s\nInterfaceSerial Attached SCSI\nBytes/Sector512\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0800JEABE SAS SC SSD Solid State Drive",null,"g"]
["VK0800GEYJT","Description:HP 800GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804602-B21\nSmartBuy Part# 804602-S21\nSpare Part# 805375-001\nAssembly Part# 804574-005\nModel# VK0800GEYJT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0800GEYJT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504820\nTypeHard Drive - Hot Plug - Gen8\nLarge Form Factor3.5 inches\nCapacity800GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nConnectivity TechnologySingle-Port\nRead IOPS61500 IOP/s\nWrite IOPS15500 IOP/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0800GEYJT SATA SC SSD Solid State Drive",null,"g"]
["VK0800GEFJK","Description:HP G8 G9 800GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) M1 Solid State Drive (SSD)\nIn HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 764945-B21\nSmartBuy Part# 764945-S21\nSpare Part# 765024-001\nAssembly Part# 764913-004\nModel# VK0800GEFJK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0800GEFJK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504624\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity800GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\nBytes/Sector512\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0800GEFJK SATA SC SSD Solid State Drive",null,"g"]
["VK0800GDJYA","Description:HP G8 G9 800GB 3.5-inch LFF Pluggable SATA  Value Endurance (VE)   6Gb/s  SC Enterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 718189-B21\nSmartBuy Part# 718189-S21\nSpare Part# 718298-001\nAssembly Part# 717968-003\nModel# VK0800GDJYA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0800GDJYA\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504144\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity800GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n4KB Random Read64000IOPS\n4KB Random Write12000IOPS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0800GDJYA SATA SC SSD Solid State Drive",null,"g"]
["VK0600GDUTQ","Description:HP G8 G9 600GB 3.5-inch LFF Pluggable SATA  Value Endurance (VE)   6Gb/s  SC Enterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 739900-B21\nSmartBuy Part# 739900-S21\nSpare Part# 739960-001\nAssembly Part# 717968-005\nModel# VK0600GDUTQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0600GDUTQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504204\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity600GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n4KB Random Read64000IOPS\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0600GDUTQ SATA SC SSD Solid State Drive",null,"g"]
["VK0480GFLKH","Description:HP 480GB 2.5-inch SFF Serial ATA (SATA) Read-Intensive (RI)\nEnterprise   6Gb/s  Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 872855-B21\nSmartBuy Part# 872855-S21\nSpare Part# 872889-001\nAssembly Part# 838403-003\nModel# VK0480GFLKH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GFLKH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505272\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS60000\nRandom Write IOPS15500\nAverage Latency155\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GFLKH SATA SC SSD Solid State Drive",null,"g"]
["VK0480GFDKH","Description:HP 480GB 3.5-inch 6Gb/s LFF SATA\nRead-Intensive (RI) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816903-B21\nSmart Buy# 816903-S21\nSpare Part# 817077-001\nAssembly Part# 816876-003\nModel# VK0480GFDKH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GFDKH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505100\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GFDKH SATA SC SSD Solid State Drive",null,"g"]
["VK0480GEYJR","Description:HP 480GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804596-B21\nSmartBuy Part# 804596-S21\nSpare Part# 805374-001\nAssembly Part# 804574-004\nModel# VK0480GEYJR\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GEYJR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504788\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nData Transfer Rate600 MB/s\nInterfaceSerial ATA\n4KB Random Read75000 IOPS\n4KB Random Write11000 IOPS\n \nFlash TypeMLC\nBest ApplicationRead-Intensive (RI)\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GEYJR SATA SC SSD Solid State Drive",null,"g"]
["VK0480GEQNB","Description:HP 480GB 2.5-inch Serial ATA (SATA) SFF6Gb/s Value Endurance (VE) Non-Hot-Plug (NHP) Solid State Drive\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# 792241-B21 \nSmartBuy Part# 792241-S21 \nSpare Part# 792368-001 \nAssembly Part# 791146-001 \nModel# VK0480GEQNB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySATA\nGenerationSATA NHP SSD\nPart NumberVK0480GEQNB\n\n\n\nProducts ID1700220\nConnector TypeSATA 6GB/s\nHost InterfaceSerial ATA\nTarget UseServer\nForm Factor2.5 inches\nEnclosure TypeInternal\nData Transfer Rate6GB/s\nHard Drive Capacity480GB\nSpindle SpeedSolid State\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GEQNB SATA NHP SSD SATA",null,"g"]
["VK0480GEPQP","Description:HP G8 G9 480GB 3.5-inch LFF Hot-Plug SATA Value Endurance (VE)   6Gb/s  Enterprise Boot (EB)Solid State Drive (SSD) in HP G8 G9 Hot-Plug Drive traySmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 789147-B21\nSmartBuy Part# 789147-S21\nSpare Part# 789357-001\nAssembly Part# 789132-002\nModel# VK0480GEPQP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GEPQP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID507580\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GEPQP SATA SC SSD Solid State Drive",null,"g"]
["VK0480GEMQR","Description:HP 480GB 2.5-inch SFF SATA Quick Release Carrier (QR)\nValue Endurance (VE) 6Gb/s Solid State Drive (SSD)\nIn HP Hot-Plug Quick Release (QR) Drive tray (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 782845-B21\nSmartBuy Part# 782845-S21\nSpare Part# 782996-001\nAssembly Part# 782848-001\nModel# VK0480GEMQR\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA QR SSD\nPart NumberVK0480GEMQR\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID1700948\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GEMQR SATA QR SSD Solid State Drive",null,"g"]
["VK0480GEFJH","Description:HP G8 G9 480GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) M1 Solid State Drive (SSD)\nIn HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 764943-B21\nSmartBuy Part# 764943-S21\nSpare Part# 765023-001\nAssembly Part# 764913-003\nModel# VK0480GEFJH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GEFJH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504608\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\nBytes/Sector512\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GEFJH SATA SC SSD Solid State Drive",null,"g"]
["VK0480GECQP","Description:HP G8 G9 480GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 756660-B21\nSmartBuy Part# 756660-S21\nSpare Part# 757372-001\nAssembly Part# 756620-002\nModel# VK0480GECQP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GECQP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504508\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GECQP SATA SC SSD Solid State Drive",null,"g"]
["VK0480GDPVT","Description:HP 480GB 2.5-inch SFF Serial ATA (SATA)\nValue Endurance (VE)   6Gb/s  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 742391-B21\nSmartBuy Part# 742391-S21\nSpare Part# 742518-001\nAssembly Part# 729855-003\nModel# VK0480GDPVT\n\t\t\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GDPVT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504316\nTypeSolid State Drive (SSD)\nCapacity480GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationValue Endurance (VE)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GDPVT SATA SC SSD Solid State Drive",null,"g"]
["VK0480GDJXV","Description:HP G8 G9 480GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE)   6Gb/s  SC EnterpriseValue (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 718183-B21\nSmartBuy Part# 718183-S21\nSpare Part# 718296-001\nAssembly Part# 717968-002\nModel# VK0480GDJXV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0480GDJXV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504104\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0480GDJXV SATA SC SSD Solid State Drive",null,"g"]
["VK0400JEABD","Description:HP 400GB 3.5-inch LFF SAS 12Gb/s Mixed-Use (MU) \nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)Hot-Plug SmartDrive Carrier (SC) (as pictured) \nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive\nPart Number(s)\nOption Part# 762268-B21\nSmartBuy Part# 762268-S21\nSpare Part# 762748-001\nAssembly Part# 750222-001\nModel# VK0400JEABD\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK0400JEABD\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID498644\nTypeSolid State Drive\nCapacity400GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nData Transfer Rate1.2GB/s\nInterfaceSerial Attached SCSI\n4KB Random Read120000 IOPS\n4KB Random Write90000 IOPS\n \nFlash TypeMLC\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0400JEABD SAS SC SSD Solid State Drive",null,"g"]
["VK0300GDUQV","Description:HP G8 G9 300GB 3.5-inch LFF  Hot-Swap SATAValue Endurance (VE)   6Gb/s  SC Enterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 Hot-Plug Drive tray SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 739890-B21\nSmartBuy Part# 739890-S21\nSpare Part# 739955-001\nAssembly Part# 717968-004\nModel# VK0300GDUQV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0300GDUQV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504176\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity300GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\nHot SwapYes\n4KB Random Read64000IOPS\n4KB Random Write10000IOPS\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0300GDUQV SATA SC SSD Solid State Drive",null,"g"]
["VK0240GFLKF","Description:HP 240GB 2.5-inch SFF Serial ATA (SATA) Read-Intensive (RI)\nEnterprise   6Gb/s  Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 872853-B21\nSmartBuy Part# 872853-S21\nSpare Part# 872888-001\nAssembly Part# 838403-002\nModel# VK0240GFLKF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GFLKF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505264\nTypeSolid State Drive\nCapacity240GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS62000\nRandom Write IOPS8400\nAverage Latency155\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GFLKF SATA SC SSD Solid State Drive",null,"g"]
["VK0240GFDKF","Description:HP 240GB 3.5-inch 6Gb/s LFF SATA\nRead-Intensive (RI) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816893-B21\nSmart Buy# 816893-S21\nSpare Part# 817068-001\nAssembly Part# 816876-002\nModel# VK0240GFDKF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GFDKF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505076\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GFDKF SATA SC SSD Solid State Drive",null,"g"]
["VK0240GEYJQ","Description:HP 240GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804590-B21\nSmartBuy Part# 804590-S21\nSpare Part# 805373-001\nAssembly Part# 804574-003\nModel# VK0240GEYJQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GEYJQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504768\nTypeHard Drive - Hot Plug - Gen8\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nConnectivity TechnologySingle-Port\nRead IOPS61500 IOP/s\nWrite IOPS10200 IOP/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GEYJQ SATA SC SSD Solid State Drive",null,"g"]
["VK0240GEPQN","Description:HP G8 G9 240GB 3.5-inch LFF Hot-Plug SATA Value Endurance (VE)   6Gb/s  Enterprise Boot (EB)Solid State Drive (SSD) in HP G8 G9 Hot-Plug Drive traySmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 789137-B21\nSmartBuy Part# 789137-S21\nSpare Part# 789352-001\nAssembly Part# 789132-001\nModel# VK0240GEPQN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GEPQN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID704704\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GEPQN SATA SC SSD Solid State Drive",null,"g"]
["VK0240GEFJF","Description:HP G8 G9 240GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) M1 Solid State Drive (SSD)\nIn HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 764941-B21\nSmartBuy Part# 764941-S21\nSpare Part# 765022-001\nAssembly Part# 764913-002\nModel# VK0240GEFJF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GEFJF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1504592\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\nBytes/Sector512\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GEFJF SATA SC SSD Solid State Drive",null,"g"]
["VK0240GECQN","Description:HP G8 G9 240GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 756639-B21\nSmartBuy Part# 756639-S21\nSpare Part# 757367-001\nAssembly Part# 756620-001\nModel# VK0240GECQN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GECQN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504480\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GECQN SATA SC SSD Solid State Drive",null,"g"]
["VK0240GDJXU","Description:HP G8 G9 240GB 3.5-inch LFF Pluggable SATA  Value Endurance (VE)   6Gb/s  SC Enterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 718177-B21\nSmartBuy Part# 718177-S21\nSpare Part# 718294-001\nAssembly Part# 717968-001\nModel# VK0240GDJXU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0240GDJXU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504068\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0240GDJXU SATA SC SSD Solid State Drive",null,"g"]
["VK0120GFDKE","Description:HP 120GB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI)  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 816883-B21\nSmart Buy# 816883-S21\nSpare Part# 817063-001\nAssembly Part# 816876-001\nModel# VK0120GFDKE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0120GFDKE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505052\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity120GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0120GFDKE SATA SC SSD Solid State Drive",null,"g"]
["VK0120GEYJP","Description:HP 120GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804584-B21\nSmartBuy Part# 804584-S21\nSpare Part# 805372-001\nAssembly Part# 804574-002\nModel# VK0120GEYJP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0120GEYJP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504752\nTypeHard Drive - Hot Plug - Gen8\nLarge Form Factor3.5 inches\nCapacity120GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nConnectivity TechnologySingle-Port\nRead IOPS61500 IOP/s\nWrite IOPS5400 IOP/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0120GEYJP SATA SC SSD Solid State Drive",null,"g"]
["VK0120GEFJE","Description:HP G8 G9 120GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) M1 Solid State Drive (SSD)\nIn HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 764939-B21\nSmartBuy Part# 764939-S21\nSpare Part# 765021-001\nAssembly Part# 764913-001\nModel# VK0120GEFJE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0120GEFJE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504576\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity120GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\nBytes/Sector512\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0120GEFJE SATA SC SSD Solid State Drive",null,"g"]
["VK0080GEYJN","Description:HP 80GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive-2 (RI) Solid State Drivein G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 804578-B21\nSmartBuy Part# 804578-S21\nSpare Part# 805371-001\nAssembly Part# 804574-001\nModel# VK0080GEYJN\t\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK0080GEYJN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504736\nTypeHard Drive - Hot Plug - Gen8\nLarge Form Factor3.5 inches\nCapacity80GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nConnectivity TechnologySingle-Port\nRead IOPS61000 IOP/s\nWrite IOPS8400 IOP/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK0080GEYJN SATA SC SSD Solid State Drive",null,"g"]
["VK007680JWSSU","Description:HP 7.68TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P06590-B21\nSmartBuy Part# P06590-S21\nSpare Part# P08611-001\nAssembly Part# P02763-004\nModel# VK007680JWSSU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK007680JWSSU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID494645\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK007680JWSSU SAS SC SSD Solid State Drive",null,"g"]
["VK007680GWSXN","Description:HP 7.68TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04482-B21\nSmartBuy Part# P04482-S21\nSpare Part# P05316-001\nAssembly Part# P03483-005\nModel# VK007680GWSXN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK007680GWSXN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID506060\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK007680GWSXN SATA SC SSD Solid State Drive",null,"g"]
["VK003840JWSST","Description:HP 3.84TB 3.5-inch LFF SAS 12Gb/s Read-Intensive (RI) \nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)Hot-Plug SmartDrive Carrier (SC) (as pictured) \nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive\nPart Number(s)\nOption Part# P11329-B21\nSmartBuy Part# P11329-S21\nSpare Part# P11360-001\nAssembly Part# P02763-003\nModel# VK003840JWSST\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK003840JWSST\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID500152\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nData Transfer Rate1.2GB/s\nInterfaceSerial Attached SCSI\n4KB Random Read120000 IOPS\n4KB Random Write90000 IOPS\n \nFlash TypeMLC\nBest UseRead Intensive (RI)\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840JWSST SAS SC SSD Solid State Drive",null,"g"]
["VK003840GWTHD","Description:HP 3.84TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P06200-B21\nSmartBuy Part# P06200-S21\nSpare Part# P06574-001\nAssembly Part# P04954-004\nModel# VK003840GWTHD\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK003840GWTHD\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID506092\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840GWTHD SATA SC SSD Solid State Drive",null,"g"]
["VK003840GWSXL","Description:HP 3.84TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04480-B21\nSmartBuy Part# P04480-S21\nSpare Part# P05315-001\nAssembly Part# P03483-004\nModel# VK003840GWSXL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK003840GWSXL\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID506052\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840GWSXL SATA SC SSD Solid State Drive",null,"g"]
["VK003840GWSRV","Description:HP 3.84TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04570-B21\nSmartBuy Part# P04570-S21\nSpare Part# P05323-001\nAssembly Part# P02760-005\nModel# VK003840GWSRV\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK003840GWSRV\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505928\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840GWSRV SATA SC SSD Solid State Drive",null,"g"]
["VK003840GWJPK","Description:HP 3.84-TB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 877766-B21\nSmartBuy Part# 877766-S21 \nSpare Part# 878856-001\nAssembly Part# 877013-005\nModel# VK003840GWJPK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK003840GWJPK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID704832\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity3.84TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840GWJPK SATA SC SSD Solid State Drive",null,"g"]
["VK003840GWCFK","Description:HP 3.84TB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI)  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 876432-B21\nSmartBuy Part# 876432-S21\nSpare Part# 875355-001\nAssembly Part# 866615-005\nModel# VK003840GWCFK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK003840GWCFK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1704940\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity3.84TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK003840GWCFK SATA SC SSD Solid State Drive",null,"g"]
["VK001920KWDUH","Description:HP 1.92 TB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 875591-B21\nSmartBuy Part# 875591-S21\nSpare Part# 875873-001\nAssembly Part# 869252-003\nModel# VK001920KWDUH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVK001920KWDUH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1711144\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920KWDUH NVMe SCN SSD Solid State Drive",null,"g"]
["VK001920JWSSR","Description:HP 1.92TB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P06586-B21\nSmartBuy Part# P06586-S21\nSpare Part# P08609-001\nAssembly Part# P02763-002\nModel# VK001920JWSSR\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK001920JWSSR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID494597\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920JWSSR SAS SC SSD Solid State Drive",null,"g"]
["VK001920GWTHC","Description:HP 1.92TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P06198-B21\nSmartBuy Part# P06198-S21\nSpare Part# P06573-001\nAssembly Part# P04954-003\nModel# VK001920GWTHC\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWTHC\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1506084\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWTHC SATA SC SSD Solid State Drive",null,"g"]
["VK001920GWSXK","Description:HP 1.92TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04478-B21\nSmartBuy Part# P04478-S21\nSpare Part# P05314-001\nAssembly Part# P03483-003\nModel# VK001920GWSXK\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWSXK\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1506028\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWSXK SATA SC SSD Solid State Drive",null,"g"]
["VK001920GWSRU","Description:HP 1.92TB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P09693-B21\nSmartBuy Part# P09693-S21\nSpare Part# P09848-001\nAssembly Part# P02760-004\nModel# VK001920GWSRU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWSRU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505912\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity1.92TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWSRU SATA SC SSD Solid State Drive",null,"g"]
["VK001920GWJPH","Description:HP 1.92TB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 877760-B21\nSmartBuy Part# 877760-S21\nSpare Part# 878853-001\nAssembly Part# 877013-004\nModel# VK001920GWJPH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWJPH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505772\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity1.92TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWJPH SATA SC SSD Solid State Drive",null,"g"]
["VK001920GWEZE","Description:HP 1.92TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 875513-B21\nSmartBuy Part# 875513-S21\nSpare Part# 875657-001\nAssembly Part# 870667-004\nModel# VK001920GWEZE\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWEZE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID493162\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWEZE SATA SC SSD Solid State Drive",null,"g"]
["VK001920GWCFH","Description:HP 1.92TB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 868826-B21\nSmartBuy Part# 868826-S21\nSpare Part# 868930-001\nAssembly Part# 866615-004\nModel# VK001920GWCFH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001920GWCFH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505392\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS61500\nRandom Write IOPS26000\nAverage Latency120\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001920GWCFH SATA SC SSD Solid State Drive",null,"g"]
["VK001600GWCNT","Description:HP 1.6TB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive (RI) Digitally Signed (DS)\nSolid State Drive in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 869388-B21\nSmartBuy Part# 869388-S21\nSpare Part# 869582-001\nAssembly Part# 867213-005\nModel# VK001600GWCNT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001600GWCNT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505492\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity1.6TB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001600GWCNT SATA SC SSD Solid State Drive",null,"g"]
["VK001200GWDRP","Description:HP 1.2TB 2.5-inch SFF Serial ATA (SATA) Read-Intensive (RI)\nEnterprise   6Gb/s  Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 869157-B21\nSmartBuy Part# 869157-S21\nSpare Part# 869196-001\nAssembly Part# 869156-001\nModel# VK001200GWDRP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK001200GWDRP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505548\nTypeSolid State Drive\nCapacity1.2TB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS55000\nRandom Write IOPS14000\nAverage Latency155\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK001200GWDRP SATA SC SSD Solid State Drive",null,"g"]
["VK000960KWDUF","Description:HP 960GB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 875589-B21\nSmartBuy Part# 875589-S21\nSpare Part# 875872-001\nAssembly Part# 869252-002\nModel# VK000960KWDUF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVK000960KWDUF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID711124\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity960GB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960KWDUF NVMe SCN SSD Solid State Drive",null,"g"]
["VK000960JWSSQ","Description:HP 960GB 12Gb/s 2.5-inch SFF SAS Read-Intensive (RI)\nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P06584-B21\nSmartBuy Part# P06584-S21\nSpare Part# P08608-001\nAssembly Part# P02763-001\nModel# VK000960JWSSQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberVK000960JWSSQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1494580\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSAS\nDrive Interface StandardSAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960JWSSQ SAS SC SSD Solid State Drive",null,"g"]
["VK000960GWTHB","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P06196-B21\nSmartBuy Part# P06196-S21\nSpare Part# P06572-001\nAssembly Part# P04954-002\nModel# VK000960GWTHB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWTHB\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1506076\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWTHB SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWSXH","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04476-B21\nSmartBuy Part# P04476-S21\nSpare Part# P05313-001\nAssembly Part# P03483-002\nModel# VK000960GWSXH\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWSXH\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1506020\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWSXH SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWSRT","Description:HP 960GB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P09689-B21\nSmartBuy Part# P09689-S21\nSpare Part# P09846-001\nAssembly Part# P02760-003\nModel# VK000960GWSRT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWSRT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505872\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity960GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWSRT SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWJPF","Description:HP 960GB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 877754-B21\nSmartBuy Part# 877754-S21\nSpare Part# 878850-001\nAssembly Part# 877013-003\nModel# VK000960GWJPF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWJPF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505740\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity960GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWJPF SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWEZD","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 875511-B21\nSmartBuy Part# 875511-S21\nSpare Part# 875656-001\nAssembly Part# 870667-003\nModel# VK000960GWEZD\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWEZD\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID493146\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWEZD SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWCNR","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 869384-B21\nSmartBuy Part# 869384-S21\nSpare Part# 869580-001\nAssembly Part# 867213-004\nModel# VK000960GWCNR\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWCNR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505476\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS55000\nRandom Write IOPS14000\nAverage Latency155\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWCNR SATA SC SSD Solid State Drive",null,"g"]
["VK000960GWCFF","Description:HP 960GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 868822-B21\nSmartBuy Part# 868822-S21\nSpare Part# 868928-001\nAssembly Part# 866615-003\nModel# VK000960GWCFF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000960GWCFF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505384\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS64000\nRandom Write IOPS24500\nAverage Latency120\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000960GWCFF SATA SC SSD Solid State Drive",null,"g"]
["VK000800GWCYU","Description:HP 800GB 2.5-inch SFF Serial ATA (SATA) Read-Intensive (RI)\nDigitally Signed (DS)   6Gb/s  Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 880507-B21\nSmartBuy Part# 880507-S21\nSpare Part# 880804-001\nAssembly Part# 867213-006\nModel# VK000800GWCYU\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.Leveraging NAND Flash technology - they support HP Proliant servers including Gen8 Gen9 and Gen10 server storage platforms. Because they are available as Small Form Factor (SFF) and Large Form Factor (LFF) hot plug devices - non-hot plug SFF devices - and SFF Quick Release devices - you have great flexibility in your installation.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000800GWCYU\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505532\nTypeSolid State Drive (SSD)\nCapacity800GB\nInterface TypeSerial ATA (SATA)\nDrive Interface Standard6Gb/s SAS\nBest applicationRead Intensive (RI)\nDrive TraySmart Carrier (SC)\nHot SwapYes\nPre-Failure WarrantyYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000800GWCYU SATA SC SSD Solid State Drive",null,"g"]
["VK000480KWDUE","Description:HP 480GB 2.5-inch SFF NVMe x4 Lanes SSD\nMainstream Performance (MP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# 875587-B21\nSmartBuy Part# 875587-S21\nSpare Part# 875871-001\nAssembly Part# 869252-001\nModel# VK000480KWDUE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) Solid State Drives are best suited for applications requiring a strong blend of high read IOPS - low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe Mainstream Performance (MP) Read Intensive (RI) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads such as read caching - social media and bulk storage that require outstanding IOPS per watt and cost per IOPS as an upgrade path from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberVK000480KWDUE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID711104\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity480GB\nInterface TypeNVMe\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480KWDUE NVMe SCN SSD Solid State Drive",null,"g"]
["VK000480GWTHA","Description:HP 480GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P06194-B21\nSmartBuy Part# P06194-S21\nSpare Part# P06571-001\nAssembly Part# P04954-001\nModel# VK000480GWTHA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWTHA\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID506068\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWTHA SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWSXF","Description:HP 480GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04474-B21\nSmartBuy Part# P04474-S21\nSpare Part# P05312-001\nAssembly Part# P03483-001\nModel# VK000480GWSXF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWSXF\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505996\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWSXF SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWSRR","Description:HP 480GB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P09687-B21\nSmartBuy Part# P09687-S21\nSpare Part# P09845-001\nAssembly Part# P02760-002\nModel# VK000480GWSRR\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWSRR\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505848\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWSRR SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWJPE","Description:HP 480GB 3.5-inch 6Gb/s LFF SATA\nHot-Plug Read-Intensive (RI) Digitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 877748-B21\nSmartBuy Part# 877748-S21 \nSpare Part# 878847-001\nAssembly Part# 877013-002\nModel# VK000480GWJPE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWJPE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505724\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWJPE SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWEZC","Description:HP 480GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 875509-B21\nSmartBuy Part# 875509-S21\nSpare Part# 875655-001\nAssembly Part# 870667-002\nModel# VK000480GWEZC\n\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWEZC\nProducts ID49313\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWEZC SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWCNQ","Description:HP 480GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive (RI) Digitally Signed (DS)\nSolid State Drive in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 869380-B21\nSmartBuy Part# 869380-S21\nSpare Part# 869578-001\nAssembly Part# 867213-003\nModel# VK000480GWCNQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWCNQ\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505452\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity480GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWCNQ SATA SC SSD Solid State Drive",null,"g"]
["VK000480GWCFE","Description:HP 480GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 868818-B21\nSmartBuy Part# 868818-S21\nSpare Part# 868926-001\nAssembly Part# 866615-002\nModel# VK000480GWCFE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000480GWCFE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505360\nTypeSolid State Drive\nCapacity480GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS66000\nRandom Write IOPS17000\nAverage Latency120\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000480GWCFE SATA SC SSD Solid State Drive",null,"g"]
["VK000240GWSRQ","Description:HP 240GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# P04556-B21\nSmartBuy Part# P04556-S21\nSpare Part# P05319-001\nAssembly Part# P02760-001\nModel# VK000240GWSRQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000240GWSRQ\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID505832\nTypeSolid State Drive\nCapacity240GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS66000\nRandom Write IOPS9800\nAverage Latency120\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000240GWSRQ SATA SC SSD Solid State Drive",null,"g"]
["VK000240GWJPD","Description:HP 240GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 877740-B21\nSmartBuy Part# 877740-S21\nSpare Part# 878844-001\nAssembly Part# 877013-001\nModel# VK000240GWJPD\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000240GWJPD\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1493178\nTypeSolid State Drive\nCapacity240GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000240GWJPD SATA SC SSD Solid State Drive",null,"g"]
["VK000240GWEZB","Description:HP 240GB 2.5-inch SFF RW SATA ReadIntensive (RI) 6Gb/s Digitally Signed Firmware (DS) Solid State Drive (SSD)In HP Hot-Plug SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 875507-B21\nSmartBuy Part# 875507-S21\nSpare Part# 875654-001\nAssembly Part# 870667-001\nModel# VK000240GWEZB\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000240GWEZB\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID700232\nProduct TypeSolid State Drive\nCapacity240GB\nInterface TypeSerial ATA-600\nDrive Interface Standard6Gb/s SATA\n4KB Random Read IOPS62500\n4KB Random Write IOPS33000\nForm Factor2.5 inch SFF\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000240GWEZB SATA SC SSD Solid State Drive",null,"g"]
["VK000240GWCNP","Description:HP 240GB 3.5-inch SCC LFF Pluggable\nSATA6Gb/s Hot-Plug Read-Intensive (RI) Digitally Signed (DS)\nSolid State Drive in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 872067-B21\nSmartBuy Part# 872067-S21\nSpare Part# 872184-001\nAssembly Part# 867213-002\nModel# VK000240GWCNP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000240GWCNP\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID704956\nTypeHard Drive - Hot Plug\nLarge Form Factor3.5 inches\nCapacity240GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000240GWCNP SATA SC SSD Solid State Drive",null,"g"]
["VK000240GWCFD","Description:HP 240GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 868814-B21\nSmartBuy Part# 868814-S21\nSpare Part# 868924-001\nAssembly Part# 866615-001\nModel# VK000240GWCFD\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000240GWCFD\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID505352\nTypeSolid State Drive\nCapacity240GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS66000\nRandom Write IOPS9800\nAverage Latency120\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000240GWCFD SATA SC SSD Solid State Drive",null,"g"]
["VK000150GWCNN","Description:HP 150GB 2.5-inch SFF SATA Read-Intensive (RI)  6Gb/s  \nDigitally Signed Firmware (DS) Solid State Drive (SSD)in G8 G9 G10 (Gen8 Gen9 Gen10) Hot-Plug\nHP SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 869374-B21\nSmartBuy Part# 869374-S21\nSpare Part# 869575-001\nAssembly Part# 867213-001\nModel# VK000150GWCNN\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberVK000150GWCNN\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1505428\nTypeSolid State Drive\nCapacity150GB\nInterface TypeSerial ATA\nDrive Interface Standard6Gb/s SATA\nRandom Read IOPS41000\nRandom Write IOPS6500\nAverage Latency145\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VK000150GWCNN SATA SC SSD Solid State Drive",null,"g"]
["VB0250EAVER","Description:HP 250GB 3.5-inch LFF Serial ATA (SATA)\n3Gb/s 7.2K Hot-Plug Entry (ETY) Hard Drive\nIn G1-G7 (Gen1-Gen7) Hot-Plug carrier (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# 681229-B21\nSmartBuy Part# 681229-S21\nSpare Part# 681647-001\nAssembly Part# 571227-002\nModel# VB0250EAVER\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SATA Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SATA interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberVB0250EAVER\n\n\n\nProducts ID1507356\nCapacity250GB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time7.6ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VB0250EAVER SATA 7.2K",null,"g"]
["VB0160EAVEQ","Description:HP 160GB 3Gb/s 7.2K 3.5-inch LFF SATA\nEntry Level (ETY) Hard Drive\nIn HP Quick Release Carrier (QR) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 574021-B21\nSmartBuy Part# 574021-S21\nSpare Part# 574269-001\nAssembly Part# 571227-001\nModel# VB0160EAVEQ\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. HP SATA 7200 rpm Hard Drives provide entry-level performance and high capacity for select Proliant servers. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA QR\nPart NumberVB0160EAVEQ\n\n\n\nProducts ID700360\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeSerial ATA\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate3GB/s\nAverage Seek Time9ms\nRotational Speed7200RPM\n \nDimensions (LxWxH)7.25 x 4.36 x 1.04 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VB0160EAVEQ SATA QR 7.2K",null,"g"]
["VB0160CBCDE","Description:160GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch highIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349238-B21\nSmartBuy Part# 349238-S21\nSpare Part# 459317-001\nAssembly Part# 593333-001\nModel# VB0160CBCDE\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberVB0160CBCDE\n\n\n\nProducts ID1461872\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# VB0160CBCDE SATA 7.2K",null,"g"]
["U4545E","Description: 3 Year Onsite Warranty 24x7 - 4 hour response\n* This item can only be purchased and applied to a new HP server from inventory.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nIncrease equipment availability and productivity with round-the-clock onsite and remote support for your HP hardware  as well as selected multivendor equipment. This flexible HP Care Pack Service covers desktops  workstations  servers  storage systems  and network equipment.\n\n\n4-hour onsite response 24x7x365 - For issues that cannot be resolved remotely  an authorized HP Services representative arrives at your site within 4 hours after your call has been logged. Service is available around-the-clock every day  including all holidays. HP Services returns your covered hardware to operational condition  repairing or replacing components or entire units as necessary. Your coverage includes all required parts and materials. \n\nSpecifications:\nCategoryHP Care Pack\nSub-Category24x7x3Yr\nGeneration4 Hour Response\nPart NumberU4545E\n\n\n\nProducts ID143110",null,"g"]
["TRS23XAEF","Description:160/320GB SDLT 160/320GB SCSI LVD Loader Library Drive\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberTRS23XAEF\nProducts ID141603",null,"g"]
["TRS23BA-YF","Description:Quantum 160/320GB SDLT320 (BRC)32MB/sec LVD Single Ended Tape DrivePart Number(s)Part# TRS23BA-YF\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryQuantum\nSub-CategoryTape Drive\nGeneration\nPart NumberTRS23BA-YF\nProducts ID1008672",null,"g"]
["TRS12XAEF","Description:TRS12XAEF DLT 110/220 GB W/Trade-In\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberTRS12XAEF\nProducts ID141602",null,"g"]
["TK0120GECQL","Description:HP G8 G9 120GB 3.5-inch LFF Pluggable Serial ATA (SATA) Value Endurance (VE) 6Gb/s SCEnterprise Value (EV) Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 756624-B21\nSmartBuy Part# 756624-S21\nSpare Part# 757362-001\nAssembly Part# 756619-001\nModel# TK0120GECQL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberTK0120GECQL\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504456\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity120GB\nInterface TypeSerial ATA-600\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# TK0120GECQL SATA SC SSD Solid State Drive",null,"g"]
["TK0120GDJXT","Description:HP G8 G9 120GB 3.5-inch LFF Hot-Plug SATA Value Endurance (VE)   6Gb/s  Enterprise Boot (EB)Solid State Drive (SSD) in HP G8 G9 Hot-Plug Drive traySmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 718171-B21\nSmartBuy Part# 718171-S21\nSpare Part# 718300-001\nAssembly Part# 717964-001\nModel# TK0120GDJXT\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberTK0120GDJXT\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID495553\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity120GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# TK0120GDJXT SATA SC SSD Solid State Drive",null,"g"]
["TK0080GDSAE","Description:HP G8 G9 80GB 3.5-inch LFF Pluggable SATA  Value Endurance (VE)   6Gb/s  SC Enterprise Boot (EB)Solid State Drive (SSD)In HP G8 G9 2 ½ inch to 3 ½ inch Hot-Plug\nSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# 734362-B21\nSmartBuy Part# 734362-S21\nSpare Part# 734563-001\nAssembly Part# 717964-002\nModel# TK0080GDSAE\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberTK0080GDSAE\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID504028\nTypeSolid State Drive\nLarge Form Factor3.5 inches\nCapacity80GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# TK0080GDSAE SATA SC SSD Solid State Drive",null,"g"]
["TH8AL-CL","Description:40/80GB DLT8000 Internal StandAlone LVD/SCSI OpalPart Number(s)Option Part# TH8AL-CL \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nAs data protection and high availability have become increasingly important, customers are demanding solid  uninterrupted performance. Continuous development and enhancement of high-performance software applications and operating systems is driving the need for secure backup solutions. Compaq TapeDrive customers can be assured that all of their backup needs will be met. The above issues will be addressed  and they will have equipment manufactured to the highest quality standards and subjected to the most rigorous testing procedures that only genuine components will realize. \n\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration40/80GB\nPart NumberTH8AL-CL\n\n\n\nProducts ID1013341\nTape TypeDLT\nNative Capacity40GB\nInterface TypeSCSI\nEnclosure TypeInternal\nCompressed Capacity80GB\nSCSI Signaling TypeLow Voltage Differential (LVD)",null,"g"]
["TA450DC","Description:Fan 4.7 inches X 4.7 inches X 1.5 inches V.D.C. 28AMP 120MM X 120MM X 40MMPart Number(s)\nHewlett-Packard Part# TA450DC\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryFan Module\nSub-Category\nGeneration\nPart NumberTA450DC\nProducts ID141365",null,"g"]
["T6F44UT#ABA","Description:HP Elitebook 840 G3 Core i5 6200U 2.3GHz Notebook PCPart Number(s)\nOption Part# T6F44UT#ABA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  EliteBook 840 empowers users to create - connect - and collaborate - using enterprise-class performance technology that helps keep you productive in and out of the office.\n\nSpecifications:\nCategoryElitebook\nSub-CategoryNotebook\nGeneration840 G3\nPart NumberT6F44UT#ABA\n\n\n\nProducts ID1490899\nManufacturerHP\nProduct TypeNotebook\nMemory Slots2 SODIMM\nMemory Standard4GB LPDDR3-1866 SDRAM\nHard Drive Description500GB 7200rpm SATA\nChipsetIntegrated with Processor\nProcessor Speed2.3GHz\nProcessorIntel Core i5-6200U\n \nGraphicsIntel HD Graphics 520\nDisplay14\" HD SVA Display\n \nBattery TypeHP Long Life 3-cell, 46 WHr LI-ion\nPower45W/65W Smart AC Adapter\n \nExpansion Slots1 Media Card Reader/1External SIM\nPorts 1 USB 3.0\n \nData Link ProtocolBluetooth 4.2, Ethernet, Fast Ethernet\nWired ProtocolGigabit Etherenet\n \n \nWireless NICIntel Dual Band Wireless-AC 8260\nOptical DriveNo Optical Drive\n \n \nDimensions WxHxD13.3in x 0.7in x 9.3in\nFrequency Required50/60Hz\n \n \nNominal VoltageAC 120/230V\nPower Provided45 Watt",null,"g"]
["SYJKT0300GBAS15K","Description:HP M6710 300GB 2.5-inch Serial AttachedSCSI (SAS) SFF 6Gb/s Hot-Plug 15K Hard DriveIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)Part Number(s)\nOption Part# QR492A\nSpare Part# 697387-001\nModel# SYJKT0300GBAS15K\nManufacturer Part# 9SW066-088\nManufacturer Part# 5697-1842\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSerial Attached SCSI (SAS) is the logical evolution of SCSI combining its long-established software advantage with the SAS electrical and physical connection.  With enterprise storage requirements escalating and becoming more complex  factors such as larger capacity  greater density  security  scalability and accessibility are more critical than ever.\n\nSpecifications:\nCategory3Par HardDrive\nSub-Category15K\nGenerationSAS 3PAR\nPart NumberSYJKT0300GBAS15K\n\n\n\nProducts ID1476583\nTypeHard Drive - Hot-Swap\nCapacity300GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nTray Type3PAR\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SYJKT0300GBAS15K SAS 3PAR 15K",null,"g"]
["ST9500620NS","Description:HP 500GB 2.5-inch SFF SATA   6Gb/s  7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 655708-B21\nSmartBuy Part# 655708-S21\nSpare Part# 656107-001\nAssembly Part# 614829-002\nModel# ST9500620NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST9500620NS-SC\n\n\n\nProducts ID472502\nTypeHard Drive - Hot-Swap - Gen8\nSmall Form Factor2.5 inches\nCapacity500GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST9500620NS SATA SC 7.2K",null,"g"]
["ST9500530NS","Description:HP 500GB 3Gb/s 7.2K 2.5-inch SFF SATA\nMidline (MDL) Hard Drive\nIn HP Quick Release Carrier (QR) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# 574953-B21\nSpare Part# 575054-001\nAssembly Part# 507749-001\nAssembly Part# 614828-002\nModel# MM0500EANCR\nModel# ST9500530NS\nModel# ST9500620NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA QR\nPart NumberST9500530NS\n\n\n\nProducts ID1461952\nTypeHard Drive - Quick Release\nSmall Form Factor2.5 inches\nCapacity500GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate3GB/s\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST9500530NS SATA QR 7.2K",null,"g"]
["ST9300653SS","Description:HP 300GB 2.5-inch SFF SAS   6Gb/s  15K RPM\nEnterprise (ENT) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SFF SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SAS Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# 652611-B21\nSpare Part# 653960-001\nAssembly Part# 652625-002\nAssembly Part# 627114-002\nModel# EH0300FCBVC\nModel# EH0300FBQDD\nModel# ST9300653SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSAS is the logical evolution of SCSI including its long-established software advantage and the serial physical connection interface. With enterprise storage requirements escalating and becoming more complex factors such as larger capacity greater density security scalability and accessibility are more critical than ever. Enterprise data centers must be online all the time fulfill requests from numerous users simultaneously allow for constant growth and expansion and be maintained while in operation. Serial Attached SCSI meets all these demands while providing the highest performance.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS SC\nPart NumberST9300653SS-SC\n\n\n\nProducts ID1472618\nTypeHard Drive - Hot-Swap\nCapacity300GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nSpeed6G = 6Gb/sec (750 MB/s)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST9300653SS SAS SC 15K",null,"g"]
["ST91000640NS","Description:HP 1TB 2.5-inch SFF SATA   6Gb/s  7.2K RPM\n512n Midline (MDL) Hot-Plug Hard Drive\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 G10 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 655710-B21\nSmartBuy Part# 655710-S21\nSpare Part# 656108-001\nAssembly Part# 614829-003\nModel# MM1000GBKAL\nModel# ST91000640NS\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST91000640NS  \n\n\n\nProducts ID1461922\nTypeHard Drive - Hot-Swap - Gen8\nSmall Form Factor2.5 inches\nCapacity1000GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST91000640NS SATA SC 7.2K",null,"g"]
["ST500NM0011","Description:HP 500GB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\n512n Midline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 658071-B21\nSpare Part# 658103-001\nAssembly Part# 658083-001\nAssembly Part# 658084-001\nModel# MB0500GCEHE\nModel# MB0500GCEHF\nModel# ST500NM0011\nSmartBuy Part# 658071-S21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST500NM0011-SC\n\n\n\nProducts ID1472934\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity500GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST500NM0011 SATA SC 7.2K",null,"g"]
["ST4000NM0023","Description:HP 4TB 3.5-inch LFF SAS   6Gb/s  7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) LFF SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SAS Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 695510-B21\nSpare Part# 695842-001\nAssembly Part# 695507-004\nAssembly Part# 652755-007\nModel# MB4000FCWDK\nSeagate Part# ST4000NM0023\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberST4000NM0023-SC\n\n\n\nProducts ID1473407\nCapacity4TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate768MB/s\nAverage Seek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST4000NM0023 SAS SC 7.2K",null,"g"]
["ST3808110AS","Description:80GB 3.5-inch LFF SATA 1.5G 7.2K\nMidline (MDL) Hard Drive\nIn HP G1-G7 Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349237-B21\nSpare Part# 397551-001\nAssembly Part# 407525-001\nModel# ST3808110AS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. HP SATA 7200 rpm Hard Drives provide entry-level performance and high capacity for select Proliant servers. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3808110AS\n\n\n\nProducts ID1461857\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity80GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (ATA) plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3808110AS SATA 7.2K",null,"g"]
["ST3802110A","Description:80 GB ATA-100 7.2 3.5-inch Hard DriveGenuine HP serial number and firmwarePart Number(s)\nOption Part# 278424-B21\nSpare Part# 287685-001\nAssembly Part# 408995-002\nModel# ST3802110A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nCompaq Hard Drives are provided with the reliability and functionality needed for today's systems. All Hard Drives are designed and tested for compatibility and interoperability in the systems for which they are intended in order to provide the immediate  flawless integration expected from Compaq storage solutions. Compaq's hard disk drives provide a cost-effective solution for those customers with increasing capacity requirements.\n\nSpecifications:\nCategoryProliant Hard Drive\nSub-CategoryATA\nGeneration7.2K\nPart NumberST3802110A \n\n\n\nProducts ID462147\nForm FactorEnterprise\nCapacity80GB\nInterfaceIDE/EIDE\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nExternal Data Transfer Rate100MB/s\nSeek Time8.5ms\n \nAverage Latency4.17ms\nInterface (Detailed)DMA/ATA-100 (Ultra)\n \nPlatformPC\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3802110A 7.2K ATA",null,"g"]
["ST3750640NS","Description:750GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch high NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 432341-B21\nSmartBuy Part# 432341-S21\nSpare Part# 432401-001\nAssembly Part# 432337-003\nModel# ST3750640NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3750640NS\n\n\n\nProducts ID506208\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity750GB\nInterface TypeSerial ATA-150\nConnectorSerial ATA (SATA) Plug\nData Transfer Rate150MB/s\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3750640NS SATA 7.2K",null,"g"]
["ST3750330NS","Description:HP MSA/MSA2 750GB 3.5-inch LFF SATA 3Gb/s 7.2K\nDual Port (DP) MidLine (MDL) Hot-Plug Hard Drive\nIn HP Hot-Plug MSA/MSA2 Hard Drive tray (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AJ868A\nSpare Part# 480941-001\nAssembly Part# 481281-001\nAssembly Part# 481286-002\nModel# ST3750330NS\n\nNote:\nFor use in HP StorageWorks MSA/MSA2 Systems only.\nModular Smart Array (MSA) 2000/2000i Systems.\nModular Smart Array 2 (MSA2) 1040/2040/P2000 Systems.\nComplete HDD compatibility table listed below.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SATA disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SATA interposers attached to the back. The SATA interposers have active logic on them that will convert a single-ported SATA disk module into a dual-ported disk module. If you look closely - you will see a MULTIPLEXER chip on the interposer which is responsible for this function. Even though the SCA-40 connector is reminiscent of a connector on a Fibre Channel disk drive - no SATA-FC bridge chip exists on this interposer.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSATA MSA2\nPart NumberST3750330NS\n\n\n\nProducts ID1461848\nCapacity750GB\nInterfaceSerial ATA\nEnclosureInternal\nHDD Form Factor3.5 inches\nSpindle Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time9ms \nAverage Latency4.17ms \n \nHot SwapYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3750330NS SATA MSA2 7.2K",null,"g"]
["ST373405LW","Description:73.4GB Wide SCSI 10K RPM 3.5-inch Part# ST373405LW \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSeagate’s enormous 73.4GB Cheetah 73 Hard Drive - the largest currently available - is perfect for workstations  disk arrays  file servers  corporate intranets  data warehousing operations  and supercomputers alike! It features an Ultra160 SCSI interface  which delivers data at up to 160MB per second  and combines Ultra2 SCSI technology with cyclic redundancy check (CRC)  domain validation  and double transition clocking! The 3.5-inch  half-height Cheetah also features an impressive 5.6ms seek time and a 427Mb per second internal transfer rate  enhancing overall drive performance.\n\nSpecifications:\nCategorySeagate HardDrive\nSub-CategoryUltra3\nGeneration10K\nPart NumberST373405LW\n\n\n\nProducts ID144121\nCapacity73400 MB\nRotational Speed10000 RPM\nAccess Time4.9 ms\nCache Size0.004096 MB\nDrive Width3.5",null,"g"]
["ST373307LW","Description:73GB Ultra 320 (U320) 3.5-inch SCSI68-Pin Non-Hot-Plug 68-pin 10K Hard DrivePart Number(s)\nSeagate Part# ST373307LW\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe Cheetah 10K lowers cost of ownership with the industry's highest reliability  designed for full duty cycle applications  Seagate-exclusive Background Media Scan  enhanced Error Correction Code; and low power and cooling requirements.\n\nSpecifications:\nCategorySeagate HardDrive\nSub-CategoryU320\nGeneration10K\nPart NumberST373307LW\n\n\n\nProducts ID141446\nHot Swap TrayNot Included\nCapacity73GB\nHeight1.0 inch/2.54cm\nWidth4.0 inch/10.16cm\nInterfaceUltra320 SCSI\nData Transfer Rate320MB/s\nSeek TimeSingle Track 0.55ms\nSeek TimeAverage 4.9ms\n \nSeek TimeFull Stroke 10.0ms\nRotational Speed10K\n \nBytes/Sector512\nManufacturerSeagate\n \nApplicationServer Storage\nBackward CompatabilityU2 and U3 Speeds\n \nPre-Failure WarrantyYes\nData Storage Device TypeSAS (Server Attached Storage)\n \n \nHard Drive Device TypeHard drive for server/storage unit",null,"g"]
["ST3600057SS-MSA","Description:HP MSA/MSA2 60GB 3.5-inch LFF SAS   6Gb/s  15K RPM\nDual Port (DP) Enterprise (ENT) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AP860A\nSpare Part# 601777-001\nAssembly Part# 586592-003\nAssembly Part# 601712-001\nAssembly Part# 604088-001\nAssembly Part# 606227-003\nModel# ST3600057SS\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category15K\nGenerationSAS MSA 2\nPart NumberST3600057SS-MSA\n\n\n\nProducts ID1462030\nCapacity600GB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed15000RPM\nExternal Data Transfer6GB/s\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\nPortsDual Port\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3600057SS-MSA SAS MSA 2 15K",null,"g"]
["ST3500641AS","Description:500GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch high NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 395473-B21\nSpare Part# 395501-001\nAssembly Part# 395474-001\nAssembly Part# 454141-002\nAssembly Part# 601452-001\nAssembly Part# 432337-002\nAssembly Part# 432337-004\nAssembly Part# 407525-004\nModel# GB0500C8046\nModel#GB0500C4413\nModel# 6H500F0\nModel# MB0500CBEPQ\nModel# ST3500630NS\nModel# ST3500641AS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3500641AS\n\n\n\nProducts ID1461850\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches\nCapacity500GB\nInterface TypeSerial ATA-150\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3500641AS SATA 7.2K",null,"g"]
["ST3500630NS","Description:HP 500GB Hot-Plug SATA 1.5G 7.2K 3.5-inch LFF NCQ (Native Command Queing)In HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 395473-B21\nSmartBuy Part# 395473-S21\nSpare Part# 395501-001\nAssembly Part# 432337-002\nModel# ST3500630NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3500630NS\n\n\n\nProducts ID200019\nCapacity500GB\nInterfaceSerial ATA\nEnclosureInternal\nSpindle Speed7200RPM\nData Transfer Rate1.5G = 1.5Gb/sec (187.5MB/s)\nAverage Latency4.17ms\nInterface TypeSerial ATA\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3500630NS SATA 7.2K",null,"g"]
["ST3500320NS","Description:HP MSA/MSA2 500GB 3.5-inch LFF SATA  3Gb/s  7.2K\nDual Port (DP) MidLine (MDL) Hot-Plug Hard Drive\nIn HP Hot-Plug MSA/MSA2 Hard Drive tray (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AJ738A\nSpare Part# 480940-001\nAssembly Part# 481280-001\nAssembly Part# 481286-001\nModel# ST3500320NS\n\nNote:\nFor use in HP StorageWorks MSA/MSA2 Systems only.\nModular Smart Array (MSA) 2000/2000i Systems.\nModular Smart Array 2 (MSA2) 1040/2040/P2000 Systems.\nComplete HDD compatibility table listed below.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SATA disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SATA interposers attached to the back. The SATA interposers have active logic on them that will convert a single-ported SATA disk module into a dual-ported disk module. If you look closely - you will see a MULTIPLEXER chip on the interposer which is responsible for this function. Even though the SCA-40 connector is reminiscent of a connector on a Fibre Channel disk drive - no SATA-FC bridge chip exists on this interposer.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSATA MSA2\nPart NumberST3500320NS\n\n\n\nProducts ID1461845\nCapacity500GB\nInterfaceSerial ATA\nEnclosureInternal\nHDD Form Factor3.5 inches\nSpindle Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time9ms \nAverage Latency4.17ms \n \nHot SwapYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3500320NS SATA MSA2 7.2K",null,"g"]
["ST336753LW","Description:Seagate Cheetah 36.7 GB 15K SCSI Ultra 320 (U320) 68-Pin Non-Hot-Plug 68-Pin Hard DriveGenuine HP serial number and firmwarePart Number(s)\nSeagate Part# ST336753LW\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberST336753LW\nProducts ID144331",null,"g"]
["ST3300657SS","Description:HP MSA/MSA2 300GB 3.5-inch LFF SAS   6Gb/s  15K RPM\nDual Port (DP) Enterprise (ENT) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AP858A\nSpare Part# 601775-001\nAssembly Part# 604086-001\nModel# ST3300657SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane. \n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category15K\nGenerationSAS MSA 2\nPart NumberST3300657SS\n\n\n\nProducts ID1475988\nForm FactorLFF\nCapacity300GB\nInterfaceSAS\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed15000RPM\nExternal Data Transfer Rate6144MB/s\nSeek Time3.5ms\n \nAverage Latency2ms\nInterface (Detailed)SAS-300\n \nHot SwapYes\nMTBF1700000 Hours\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3300657SS SAS MSA 2 15K",null,"g"]
["ST33000650SS","Description:HP P2000 3TB 3.5-inch Serial Attached SCSI (SAS) LFF 6Gb/sDual Port Midline (MDL) Hot-Plug 7.2K MSA2 Hard Drive in HP MSA/MSA2 drive tray with interposer connector (as pictured )In HP Hot-Plug MSA Hard Drive Tray (as pictured)For HP MSA1040 MSA2040 MSA2050 MSA2052 MSA2000 MSA2000i\nand P2000 SAN Storage ArraysGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# QK703A\nSpare Part# 656102-001\nAssembly Part# 658430-001\nModel# ST33000650SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberST33000650SS\n\n\n\nProducts ID475989\nTypeHard Drive - Hot-Plug\nCapacity3TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed6GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST33000650SS SAS MSA 2 7.2K",null,"g"]
["ST33000650NS","Description:HP 3TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\n512n Midline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 628061-B21\nSpare Part# 628182-001\nAssembly Part# 614827-001\nModel# MB3000GBKAC\nModel# ST33000650NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST33000650NS-SC\n\n\n\nProducts ID1472830\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity3000GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST33000650NS SATA SC 7.2K",null,"g"]
["ST3250624AS","Description:HP 250GB 1.5G 7.2K RPM 3.5-inch HotPlug SATA DriveFor HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349239-B21\nSpare Part# 397553-001\nAssembly Part# 352561-001\nAssembly Part# 353044-001\nAssembly Part# 391335-002\nAssembly Part# 391335-004\nAssembly Part# 397377-004\nAssembly Part# 407525-003\nAssembly Part# 431689-001\nAssembly Part# 432337-001\nAssembly Part# 454141-001\nModel# GB0250C8045\nModel# 6L250S0\nModel# 7L250S0\nModel# ST3250624AS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3250624AS\n\n\n\nProducts ID461852\nTypeHardDrive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity250GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time10ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3250624AS SATA 7.2K",null,"g"]
["ST3250620NS","Description:250GB 3.5-inch SATA 1.5Gb/s 7.2K NHP Hard DriveGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 411276-B21\nSmartBuy Part# 411276-S21\nSpare Part# 399969-001\nAssembly Part# 432337-001\nModel# ST3250620NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThis HP 250GB 7.2K RPM NHP  3.5 Hard Disk Drive is SMART capable and offers data integrity along with the lowest cost per GB targeted for non-mission critical applications with low workloads of 50% or less. SMART stands for Self Monitoring Analysis and Reporting Technology. First developed at HP  it detects possible hard disk failure before it occurs  allowing replacement of the component before failure occurs. \n\nSpecifications:\nCategoryProliant Hard Drive\nSub-Category7.2K\nGenerationSATA NHP HDD\nPart NumberST3250620NS\n\n\n\nProducts ID1462001\nConnector TypeSATA 1.5GB/s\nConnectorSerial ATA 7-pin\nTarget UseServer\nForm Factor3.5 inches\nEnclosure TypeInternal\nAverage Seek Time10ms\nData Transfer Rate1.5GB/s\nHard Drive Capacity250GB\n \nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3250620NS SATA NHP HDD 7.2K",null,"g"]
["ST32000644NS","Description:HP MSA/MSA2 2TB 3.5-inch LFF SATA 3Gb/s 7.2K\nDual Port (DP) MidLine (MDL) Hot-Plug Hard Drive\nIn HP Hot-Plug MSA/MSA2 Hard Drive tray (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AW556A\nSpare Part# 601778-001\nAssembly Part# 507631-003\nAssembly Part# 599690-003\nModel# ST32000644NS\nNote:For use only in HP StorageWorks SystemsModular Smart Array MSA G1 MSA G2 and P2000 Systems only.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SATA disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SATA interposers attached to the back. The SATA interposers have active logic on them that will convert a single-ported SATA disk module into a dual-ported disk module. If you look closely - you will see a MULTIPLEXER chip on the interposer which is responsible for this function. Even though the SCA-40 connector is reminiscent of a connector on a Fibre Channel disk drive - no SATA-FC bridge chip exists on this interposer.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSATA MSA2\nPart NumberST32000644NS\n\n\n\nProducts ID462080\nCapacity2TB\nInterfaceSerial ATA\nEnclosureInternal\nHDD Form Factor3.5 inches\nSpindle Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time9ms \nAverage Latency4.17ms \n \nHot SwapYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST32000644NS SATA MSA2 7.2K",null,"g"]
["ST32000444SS","Description:HP 2TB 3.5-inch LFF SAS   6Gb/s  7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) LFF SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SAS Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)Option Part# 652757-B21Spare Part# 653948-001Assembly Part# 507613-002Assembly Part# 638521-001Assembly Part# 649327-002Assembly Part# 625030-002Assembly Part# 649327-002Assembly Part# 507613-002Model# MB2000FAMYVModel# MB2000FBUCLModel# MB2000FBZPNModel# MB2000FCQPFModel# ST2000NM0001Model# ST32000444SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberST32000444SS-SC\n\n\n\nProducts ID472698\nCapacity2TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST32000444SS SAS SC 7.2K",null,"g"]
["ST318438LW","Description:Seagate 18.4GB Ultra160 3.5-inch SCSI Hot-Plug 7.2K Hard Drive\nPart Number(s):\nPart# ST318438LW\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSeagate Hard Drives undergo an intense qualification process that eliminates data integrity problems firmware and O/S incompatibilities and other causes of data corruption or premature failure. Seagate Hard Drives are specifically designed and tested for flawless operation in your equipment.\n\nSpecifications:\nCategorySeagate HardDrive\nSub-CategoryU160\nGeneration7.2K\nPart NumberST318438LW\n\n\n\nProducts ID491796\nHot Swap TrayNot Included\nCapacity18.4GB\nHeight1.0 inch/2.54cm\nWidth4.0 inch/10.16cm\nInterfaceUltra SCSI Wide\nData Transfer Rate160MB/s",null,"g"]
["ST318406LC","Description:Seagate 18.2GB Ultra160 3.5-inch SCSI\nHot-Plug 10K 80-pin Hard DrivePart Number(s)Seagate Part# ST318406LC\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryHard Drive\nSub-Category10K\nGenerationUltra160\nPart NumberST318406LC\nProducts ID1144125",null,"g"]
["ST318404LC","Description:Seagate 18.4GB internal hard drive 3.5-inch - Ultra160 SCSI 10KPart# ST318404LC\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategorySeagate HardDrive\nSub-CategoryU160\nGeneration10K\nPart NumberST318404LC\nProducts ID144223",null,"g"]
["ST3160815A","Description:160GB ATA/100 7.2K 3.5-inch Hard Drive Part Number(s)\nOption Part# 366486-B21\nSpare Part# 326510-001\nAssembly Part# 439944-002\nModel# ST3160815A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  ATA 100 Hard Drives offering data integrity and availability in a non-pluggable model. HP 7200 rpm Hard Drives provide entry-level performance for the Proliant DL320  DL320 G2  ML310  ML330e and ML330 G2 servers. All HP Hard Drives pass a rigorous qualification process  which ensures that every HP drive is proven to perform in your Proliant server or workstation. Before final certification all HP Parallel-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant\nSub-CategoryHard Drive\nGenerationATA\nPart NumberST3160815A\n\n\n\nProducts ID462154\nTypeHard Drive - Internal\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeATA - 100\nConnector40 pin IDC\nData Transfer Rate100MB/s\nAverage Seek Time10ms\nSpindle Speed7200RPM",null,"g"]
["ST3160812AS","Description:160GB Hot-Plug SATA 1.5GB/s Hard Drive 7200 RPM 3.5-inch form factor 1.0 inch highIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 349238-B21\nSpare Part# 399968-001\nAssembly Part#391334-002\nAssembly Part# 391334-004\nAssembly Part# 440300-002\nAssembly Part# 407525-002\nModel# 6L160M0\nModel# FB160C4081\nModel# ST3160812AS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberST3160812AS\n\n\n\nProducts ID461855\nTypeHard Drive - Hot-Swap\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeSerial ATA-150\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate150MB/s\nAverage Seek Time9ms\nSpindle Speed7200RPM\n \nDimensions (WxH)4 in x 1 in\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST3160812AS SATA 7.2K",null,"g"]
["ST3160021A","Description:160GB ATA/100 7.2K 3.5-inch Hard Drive Part Number(s)\nOption Part# 366486-B21\nSpare Part# 326510-001\nAssembly Part# 320143-001\nModel# ST3160021A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nA variety of tested  HP -qualified  SMART capable  ATA 100 Hard Drives offering data integrity and availability in a non-pluggable model. HP 7200 rpm Hard Drives provide entry-level performance for the Proliant DL320  DL320 G2  ML310  ML330e and ML330 G2 servers. All HP Hard Drives pass a rigorous qualification process  which ensures that every HP drive is proven to perform in your Proliant server or workstation. Before final certification all HP Parallel-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager. \n\nSpecifications:\nCategoryProliant\nSub-CategoryHard Drive\nGenerationATA\nPart NumberST3160021A\n\n\n\nProducts ID1462150\nTypeHard Drive - Internal\nForm Factor3.5 inches x 1/3H\nCapacity160GB\nInterface TypeATA - 100\nConnector40 pin IDC\nData Transfer Rate100MB/s\nAverage Seek Time10ms\nSpindle Speed7200RPM",null,"g"]
["ST3146707LC","Description:146GB Ultra 320 (U320) 3.5-inch SCSI Hot-Plug 10K 80-pin Hard DriveGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)Manufacturer Part# ST3146707LC\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe Cheetah 10K lowers cost of ownership with the industry's highest reliability  designed for full duty cycle applications  Seagate-exclusive Background Media Scan  enhanced Error Correction Code; and low power and cooling requirements. The Cheetah 10K comes with Ultra320 SCSI or 2 Gbit/sec Fiber Channel interfaces.\n\nSpecifications:\nCategorySeagate HardDrive\nSub-Category10K\nGenerationUltra320\nPart NumberST3146707LC\n\n\n\nProducts ID144224\nHot Swap TrayNot Included\nCapacity146GB\nHeight1.0 inch/2.54 cm\nWidth4.0 inch/10.16 cm\nInterfaceUltra320 SCSI\nData Transfer Rate320MB/s\nSeek TimeSingle Track 0.55ms\nSeek TimeAverage 4.9ms\n \nSeek TimeFull Stroke 10.0ms\nRotational Speed10K\n \nBytes/Sector512\nManufacturerSeagate\n \nApplicationServer Storage\nBackward CompatabilityU2 and U3 Speeds\n \nPre-Failure WarrantyYes\nData Storage Device TypeSAS ( Server Attached Storage)\n \n \nHard Drive Device TypeHard Drive for Server/Storage Unit",null,"g"]
["ST31000524NS","Description:HP MSA/MSA2 1TB 3.5-inch LFF SATA 3Gb/s 7.2K\nDual Port (DP) MidLine (MDL) Hot-Plug Hard Drive\nIn HP Hot-Plug MSA/MSA2 Hard Drive tray (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)Option Part# AJ740A\nOption Part# AJ740B\nSpare Part# 480942-001\nSpare Part# 480942-002\nAssembly Part# 481282-001\nModel# ST31000340NS\nModel# ST31000524NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SATA disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SATA interposers attached to the back. The SATA interposers have active logic on them that will convert a single-ported SATA disk module into a dual-ported disk module. If you look closely - you will see a MULTIPLEXER chip on the interposer which is responsible for this function. Even though the SCA-40 connector is reminiscent of a connector on a Fibre Channel disk drive - no SATA-FC bridge chip exists on this interposer.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSATA MSA2\nPart NumberST31000524NS\n\n\n\nProducts ID200356\nCapacity1TB\nInterfaceSerial ATA\nEnclosureInternal\nHDD Form Factor3.5 inches\nSpindle Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time9ms \nAverage Latency4.17ms \n \nHot SwapYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST31000524NS SATA MSA2 7.2K",null,"g"]
["ST31000424SS","Description:HP 1TB 3.5-inch LFF SAS   6Gb/s  7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) LFF SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SAS Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 652753-B21\nSpare Part# 653947-001\nAssembly Part# 507613-001\nModel# ST31000424SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberST31000424SS-SC\n\n\n\nProducts ID472718\nCapacity1TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST31000424SS SAS SC 7.2K",null,"g"]
["ST31000340NS","Description:HP MSA/MSA2 1TB 3.5-inch LFF SATA 3Gb/s 7.2K\nDual Port (DP) MidLine (MDL) Hot-Plug Hard Drive\nIn HP Hot-Plug MSA/MSA2 Hard Drive tray (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)Option Part# AJ740AOption Part# AJ740BSpare Part# 480942-001Spare Part# 480942-002Assembly Part# 481282-001Model# ST31000340NSModel# ST31000524NS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SATA disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SATA interposers attached to the back. The SATA interposers have active logic on them that will convert a single-ported SATA disk module into a dual-ported disk module. If you look closely - you will see a MULTIPLEXER chip on the interposer which is responsible for this function. Even though the SCA-40 connector is reminiscent of a connector on a Fibre Channel disk drive - no SATA-FC bridge chip exists on this interposer.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSATA MSA2\nPart NumberST31000340NS\n\n\n\nProducts ID1200352\nCapacity1TB\nInterfaceSerial ATA\nEnclosureInternal\nHDD Form Factor3.5 inches\nSpindle Speed7200RPM\nData Transfer Rate300MB/s\nAverage Seek Time9ms \nAverage Latency4.17ms \n \nHot SwapYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST31000340NS SATA MSA2 7.2K",null,"g"]
["ST2000NX0273","Description:HP 2TB 2.5-inch SFF SAS 12Gb/s 7.2K RPM\n512e Midline (MDL) Digitally Signed (DS) Hot-Plug Hard Drive\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)Genuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 765466-B21\nSpare Part# 765873-001\nAssembly Part# 765452-002\nGPN# 765470-004\nModel# MM2000JEFRC\nSeagate Part# ST2000NX0273\nSmartBuy Part# 765466-S21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP SAS Hard Drive delivers high reliability for mission critical applications. Robust SAS interface (dual port - full duplex) for increased performance. HP Smart Carrier for HP Proliant Servers (both Gen8 and Gen9 are supported). They are ideal for transaction processing - database applications - analytics - high-performance computing and business applications. The 512e Advance Format Drive is ideal for 4KiB aligned operating systems and applications. They also support legacy 512K native applications.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberST2000NX0273\n\n\n\nProducts ID1478197\nTypeHard Drive - Hot-Swap\nCapacity2TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST2000NX0273 SAS SC 7.2K",null,"g"]
["ST2000NM0063","Description:HP 2TB 3.5-inch Serial Attached SCSI (SAS) LFF 6Gb/sMidline (MDL) Self-Encrypted Hot-Plug 7.2K MSA Hard Drivein HP MSA drive tray with interposer connector (as pictured )For HP MSA1040 MSA2040 MSA2050 MSA2052 MSA2000 MSA2000i\nand P2000 SAN Storage ArraysGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# C8R22A\nSpare Part# 717872-001\nAssembly Part# 757569-001\nModel# ST2000NM0063\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA\nPart NumberST2000NM0063\n\n\n\nProducts ID492441\nTypeHard Drive - Hot-Plug\nCapacity2TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nSpeed6GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST2000NM0063 SAS MSA 7.2K",null,"g"]
["ST2000NM0011","Description:HP 2TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\n512n Midline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 658079-B21\nSpare Part# 658102-001\nAssembly Part# 638519-002\nAssembly Part# 658084-003\nModel# MB2000GBUPB\nModel# MB2000GCEHK\nModel# ST2000NM0011\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less. HP SATA Hard Drives are available in both Large Form Factor (LFF) 3.5-inch and Small Form Factor (SFF) 2.5-inch. \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST2000NM0011-SC\n\n\n\nProducts ID1472878\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity2000GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST2000NM0011 SATA SC 7.2K",null,"g"]
["ST2000NM0001","Description:HP P2000 2TB 3.5-inch Serial Attached SCSI (SAS) LFF 6Gb/sDual Port Midline (MDL) Hot-Plug 7.2K MSA2 Hard Drive in HP MSA/MSA2 drive tray with interposer connector (as pictured )In HP Hot-Plug MSA Hard Drive Tray (as pictured)For HP MSA1040 MSA2040 MSA2050 MSA2052 MSA2000 MSA2000i\nand P2000 SAN Storage ArraysGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# AW555A\nSpare Part# 605475-001\nAssembly Part# 604091-001\nSeagate Part# ST2000NM0001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000 / MSA2000i and P2000 controller enclosures accept unique HP SAS2.5-inch SFF and 3.5-inch LFF  Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 3.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000 / MSA2000i or P2000 series SAN Storage Array with 3.5-inch LFF drive bays. This hard drive will come with the correct firmware for these systems.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberST2000NM0001\n\n\n\nProducts ID1475093\nTypeHard Drive - Hot-Plug\nCapacity2TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed6GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST2000NM0001 SAS MSA 2 7.2K",null,"g"]
["ST173404LCV","Description:ST173404LCV 73GB 10K RPM Ultra SCSI Hard DriveGenuine HP serial number and firmwarePart Number(s)HP Part# ST173404LCV\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryHP Hard Drive\nSub-Category\nGeneration\nPart NumberST173404LCV\nProducts ID144254",null,"g"]
["ST12000NM0038","Description:HP MSA/MSA2 12TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\n512e Dual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# Q2R42A\nSpare Part# P00442-001\nModel# HUH721212AL5204\nModel# ST12000NM0038\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberST12000NM0038\n\n\n\nProducts ID1737620\nTypeHard Drive - Hot-Plug\nCapacity12TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST12000NM0038 SAS MSA 2 7.2K",null,"g"]
["ST1000NM0011","Description:HP 1TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\n512n Midline (MDL) Hot-Plug Hard Drive\nIn G8 G9 (Gen8 Gen9) SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 Proliant SATA Servers and Storage Arrays\nGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# 657750-B21\nSpare Part# 657739-001\nAssembly Part# 657749-001\nAssembly Part# 658084-002\nModel# MB1000GCEEK\nModel# MB1000GCEHH\nModel# ST1000NM0011\nSmartBuy Part# 657750-S21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Hard Drives are designed for the reliability and larger capacities demanded by today's entry server and external storage environments. HP SATA Midline Hard Drives are designed with economical reliability and performance for external storage backups and archival applications. Midline SATA Hard Drives provide the best price advantage for non-mission critical applications with low workloads of 40% or less.  \n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberST1000NM0011-SC\n\n\n\nProducts ID472610\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity1000GB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nNative Command QueuingSupported\n \nBytes/Sector512\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST1000NM0011 SATA SC 7.2K",null,"g"]
["ST10000NM0528","Description:HP MSA/MSA2 10TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\n512e Dual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# P9M82A\nSpare Part# 868230-001\nAssembly Part# 868151-002\nModel# HUH721010AL5204\nModel# ST10000NM0528\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberST10000NM0528\n\n\n\nProducts ID737628\nTypeHard Drive - Hot-Plug\nCapacity10TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# ST10000NM0528 SAS MSA 2 7.2K",null,"g"]
["SSDSC2BA400G3P","Description:HP G8 G9 400GB 2.5-inch Small Form Factor SFF Pluggable Mainstream Endurance (ME) Serial ATA (SATA) 6Gb/s Solid State Drive (SSD)Enterprise Mainstream (EM) Solid State DriveIn HP 2.5-inch G8 G9 Hot-Plug Solid State DriveSmartDrive Carrier (SC) (as pictured)Genuine HP serial number and SSD firmwareGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# 691866-B21\nSpare Part# 692166-001\nAssembly Part# 691842-003\nModel# MK0400GCTZA\nModel# SSDSC2BA400G3P\n\n  \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA SC SSD\nPart NumberSSDSC2BA400G3P\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID479990\nTypeSolid State Drive\nSmall Form Factor2.5 inches\nCapacity400GB\nInterface TypeSerial ATA\nData Transfer Rate6G = 6Gb/sec\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SSDSC2BA400G3P SATA SC SSD Solid State Drive",null,"g"]
["SR2SS","Description:HP Intel® Xeon® E7-8890v4 DL580 G9(2.2GHz/24-core/60MB/165W)Processor KitPart Number(s)\nManufacturer Part# SR2SS\n\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# SR2SS\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSolve your mission-critical IT challenges of managing and keeping secure the capabilities and data crucial to your business with a powerful and reliable Intel Xeon processor server. These top-of-the-line processors deliver performance that is ideal for your most data-demanding workloads with improved scalability and increased memory and I/O capacity  allowing you to handily adapt to changes in short-term business demands and address requirements for longer-term business growth. These advanced reliability and security features work to maintain data integrity  accelerate encrypted transactions  and maximize the availability of mission-critical applications. The powerful and reliable Intel Xeon processor servers provide flexibility for your business critical solutions.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG9\nPart NumberSR2SS\n\n\n\nProducts ID490023\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTetracosa-Core\nProcessor Qty1\nClock Speed2.2GHz\nQuickPath Interconnect9.6GT/s\nL2 Cache6MB\nL3 Cache60MB\n \n64-bit ProcessingYes\nProcess Technology14nm\n \nProcessor SocketSocket R LGA-2011\nThermal Design Power165W\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SR2SS G9 Intel Xeon",null,"g"]
["SDX500C","Description:Sony 50/100GB AIT-2 SCSI LVDInternal Carbon Tape Library DrivePart Number(s)\nPart# SDX500C\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe explosive growth of computer disk capacity  networks and database applications has driven a huge demand for data storage products. And tape drives  due to their low cost per megabyte  are the solution of choice for regular data backup and storage. But as the speed at which information is created continues to skyrocket  traditional tape backup solutions are hard-pressed to keep up. For organizations with data-intensive applications and large information storage requirements  the problem is even more critical-as the volume of information grows  the time and cost required to safely back up that data also increases. These organizations need reliable  high-performance  high-capacity storage solutions that can keep pace with their businesses.??Sony's Advanced Intelligent Tape (AIT) technology is the latest in a long line of innovative tape solutions developed and brought to market by Sony.\n\nSpecifications:\nCategorySony\nSub-CategoryTapeDrive\nGeneration50/100GB\nPart NumberSDX500C\n\n\n\nProducts ID142428\nTape TypeAIT\nNative Capacity50GB\nInterface TypeSCSI\nEnclosure TypeInternal\nNative Data Transfer Rate6MBps\nCompressed Capacity100GB\nData Transfer Rate - Compressed12MBps\nForm Factor3.5 inches x 1/3H\n \nPlatformPC\nDimensions (HxWxD)1.62 in x 4.02 in x 6.11 in\n \nWeight1.76 lbs",null,"g"]
["SDX-400V","Description:Sony AIT1 35/70GB Internal LVD Tape DrivePart Number(s)\nSony Part# SDX-400V\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nAs data protection and high availability have become increasingly important, customers are demanding solid  uninterrupted performance. Continuous development and enhancement of high-performance software applications and operating systems is driving the need for secure backup solutions. TapeDrive customers can be assured that all of their backup needs will be met. The above issues will be addressed  and they will have equipment manufactured to the highest quality standards and subjected to the most rigorous testing procedures that only genuine components will realize.\n\nSpecifications:\nCategorySony\nSub-CategoryTape Drive\nGeneration35/70GB\nPart NumberSDX-400V\n\n\n\nProducts ID458891\nTape TypeAIT1\nNative Capacity35GB\nEnclosure TypeInternal\nCompressed Capacity91GB\nSCSI Signaling TypeLow Voltage Differential (LVD)",null,"g"]
["SB234CX","Description:HP 450GB 15K 3.5-inch FC for EVA M5314 Enclosure40 pin 2/4 Gb/s HotSwap FC-AL DriveGenuine HP Serial number and firmwarePart Number(s)\nOption Part# AG804A\nOption Part# AG804B\nOption Part# AG804-64201\nOption Part# AN595A\nOption Part# AN596A\nOption Part# SB234AX\nOption Part# SB234BX\nOption Part# SB234CX\nSpare Part# 454415-001\nAssembly Part# 495277-005\nModel# BF450DAJZR\n\nNote: Model/Assembly numbers are used in multiple types of EVA Systems because they only represent the bare drive.  Please select the correct option part number in order to get the correct enclosure and drive as a kit.\n\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nCompaq/HP  FCAL Hard Drives are provided with the speed  reliability and functionality needed for today's StorageWorks systems. All Compaq/HP  Hard Drives are designed and tested for compatibility and interoperability in the systems for which they are intended in order to provide the immediate  flawless integration expected from Compaq/HP  storage solutions. \n\nSpecifications:\nCategoryStorageworks HDD\nSub-Category15K\nGenerationFibre Channel\nPart NumberSB234CX\n\n\n\nProducts ID1459756\nTypeHard Drive Hot-Swap\nForm Factor3.5 inch x 1 inch Plug-in Module\nCapacity450GB\nInterface TypeFC-AL\nData Transfer Rate2/4Gb/s\nRotational Speed15000RPM\nPins40\nManufacturerHP/Compaq\n \nPre-Failure WarrantyYes\nApplicationEVA M5314 Enclosure\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SB234CX Fibre Channel 15K",null,"g"]
["SB234BX","Description:HP 450GB 15K 3.5-inch FC for EVA M5314 Enclosure40 pin 2/4 Gb/s HotSwap FC-AL DriveGenuine HP Serial number and firmwarePart Number(s)\nOption Part# AG804A\nOption Part# AG804B\nOption Part# AG804-64201\nOption Part# AN595A\nOption Part# AN596A\nOption Part# SB234AX\nOption Part# SB234BX\nOption Part# SB234CX\nSpare Part# 454415-001\nAssembly Part# 495277-005\nModel# BF450DAJZR\n\nNote: Model/Assembly numbers are used in multiple types of EVA Systems because they only represent the bare drive.  Please select the correct option part number in order to get the correct enclosure and drive as a kit.\n\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nCompaq/HP  FCAL Hard Drives are provided with the speed  reliability and functionality needed for today's StorageWorks systems. All Compaq/HP  Hard Drives are designed and tested for compatibility and interoperability in the systems for which they are intended in order to provide the immediate  flawless integration expected from Compaq/HP  storage solutions. \n\nSpecifications:\nCategoryStorageworks HDD\nSub-Category15K\nGenerationFibre Channel\nPart NumberSB234BX\n\n\n\nProducts ID1459755\nTypeHard Drive Hot-Swap\nForm Factor3.5 inch x 1 inch Plug-in Module\nCapacity450GB\nInterface TypeFC-AL\nData Transfer Rate2/4Gb/s\nRotational Speed15000RPM\nPins40\nManufacturerHP/Compaq\n \nPre-Failure WarrantyYes\nApplicationEVA M5314 Enclosure\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SB234BX Fibre Channel 15K",null,"g"]
["SB234AX","Description:HP 450GB 15K 3.5-inch FC for EVA M5314 Enclosure40 pin 2/4 Gb/s HotSwap FC-AL DriveGenuine HP Serial number and firmwarePart Number(s)\nOption Part# AG804A\nOption Part# AG804B\nOption Part# AG804-64201\nOption Part# AN595A\nOption Part# AN596A\nOption Part# SB234AX\nOption Part# SB234BX\nOption Part# SB234CX\nSpare Part# 454415-001\nAssembly Part# 495277-005\nModel# BF450DAJZR\n\nNote: Model/Assembly numbers are used in multiple types of EVA Systems because they only represent the bare drive.  Please select the correct option part number in order to get the correct enclosure and drive as a kit.\n\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nCompaq/HP  FCAL Hard Drives are provided with the speed  reliability and functionality needed for today's StorageWorks systems. All Compaq/HP  Hard Drives are designed and tested for compatibility and interoperability in the systems for which they are intended in order to provide the immediate  flawless integration expected from Compaq/HP  storage solutions. \n\nSpecifications:\nCategoryStorageworks HDD\nSub-Category15K\nGenerationFibre Channel\nPart NumberSB234AX\n\n\n\nProducts ID1459754\nTypeHard Drive Hot-Swap\nForm Factor3.5 inch x 1 inch Plug-in Module\nCapacity450GB\nInterface TypeFC-AL\nData Transfer Rate2/4Gb/s\nRotational Speed15000RPM\nPins40\nManufacturerHP/Compaq\n \nPre-Failure WarrantyYes\nApplicationEVA M5314 Enclosure\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# SB234AX Fibre Channel 15K",null,"g"]
["S0F32A","Description:HP MSA 20TB 7.2K SAS 3.5 12G Midline (MDL) M.2 HDD\nPart Number(s)\nOption Part# S0F32A\nSpare Part# P59819-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberS0F32A\n\n\n\nProducts ID1738337\nCapacity20TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM",null,"g"]
["RAS-2662P","Description:HP 200W Power SupplyMSL5000/6000 LibraryPart Number(s):Assembly Part# RAS-2662PSpare Part# 231668-001\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryPower Supply\nSub-CategoryMSL\nGeneration5000/6000\nPart NumberRAS-2662P\nProducts ID200649",null,"g"]
["R9D18A","Description:Genuine HP Aruba Instant On 10G SFP+ LC SR 300m OM3 MMF Transceiver\nPart Number(s)\nManufacturer Part# R9D18A\nSpare Part# R9D18-61001\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP+\nPart NumberR9D18A\n\n\n\nProducts ID1737975\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP+\nI/O Ports1 x LC 1000Base-SR\nForm FactorPlug-in Module\nData Transfer Rate10000MB/s",null,"g"]
["R9D18-61001","Description:Genuine HP Aruba Instant On 10G SFP+ LC SR 300m OM3 MMF Transceiver\nPart Number(s)\nManufacturer Part# R9D18A\nSpare Part# R9D18-61001\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP+\nPart NumberR9D18-61001\n\n\n\nProducts ID1737976\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP+\nI/O Ports1 x LC 1000Base-SR\nForm FactorPlug-in Module\nData Transfer Rate10000MB/s",null,"g"]
["R9D17A","Description:Genuine HP Aruba 1GB SFP RJ45 T 100m Cat5e Transceiver\nPart Number(s)\nOption Part# R9D17A\nSpare Part# R9D17-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberR9D17A\n\n\n\nProducts ID737965\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP\nCabling Type1000Base-LX\nForm FactorPlug-in Module\nData Transfer Rate1Gb/s",null,"g"]
["R9D17-61001","Description:Genuine HP Aruba 1GB SFP RJ45 T 100m Cat5e Transceiver\nPart Number(s)\nOption Part# R9D17A\nSpare Part# R9D17-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberR9D17-61001\n\n\n\nProducts ID1737966\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP\nCabling Type1000Base-LX\nForm FactorPlug-in Module\nData Transfer Rate1Gb/s",null,"g"]
["R800A001H","Description:HP 800W Flex Slot Platinum Hot-PlugLow Halogen Power Supply KitPart Number(s)\nOption Part# R800A001H\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP Flexible Slot (Flex Slot) Power Supplies share a common electrical and physical design that allows for hot plug - tool-less installation into HP Proliant Gen10 Performance Servers. Flex Slot power supplies are certified for high-efficiency operation and offer multiple power output options - allowing users to right-size a power supply for specific server configurations. This flexibility helps to reduce power waste - lower overall energy costs - and avoid trapped power capacity in the data center.\n\nSpecifications:\nCategoryProliant\nSub-CategoryProliant Power Supply\nGenerationG10\nPart NumberR800A001H\n\n\n\nProducts ID730094\nDevice TypePower Supply\nPower Provided800 Watts\nFanInternal\nManufacturerHewlett Packard\nForm FactorPlug-In Module\nEfficiency96%\nSpecification ComplianceFlex Slot\nVoltage RequiredAC 100-240 VAC\n \nHot PlugYes\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R800A001H G10 Proliant Power Supply",null,"g"]
["R7N78A","Description:HP StoreFabric SN1700E 64Gb Fibre Channel (FC) Adapter CardDual Port (DP) PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# R7N78A\nSpare Part# P43136-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1700E 64Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR7N78A\n\n\n\nProducts ID1735480\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate64Gb\nPortsDual Port",null,"g"]
["R7N77A","Description:HP StoreFabric SN1700E 64Gb Fibre Channel (FC) Adapter CardSingle Port PCI-e Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# R7N77A\n\nSpare Part# P43135-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1700E 64Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR7N77A\n\n\n\nProducts ID1735474\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate64Gb\nPortsSingle Port",null,"g"]
["R7L71A","Description:HP MSA 108TB (18TB x6) 7.2K SAS 3.5 12G MDL HDD (6-pack)\nPart Number(s)\nOption Part# R7L71A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR7L71A\n\n\n\nProducts ID737783\nCapacity18TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R7L71A SAS MSA StorageWorks HardDrive",null,"g"]
["R7L70A","Description:HP MSA/MSA2 18TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA2062 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R7L70A\nSpare Part# P42803-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberR7L70A\n\n\n\nProducts ID736750\nTypeHard Drive - Hot-Plug\nCapacity18TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R7L70A SAS MSA 2 7.2K",null,"g"]
["R6B14A","Description:Genuine HP B-series Short Wave (SW)\nTransceiver Fibre Channel 10GB SFP+\nPart Number(s)\nGenuine HP Part# R6B14A\nGenuine HP Spare Part# P29146-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\n\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP+\nPart NumberR6B14A\n\n\n\nProducts ID738478\nManufacturerHP",null,"g"]
["R6B12A","Description:Genuine HP B-series Short Wave (SW)\nTransceiver Fibre Channel 32GB SFP28\nPart Number(s)\nGenuine HP Part# R6B12A\nGenuine HP Spare Part# P29141-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\n\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP28\nPart NumberR6B12A\n\n\n\nProducts ID738468",null,"g"]
["R5Y70A","Description:HP 1.92TB 2.5-inch Serial ATA (SATA) SFF6Gb/s Mixed-Use (MU)\nNon-Hot-Plug (NHP) Digitally Signed (DS) Solid State Drive\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# R5Y70A \n\n\t\t\t\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySATA\nGenerationSATA NHP SSD\nPart NumberR5Y70A\n\n\n\nProducts ID1702544\nConnector TypeSATA 6GB/s\nHost InterfaceSerial ATA\nTarget UseServer\nForm Factor2.5 inches\nEnclosure TypeInternal\nData Transfer Rate6GB/s\nHard Drive Capacity1.92TB\nSpindle SpeedSolid State\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R5Y70A SATA NHP SSD SATA",null,"g"]
["R5Y69A","Description:HP 960GB 2.5-inch Serial ATA (SATA) SFF6Gb/s Mixed-Use (MU)\nNon-Hot-Plug (NHP) Digitally Signed (DS) Solid State Drive\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# R5Y69A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySATA\nGenerationSATA NHP SSD\nPart NumberR5Y69A\n\n\n\nProducts ID1702872\nConnector TypeSATA 6GB/s\nHost InterfaceSerial ATA\nTarget UseServer\nForm Factor2.5 inches\nEnclosure TypeInternal\nData Transfer Rate6GB/s\nHard Drive Capacity960GB\nSpindle SpeedSolid State\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R5Y69A SATA NHP SSD SATA",null,"g"]
["R5Y68A","Description:HP 480GB 2.5-inch Serial ATA (SATA) SFF6Gb/s Mixed-Use (MU)\nNon-Hot-Plug (NHP) Digitally Signed (DS) Solid State Drive\nGenuine HP serial number and firmware\nGenuine HP Hard DrivePart Number(s)\nOption Part# R5Y68A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySATA\nGenerationSATA NHP SSD\nPart NumberR5Y68A\n\n\n\nProducts ID1702752\nConnector TypeSATA 6GB/s\nHost InterfaceSerial ATA\nTarget UseServer\nForm Factor2.5 inches\nEnclosure TypeInternal\nData Transfer Rate6GB/s\nHard Drive Capacity480GB\nSpindle SpeedSolid State\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R5Y68A SATA NHP SSD SATA",null,"g"]
["R3U73A","Description:HP 96TB (16TB x6) MSA 12G 7.2K\n3.5 512n Midline SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R3U73A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS\nPart NumberR3U73A\n\n\n\nProducts ID737937\nTypeHard Drive - Hot-Swap\nCapacity16TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R3U73A SAS 7.2K",null,"g"]
["R3U72A","Description:HP MSA 16TB 3.5-inch LFF SAS   12Gb/s  7.2K RPM\nDual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R3U72A\nSpare Part# P21581-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA\nPart NumberR3U72A\n\n\n\nProducts ID737757\nTypeHard Drive - Hot-Plug\nCapacity16TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R3U72A SAS MSA 7.2K",null,"g"]
["R3R30A","Description:HP 3.84TB MSA SFF 2.5-inch Serial Attached SCSI(SAS) Read-Intensive (RI) 12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R3R30A\nSpare Part# P19558-001\nModel# KPM51RUG3T84\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR3R30A\n\n\n\nProducts ID734453\nTypeSolid State Drive\nStorage Capacity3.84TB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm FactorInternal\nHot SwapYes",null,"g"]
["R2J63A","Description:HP StoreFabric SN1610E 32Gb Fibre Channel (FC) Adapter CardDual Port (DP) PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# R2J63A\nSpare Part# P14422-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1610Q 32Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR2J63A\n\n\n\nProducts ID1728806\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate32Gb/s\nPortsDual Port",null,"g"]
["R2J62A","Description:HP StoreFabric SN1610E 32Gb Fibre Channel (FC) Adapter CardSingle Port PCI-e Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# R2J62A\nSpare Part# P14421-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1610Q 32Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR2J62A\n\n\n\nProducts ID728804\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate32Gb/s\nPortsSingle Port",null,"g"]
["R2E09A","Description:HP StoreFabric SN1610Q 32Gb Fibre Channel (FC) Adapter CardDual Port (DP) PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# R2E09A\nSpare Part# P14420-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1610Q 32Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR2E09A\n\n\n\nProducts ID1728802\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate32Gb/s\nPortsDual Port",null,"g"]
["R2E08A","Description:HP StoreFabric SN1610Q 32Gb Fibre Channel (FC) Adapter CardSingle Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# R2E08A\nSpare Part# P14419-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE SN1610Q 32Gb Fibre Channel Host Bus Adapter provides significant I/O performance and security benefits to accelerate databases - host more virtual machines - support emerging technologies such as NVMe and reduce total cost of ownership. It delivers better business outcomes across multiple industry verticals that rely on high performance - safe - and reliable storage connectivity for their storage infrastructure.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberR2E08A\n\n\n\nProducts ID728800\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate32Gb/s\nPortsSingle Port",null,"g"]
["R0Z26A","Description:HP Aruba 100G QSFP28 to QSFP28 5m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0Z26A\nSpare Part# R0Z26-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationQSFP28\nPart NumberR0Z26A\n\n\n\nProducts ID736546\nLength 16.40ft. (5m) \nCable Type\tQSFP28\nConnector Type on First EndQSFP28 Network\nConnector Type on Second End\tQSFP28 Network\nData Transfer Rate100Gb/s",null,"g"]
["R0Z26-61001","Description:HP Aruba 100G QSFP28 to QSFP28 5m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0Z26A\nSpare Part# R0Z26-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationQSFP28\nPart NumberR0Z26-61001\n\n\n\nProducts ID1736547\nLength 16.40ft. (5m) \nCable Type\tQSFP28\nConnector Type on First EndQSFP28 Network\nConnector Type on Second End\tQSFP28 Network\nData Transfer Rate100Gb/s",null,"g"]
["R0Z25A","Description:HP Aruba 100G QSFP28 to QSFP28 1m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0Z25A\nSpare Part# R0Z25-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationQSFP28\nPart NumberR0Z25A\n\n\n\nProducts ID736542\nLength 3.28ft. (1m) \nCable Type\tQSFP28\nConnector Type on First EndQSFP28 Network\nConnector Type on Second End\tQSFP28 Network\nData Transfer Rate100Gb/s",null,"g"]
["R0Z25-61001","Description:HP Aruba 100G QSFP28 to QSFP28 1m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0Z25A\nSpare Part# R0Z25-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationQSFP28\nPart NumberR0Z25-61001\n\n\n\nProducts ID1736543\nLength 3.28ft. (1m) \nCable Type\tQSFP28\nConnector Type on First EndQSFP28 Network\nConnector Type on Second End\tQSFP28 Network\nData Transfer Rate100Gb/s",null,"g"]
["R0Z21A","Description:HP Aruba 25G SFP28 to SFP28 15m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0Z21A\nSpare Part# R0Z21-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0Z21A\n\n\n\nProducts ID736529\nLength 49.21ft. (15m) \nConnector Type on First End\tSFP28 Network\nConnector Type on Second End\tSFP28 Network\nData Transfer Rate\t25Gb/s",null,"g"]
["R0Z21-61001","Description:HP Aruba 25G SFP28 to SFP28 15m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0Z21A\nSpare Part# R0Z21-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0Z21-61001\n\n\n\nProducts ID1736530\nLength 49.21ft. (15m) \nConnector Type on First End\tSFP28 Network\nConnector Type on Second End\tSFP28 Network\nData Transfer Rate\t25Gb/s",null,"g"]
["R0Y63A","Description:Genuine HP Aruba 1GB SFP RJ45 T 100m Transceiver\nPart Number(s)\nOption Part# R0Y63A\nSpare Part# P11592-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberR0Y63A\n\n\n\nProducts ID737972\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP\nCabling Type1000Base-LX\nForm FactorPlug-in Module\nData Transfer Rate1Gb/s",null,"g"]
["R0Q72A","Description:HP MSA 84TB (14TB x6) 7.2K SAS 3.5 12G MDL HDD (6-pack)\nPart Number(s)\nOption Part# R0Q72A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q72A\n\n\n\nProducts ID1737777\nCapacity14TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM",null,"g"]
["R0Q71A","Description:HP MSA 72TB (12TB x6) 7.2K SAS 3.5 12G MDL HDD (6-pack)\nPart Number(s)\nOption Part# R0Q71A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q71A\n\n\n\nProducts ID1737778\nCapacity12TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM",null,"g"]
["R0Q70A","Description:HP 60TB (10TB x6) MSA 12G 7.2K\n3.5 512n Midline SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q70A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS\nPart NumberR0Q70A\n\n\n\nProducts ID1737936\nTypeHard Drive - Hot-Swap\nCapacity10TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q70A SAS 7.2K",null,"g"]
["R0Q69A","Description:HP MSA 8TB 7.2K SAS 3.5 12G MDL HDD (6-pack)\nPart Number(s)\nOption Part# R0Q69A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q69A\n\n\n\nProducts ID737779\nCapacity8TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q69A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q67A","Description:HP 14.4TB (2.4 x6) MSA 12G 10K 2.5 SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q67A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0Q67A\n\n\n\nProducts ID737781\nTypeHard Drive - Hot-Swap\nCapacity2.4TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0Q66A","Description:HP 10.8TB (1.8TB x6) MSA 12G 10K 2.5 SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q66A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0Q66A\n\n\n\nProducts ID737785\nTypeHard Drive - Hot-Swap\nCapacity1.8TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0Q65A","Description:HP MSA 7.2-TB (1.2TB x6) 10K SAS 2.5 12G M.2 HDD (6-Pack)Part Number(s)\nOption Part# R0Q65A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\\\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q65A\n\n\n\nProducts ID737755\nCapacity1.2 TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeEnterprise\nInterfaces1 x SAS 12 Gb/s\nDrive Rotational Speed10000 RPM",null,"g"]
["R0Q64A","Description:HP 5.4TB (900GB x6) MSA 12G 15K 2.5 SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q64A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS\nPart NumberR0Q64A\n\n\n\nProducts ID737782\nTypeHard Drive - Hot-Swap\nCapacity900GB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0Q62A","Description:HP MSA 14TB 3.5-inch LFF SAS   12Gb/s  7.2K RPM\nMidline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q62A\nSpare Part# P13252-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA\nPart NumberR0Q62A\n\n\n\nProducts ID1737765\nTypeHard Drive - Hot-Plug\nCapacity14TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q62A SAS MSA 7.2K",null,"g"]
["R0Q61A","Description:HP MSA/MSA2 12TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\nHot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA2060 MSA2062 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q61A\nSpare Part# P13251-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberR0Q61A\n\n\n\nProducts ID1736746\nTypeHard Drive - Hot-Plug\nCapacity12TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q61A SAS MSA 2 7.2K",null,"g"]
["R0Q60A","Description:HP MSA 10TB 7.2K SAS 3.5 12G Midline (MDL) M.2 HDD\nPart Number(s)\nOption Part# R0Q60A\nSpare Part# P13250-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q60A\n\n\n\nProducts ID737736\nCapacity10TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q60A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q59A","Description:HP MSA 8TB 7.2K SAS 3.5 12G Midline (MDL) M.2 HDD\nPart Number(s)\nOption Part# R0Q59A\nSpare Part# P13249-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q59A\n\n\n\nProducts ID737728\nCapacity8TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q59A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q58A","Description:HP MSA 6TB 7.2K SAS 3.5 12G Midline (MDL) M.2 HDD\nPart Number(s)\nOption Part# R0Q58A\nSpare Part# P13248-001\nModel# HUS726T6TAL5204\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q58A\n\n\n\nProducts ID1737871\nCapacity6TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q58A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q57A","Description:HP MSA 2.4TB 2.5-inch SFF SAS 12Gb/s 10K RPM\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q57A\nSpare Part# P13247-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA1060 controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA1060 series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0Q57A\n\n\n\nProducts ID1734457\nTypeHard Drive - Hot-Swap\nCapacity2.4TB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0Q56A","Description:HP MSA 1.8TB 2.5-inch SFF SAS 12Gb/s 10K RPM\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q56A\nSpare Part# P13246-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA1060 controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA1060 series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0Q56A\n\n\n\nProducts ID736951\nTypeHard Drive - Hot-Swap\nCapacity1.8TB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0Q55A","Description:HP MSA 1.2TB 10K SAS 2.5 12G M.2 Enterprise HDDPart Number(s)\nOption Part# R0Q55A\nSpare Part# P13245-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Server Enterprise Hard Drives are ideal for transaction processing database applications Big Data analytics and high-performance computing.\nBroad portfolio of customized solutions provide up to 2.4 TB of storage.\nEfficient drives provide power for space constrained data centers.\nLatest 12G SAS interface for increased performance.\nStable and consistent portfolio of drives offering long life cycles and steady supply.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q55A\n\n\n\nProducts ID1737600\nCapacity1.2TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeEnterprise\nData Transfer Rate12 Gb/sec (external)\nInterfaces1 x SAS 12 Gb/s\nDrive Rotational Speed10000 RPM",null,"g"]
["R0Q54A","Description:HP MSA 600GB 2.5-inch SFF SAS 12Gb/s 10K RPM\nEnterprise (ENT) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray (as pictured)\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q54A\nSpare Part# P13244-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-Category10K\nGenerationSAS MSA\nPart NumberR0Q54A\n\n\n\nProducts ID1737938\nTypeHard Drive - Hot-Swap\nCapacity600GB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nDrive Interface Standard12Gb/s SAS\nForm Factor2.5\" SFF\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q54A SAS MSA 10K",null,"g"]
["R0Q53A","Description:HP MSA 900GB 15K 2.5 SAS 12G Enterprise M.2 HDDPart Number(s)\nOption Part# R0Q53A\nSpare Part# P13243-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q53A\n\n\n\nProducts ID737696\nCapacity900GB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeEnterprise\nData Transfer Rate12 Gb/sec (external)\nDrive Rotational Speed15000 RPM",null,"g"]
["R0Q49A","Description:HP MSA 1.92TB 3.5in SAS 12G Read Intensive (RI) SSD\nGenuine HP serial number and MSA firmware\nGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R0Q49A\nSpare Part# P13239-001\nModel# KPM51RUG1T92\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR0Q49A\n\n\n\nProducts ID737859\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q49A SAS MSA Solid State Drive",null,"g"]
["R0Q47A","Description:HP 1.92TB MSA SFF 2.5-inch Serial Attached SCSI (SAS)Read-Intensive (RI) 12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R0Q47A\nSpare Part# P13237-001\nModel# KPM51RUG1T92\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR0Q47A\n\n\n\nProducts ID1725942\nTypeSolid State Drive\nStorage Capacity1.92TB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm FactorInternal\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q47A SAS MSA Solid State Drive",null,"g"]
["R0Q46A","Description:HP 960GB MSA SFF 2.5-inch Serial Attached SCSI(SAS) Read-Intensive (RI) 12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R0Q46A\nSpare Part# P13236-001\nModel# XS960SE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR0Q46A\n\n\n\nProducts ID1725938\nTypeSolid State Drive\nStorage Capacity960GB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm FactorInternal\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q46A SAS MSA Solid State Drive",null,"g"]
["R0Q38A","Description:HP MSA 1.92TB 3.5in SAS 12G Read Intensive (RI) SSD\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q38A\nSpare Part# P13013-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q38A\n\n\n\nProducts ID737704\nTypeHard Drive - Hot-Plug\nCapacity1.92TB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q38A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q37A","Description:HP MSA 1.92TB 2.5inch SFF SAS 12Gb/sRead Intensive (RI)\nSolid State Drive (SSD)Part Number(s)\nOption Part# R0Q37A\nSpare Part# P13012-001\nModel# XS1920SE70004\nModel# VO001920JWTBL\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Server Read Intensive (RI) Solid State Drives (SSDs) deliver high performance and endurance for applications requiring high random read IOPs performance. HPE (RI) SSDs typically have an endurance of <1 drive writes per day. All HPE SSDs are backed by over 3.35 million hours of testing and qualification ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to your data by providing the assurance that drive firmware comes from a trusted source. The self-describing icons on the HPE Smart Carrier take the guesswork out of a drive’s status and a \"do not remove\" button prevents data loss from human error. You can also monitor the lifespan of your SSD with HPE SmartSSD Wear Gauge compatibility in management tools allowing you to determine if any drives are at risk of failure.\n\nSpecifications:\nCategoryHP\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR0Q37A\n\n\n\nProducts ID1737584\nCapacity1.92TB\nInterfaceSAS\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeRead Intensive\nData Transfer Rate12 Gb/sec (external)\nInterfaces1 x SAS 12 Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q37A SAS MSA Solid State Drive",null,"g"]
["R0Q36A","Description:HP MSA 960GB 3.5in SAS 12G Read Intensive (RI) SSD\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q36A\nSpare Part# P13011-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0Q36A\n\n\n\nProducts ID1737720\nTypeHard Drive - Hot-Plug\nCapacity960GB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q36A SAS MSA StorageWorks HardDrive",null,"g"]
["R0Q35A","Description:HP 960GB MSA SFF 2.5-inch Serial Attached SCSI(SAS) Read-Intensive (RI) 12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# R0Q35A\nSpare Part# P13010-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberR0Q35A\n\n\n\nProducts ID1728288\nTypeSolid State Drive\nStorage Capacity960GB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm FactorInternal\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q35A SAS MSA Solid State Drive",null,"g"]
["R0Q21A","Description:HP MSA 14TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\n512e Dual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0Q21A\nSpare Part# P11785-001\nAssembly Part# P12341-003\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA\nPart NumberR0Q21A\n\n\n\nProducts ID1494809\nTypeHard Drive - Hot-Plug\nCapacity14TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0Q21A SAS MSA 7.2K",null,"g"]
["R0P92A","Description:HP 72TB (12TB x6) MSA 12G 7.2K\n3.5 512n Midline SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P92A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS\nPart NumberR0P92A\n\n\n\nProducts ID1737790\nTypeHard Drive - Hot-Swap\nCapacity12TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0P91A","Description:HP MSA 60TB 7.2K SAS 3.5 12G MDL HDD (6-pack)\nPart Number(s)\nOption Part# R0P91A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0P91A\n\n\n\nProducts ID1737784\nCapacity10TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM",null,"g"]
["R0P90A","Description:HP 48TB (8TB x6) MSA 12G 7.2K\n3.5 512n Midline SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P90A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS\nPart NumberR0P90A\n\n\n\nProducts ID1737789\nTypeHard Drive - Hot-Swap\nCapacity8TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# R0P90A SAS 7.2K",null,"g"]
["R0P89A","Description:HP 900GB x6 MSA 12G 15K 2.5 512n Enterprise SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P89A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS\nPart NumberR0P89A\n\n\n\nProducts ID737788\nTypeHard Drive - Hot-Swap\nCapacity900GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0P88A","Description:HP 3.6TB (600GB x6) MSA 12G 15K\n2.5 512n Enterprise SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P88A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS\nPart NumberR0P88A\n\n\n\nProducts ID1737787\nTypeHard Drive - Hot-Swap\nCapacity600GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nDrive Interface Standard12Gb/s SAS\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0P87A","Description:HP 2.4TB MSA 12G 10K 2.5 SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P87A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0P87A \n\n\n\nProducts ID1737780\nTypeHard Drive - Hot-Swap\nCapacity2.4TB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0P86A","Description:HP MSA 10.8-TB (1.8TB x6) Enterprise 10K SAS 2.5 12G M.2 HDD (6-Pack)\nPart Number(s)\nOption Part# R0P86A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\\\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberR0P86A\n\n\n\nProducts ID1737756\nCapacity1.8TB x6\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor2.5 inches\nWorkload TypeEnterprise\nInterfaces1 x SAS 12 Gb/s\nDrive Rotational Speed10000 RPM",null,"g"]
["R0P85A","Description:HP 7.2TB (1.2TB x6) MSA 12G 10K 2.5 512n SAS HDD (6-pack)\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# R0P85A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category10K\nGenerationSAS\nPart NumberR0P85A\n\n\n\nProducts ID1737786\nTypeHard Drive - Hot-Swap\nCapacity1.2TB x6\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nSpeed12GB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["R0M47A","Description:HP Aruba 50G SFP56 to SFP56 3m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0M47A\nSpare Part# R0M47-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP\nPart NumberR0M47A\n\n\n\nProducts ID738437\nLength 9.84ft. (3m) \nCable Type\tSFP56\nConnector Type on First EndSFP56 Network\nConnector Type on Second End\tSFP56 Network\nData Transfer Rate50Gb/s",null,"g"]
["R0M47-61001","Description:HP Aruba 50G SFP56 to SFP56 3m Direct Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0M47A\nSpare Part# R0M47-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP\nPart NumberR0M47-61001\n\n\n\nProducts ID1738438\nLength 9.84ft. (3m) \nCable Type\tSFP56\nConnector Type on First EndSFP56 Network\nConnector Type on Second End\tSFP56 Network\nData Transfer Rate50Gb/s",null,"g"]
["R0M46A","Description:HP Aruba 50G SFP56 to SFP56 0.65mDirect Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0M46A\nSpare Part# R0M46-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP\nPart NumberR0M46A\n\n\n\nProducts ID1738439\nLength 2.13ft. (0.65m) \nCable Type\tSFP56\nConnector Type on First EndSFP56 Network\nConnector Type on Second End\tSFP56 Network\nData Transfer Rate50Gb/s",null,"g"]
["R0M46-61001","Description:HP Aruba 50G SFP56 to SFP56 0.65mDirect Attach Copper (DAC) Cable\nPart Number(s)\nOption Part# R0M46A\nSpare Part# R0M46-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Direct Attach Cables provide connections to meet the exponential data growth in data centers and cloud-based services.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP\nPart NumberR0M46-61001\n\n\n\nProducts ID738440\nLength 2.13ft. (0.65m) \nCable Type\tSFP56\nConnector Type on First EndSFP56 Network\nConnector Type on Second End\tSFP56 Network\nData Transfer Rate50Gb/s",null,"g"]
["R0M45A","Description:HP Aruba 25G SFP28 to SFP28 7m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0M45A\nSpare Part# R0M45-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0M45A\n\n\n\nProducts ID1736480\nLength 22.97 ft. (7m) \nOperating temperature32ºF to 158ºF (0ºC to 70ºC)  \nOperating relative humidity-40ºF to 185ºF (-40ºC to 85ºC) \nNon-operating/ Storage relative humidity0% to 85%, noncondensing",null,"g"]
["R0M45-61001","Description:HP Aruba 25G SFP28 to SFP28 7m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0M45A\nSpare Part# R0M45-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0M45-61001\n\n\n\nProducts ID1736481\nLength 22.97 ft. (7m) \nOperating temperature32ºF to 158ºF (0ºC to 70ºC)  \nOperating relative humidity-40ºF to 185ºF (-40ºC to 85ºC) \nNon-operating/ Storage relative humidity0% to 85%, noncondensing",null,"g"]
["R0M44A","Description:HP Aruba 25G SFP28 to SFP28 3m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0M44A\nSpare Part# R0M44-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0M44A\n\n\n\nProducts ID736482\nLength 9.84 ft. (3m) \nOperating temperature32ºF to 158ºF (0ºC to 70ºC)  \nOperating relative humidity-40ºF to 185ºF (-40ºC to 85ºC) \nNon-operating/ Storage relative humidity0% to 85%, noncondensing",null,"g"]
["R0M44-61001","Description:HP Aruba 25G SFP28 to SFP28 3m Active Optical Cable (AOC)\nPart Number(s)\nOption Part# R0M44A\nSpare Part# R0M44-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Active Optical Cables (AOCs) provide the bandwidth to meet the exponential data growth in Telco e-Commerce and high performance computing (HPC). The HPE Active Optical Cables (AOCs) are much lighter and consume less power than traditional copper cables. They are ideal cable solutions for high–density data center and high performance computing applications.\n\nSpecifications:\nCategoryHP\nSub-CategoryCable\nGenerationSFP28\nPart NumberR0M44-61001\n\n\n\nProducts ID1736483\nLength 9.84 ft. (3m) \nOperating temperature32ºF to 158ºF (0ºC to 70ºC)  \nOperating relative humidity-40ºF to 185ºF (-40ºC to 85ºC) \nNon-operating/ Storage relative humidity0% to 85%, noncondensing",null,"g"]
["QW990A","Description:HP StorageWorks CN1100R Dual PortConverged Network AdapterPart Number(s)HP Part# QW990A\nSpare Part# 706801-001\nNote:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks Converged Network Adapters (CNAs) are dual port adapters that provide both Ethernet and Fibre Channel (FC) connectivity over 10 GbE using both Fibre Channel over Ethernet (FCoE) and Converged Enhanced Ethernet (CEE) standards. By consolidating Ethernet and FC onto a converged adapter  HP CNAs reduce the number of separate adapters and cables required for your datacenter and also reduce operational  power and cooling costs while preserving existing Ethernet and Fibre Channel infrastructure. HP CNAs have also been thoroughly tested with HP Proliant servers and HP Top of Rack (ToR) switches to ensure an optimal HP FCoE solution for your datacenter.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryEthernet Adapter\nGenerationCN1100R\nPart NumberQW990A\n\n\n\nProducts ID493592\nManufacturerHP StoreFabric\nProduct TypeNetwork Adapter\nPorts/Channels2 x Fibre Channel\nHost InterfacePCI Express 2.0 x8\nData Transfer Rate10 Gbps Ethernet\nExpansion Slots2 x SFP+\nForm FactorFull-height bracket/Low-profile bracket\nPort Speed10 GbE Converged Enhanced Ethernet (CEE)\n \nSlot TypePCIe\n\n \n \n \n \n\n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QW990A CN1100R Ethernet Adapter",null,"g"]
["QW972A","Description:HP StoreFabric SN1000Q\n16Gb Fibre Channel Adapter Card\nDual Port PCI-e Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# QW972A\nSpare Part# 699764-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP StoreFabric SN1000Q 16Gb Host Bus Adapters enable more rapid storage and retrieval of critical information when using high bandwidth cloud applications and storage intensive applications such as backup - database transactions and rich media. The SN1000Q 16Gb HBA is backward compatible with 8 and 4 Gb storage networks and will protect future investments. With the ability to deliver twice the I/O performance of 8 Gb FC HBAs. The SN1000Q takes Storage Networking performance and efficiency to the next level. \n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQW972A\n\n\n\nProducts ID1725530\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card (Low Profile)\nInterface Type3.0 x 4 PCI Express\nData Transfer Rate16Gbps\nPorts2 x Fibre Channel\nExpansion SlotsSFP+",null,"g"]
["QW971A","Description:HP StoreFabric SN1000Q\n16Gb Fibre Channel Adapter Card\nSinlge Port PCI-e Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# QW971A\nSpare Part# 699764-001\nNote:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP StoreFabric SN1000Q 16Gb Host Bus Adapters enable more rapid storage and retrieval of critical information when using high bandwidth cloud applications and storage intensive applications such as backup - database transactions and rich media. The SN1000Q 16Gb HBA is backward compatible with 8 and 4 Gb storage networks and will protect future investments. With the ability to deliver twice the I/O performance of 8 Gb FC HBAs. The SN1000Q takes Storage Networking performance and efficiency to the next level. \n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQW971A\n\n\n\nProducts ID492427\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card (Low Profile)\nInterface Type3.0 x 4 PCI Express\nData Transfer Rate16Gbps\nPorts2 x Fibre Channel\nExpansion SlotsSFP+",null,"g"]
["QW971-60001","Description:HP StoreFabric SN1000Q\n16Gb Fibre Channel Adapter Card\nSingle Port PCI-e Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# QW971-60001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP StoreFabric SN1000Q 16Gb Host Bus Adapters enable more rapid storage and retrieval of critical information when using high bandwidth cloud applications and storage intensive applications such as backup - database transactions and rich media. The SN1000Q 16Gb HBA is backward compatible with 8 and 4 Gb storage networks and will protect future investments. With the ability to deliver twice the I/O performance of 8 Gb FC HBAs. The SN1000Q takes Storage Networking performance and efficiency to the next level. \n\nSpecifications:\nCategoryHost Bus Adapter\nSub-CategoryFibreChannel\nGenerationSN1000Q\nPart NumberQW971-60001\n\n\n\nProducts ID1725524\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card (Low Profile)\nInterface Type3.0 x 4 PCI Express\nData Transfer Rate16Gbps\nPorts2 x Fibre Channel\nExpansion SlotsSFP+",null,"g"]
["QW967A","Description:HP D3700 25-Bay SFF Rack-Mountable Storage Enclosure Part Number(s)HP Part# QW967A\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryHP\nSub-CategoryEncolsure\nGenerationD3700\nPart NumberQW967A\nProducts ID493598",null,"g"]
["QW923A","Description:Genuine HP Short Wave 16Gb/s Fibre Channel\nSFP+ Transceiver Module\nPart Number(s)\nManufacturer Part# QW923A\nSpare Part# 680536-001\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberQW923A\n\n\n\nProducts ID1736445\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP+\nData Link Protocols16Gb Fibre Channel (Short Wave)\nForm FactorPlug-in Module\nData Transfer Rate14.025Gb/s\nProduct Dimensions (WxHxD)4.40 x 2.90 x 6.20in",null,"g"]
["QR500A","Description:HP M6720 3TB 3.5-inch LFF Serial Attached SCSI (SAS)6Gb/s Hot-Plug 7.2K (Nearline) Hard DriveIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)\nPart Number(s)\nOption Part# QR500A\nSpare Part# 697391-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSerial Attached SCSI (SAS) is the logical evolution of SCSI combining its long-established software advantage with the SAS electrical and physical connection.  With enterprise storage requirements escalating and becoming more complex  factors such as larger capacity  greater density  security  scalability and accessibility are more critical than ever.\n\nSpecifications:\nCategory3Par HardDrive\nSub-Category7.2K\nGenerationSAS 3PAR\nPart NumberQR500A\n\n\n\nProducts ID200862\nTypeHard Drive - Hot-Swap\nCapacity3TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nTray Type3PAR\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR500A SAS 3PAR 7.2K",null,"g"]
["QR498A","Description:HP M6710 1TB 2.5-inch Serial AttachedSCSI (SAS) SFF 6Gb/s Hot-Plug 7.2K (Nearline) Hard DriveIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)Part Number(s)\nOption Part# QR498A\nSpare Part# 727397-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSerial Attached SCSI (SAS) is the logical evolution of SCSI combining its long-established software advantage with the SAS electrical and physical connection.  With enterprise storage requirements escalating and becoming more complex  factors such as larger capacity  greater density  security  scalability and accessibility are more critical than ever.\n\nSpecifications:\nCategory3Par HardDrive\nSub-Category7.2K\nGenerationSAS 3PAR\nPart NumberQR498A\n\n\n\nProducts ID1476643\nTypeHard Drive - Hot-Swap\nCapacity1TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nTray Type3PAR\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR498A SAS 3PAR 7.2K",null,"g"]
["QR496A","",null,"g"]
["QR494A","Description:HP M6710 450GB 2.5-inch Serial AttachedSCSI (SAS) SFF 6Gb/s Hot-Plug 10K Hard DriveIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)Part Number(s)\nOption Part# QR494A\nSpare Part# 697388-001\nGPN# 702504-001\nHP PN# 5697-1286\nHitachi Model# HUC109045CSS600\nHitachi P/N# 0B26012\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategory3Par HardDrive\nSub-Category10K\nGenerationM6710 SAS\nPart NumberQR494A\n\n\n\nProducts ID981\nForm FactorSFF\nCapacity450GB\nInterfaceSAS\nEnclosureM6710 - SFF\nDrive Dimensions2.5 inches x 1/3H (Low Profile)\nSpindle Speed10000 RPM\nExternal Data Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\n \nAverage Latency2ms\nInterface (Detailed)SAS-600\n \nHot SwapYes\nMTBF1700000 Hours\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR494A M6710 SAS 10K",null,"g"]
["QR492A","Description:HP M6710 300GB 2.5-inch Serial AttachedSCSI (SAS) SFF 6Gb/s Hot-Plug 15K Hard DriveIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)Part Number(s)\nOption Part# QR492A\nSpare Part# 697387-001\nModel# SYJKT0300GBAS15K\nManufacturer Part# 9SW066-088\nManufacturer Part# 5697-1842\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSerial Attached SCSI (SAS) is the logical evolution of SCSI combining its long-established software advantage with the SAS electrical and physical connection.  With enterprise storage requirements escalating and becoming more complex  factors such as larger capacity  greater density  security  scalability and accessibility are more critical than ever.\n\nSpecifications:\nCategory3Par HardDrive\nSub-Category15K\nGenerationSAS 3PAR\nPart NumberQR492A\n\n\n\nProducts ID1476581\nTypeHard Drive - Hot-Swap\nCapacity300GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nTray Style3PAR\nEnclosure TypeM6710 - 2.5-inch\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR492A SAS 3PAR 15K",null,"g"]
["QR479A","Description:\nHP Enterprise Virtual Array (EVA) 3TB Serial Attached SCSI (SAS)6Gb/s 7.2K 3.5-inch LFF Hot-Plug DriveIn HP SAS EVA Hot-Plug Hard Drive tray (as pictured)For HP P6000 series M6612 EVA enclosures onlyP6000 P6300 P6350 P6500 P6550 with 3.5-inch LFF SAS Drive BaysGenuine HP serial number and EVA 6612 enclosure firmwarePart Number(s)\nOption Part# QR479A\nSpare Part# 687045-001\nAssembly Part# 625030-001\nAssembly Part# 638521-002\nModel# MB3000FBNWV\nModel# MB3000FBUCN\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryP6000 EVA Hard Drive\nSub-Category7.2K\nGenerationSAS\nPart NumberQR479A \n\n\n\nProducts ID1462020\nCapacity3TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureEVA M6612\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200 RPM\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR479A SAS 7.2K",null,"g"]
["QR478A","Description: HP Enterprise Virtual Array (EVA) HP 900GB 2.5-inch Serial Attached SCSI (SAS) SFF 6Gb/s Dual Port Hot-Plug 10K Enterprise Hard DriveIn HP 2.5-inch SFF SAS EVA Hot-Plug Hard Drive tray (as pictured)For HP P6000 series M6625 EVA enclosures onlyP6000 P6300 P6350 P6500 P6550 with 2.5-inch SFF SAS Drive BaysGenuine HP serial number and EVA M6625 enclosure firmware\nPart Number(s)\nOption Part# QR478A\nSpare Part# 665749-001\nAssembly Part# 619286-004-M6625\nModel# EG0900FBLSK-M6625\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nSerial Attached SCSI (SAS) is the logical evolution of SCSI combining its long-established software advantage with the SAS electrical and physical connection.  With enterprise storage requirements escalating and becoming more complex  factors such as larger capacity  greater density  security  scalability and accessibility are more critical than ever.\n\nSpecifications:\nCategoryP6000 EVA Hard Drive\nSub-Category10K\nGenerationSAS\nPart NumberQR478A\n\n\n\nProducts ID474217\nTypeHard Drive - Hot-Swap\nCapacity900GB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nPortsDual Port\nSpeed6GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR478A SAS 10K",null,"g"]
["QR477A","Description: HP Enterprise Virtual Array (EVA) 300GB 2.5-inch Serial Attached SCSI (SAS) SFF 6Gb/s Dual Port Hot-Plug 15K Enterprise Hard DriveIn HP 2.5-inch SFF SAS EVA Hot-Plug Hard Drive tray (as pictured)For HP P6000 series M6625 EVA enclosures onlyP6000 P6300 P6350 P6500 P6550 with 2.5-inch SFF SAS Drive BaysGenuine HP serial number and EVA M6625 enclosure firmwarePart Number(s)\nOption Part# QR477A\nSpare Part# 665750-001\nAssembly Part# 627114-002-M6625\nModel# EH0300FBQDD-M6625\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryP6000 EVA Hard Drive\nSub-Category15K\nGenerationSAS\nPart NumberQR477A\n\n\n\nProducts ID475295\nForm FactorSFF\nCapacity300GB\nInterfaceSAS\nEnclosureEVA M6625\nDrive Dimensions2.5 inches x 1/3H (Low Profile)\nSpindle Speed15000RPM\nExternal Data Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\n \nAverage Latency2ms\nInterface (Detailed)SAS-600\n \nHot SwapYes\nMTBF1700000 Hours\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QR477A SAS 15K",null,"g"]
["QLE2692","Description:HP StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# QLE2692Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1100Q 16Gb Fibre Channel (FC) Adapter Dual Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQLE2692\n\n\n\nProducts ID1725442\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPortsDual Port\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)\n \nExpansion Slots2 (Total) 0 (Free) X SFP+\nInterfaces2 x 16GB FC (Short Wave) -LC Multi-Mode",null,"g"]
["QLE2562","Description:HP StorageWorks 82Q 8GB PCI-e FC HBA Dual Port\nPart Number(s)\nOption Part# QLE2562\nNote:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP 8Gb PCIe Fibre Channel Host Bus Adapters brings datacenter infrastructure components to a higher level of performance and efficiency with the ability to deliver twice the I/O performance of 4Gb HBAs. An 8Gb FC HBA purchased today is backward compatible with 4 and 2 Gb storage networks and will protect future investments. When using storage intensive applications  such as backup/restore  database transactions  virtualization  and rich media  the increased performance of the 8 Gb infrastructure enables more rapid storage and retrieval of critical information.\n\nSpecifications:\nCategoryHP Option Controller\nSub-CategoryHost Bus Adapter\nGeneration82Q\nPart NumberQLE2562\n\n\n\nProducts ID725498\nManufacturerHP\nProduct TypeHost Bus Adapter\nPerformance8GB\nNumber of ChannelsDual Port\nSlot Type SupportedPCI Express 2.0 to Fibre Channel\nPort Speed8GB\nOperating Temperature32° to 131° F (0° to 55° C)\nPCIe ConnectorPCIe x8\n \n \n \n \n \n\n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QLE2562 82Q Host Bus Adapter",null,"g"]
["QK764A","Description: HP Enterprise Virtual Array (EVA) 1TB 2.5-inch Serial Attached SCSI (SAS) SFF 6Gb/s Dual Port Hot-Plug 7.2K Hard DriveIn HP 2.5-inch SFF SAS EVA Hot-Plug Hard Drive tray (as pictured)For HP P6000 series M6625 EVA enclosures onlyP6000 P6300 P6350 P6500 P6550 with 2.5-inch SFF SAS Drive BaysGenuine HP serial number and EVA M6625 enclosure firmwarePart Number(s)\nOption Part# QK764A\nSpare Part# 660678-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryP6000 EVA Hard Drive\nSub-Category7.2K\nGenerationSAS\nPart NumberQK764A\n\n\n\nProducts ID200545\nForm FactorSFF\nCapacity1TB\nInterfaceSAS\nEnclosureEVA M6625\nDrive Dimensions2.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nExternal Data Transfer Rate6G = 6Gb/sec (750 MB/s)\nSeek Time3.5ms\n \nAverage Latency2ms\nInterface (Detailed)SAS-600\n \nHot SwapYes\nMTBF1700000 Hours\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QK764A SAS 7.2K",null,"g"]
["QK735A","Description:HP PremierFlex LC/LC OM4 CablePart Number(s)\nOption Part# QK735A\nSpare Part# 656430-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE's PremierFlex cables use a bendable fiber technology that significantly improves bend performance over existing fiber cables. This, combined with improvements in fiber clarity and bandwidth, allows HPE PremierFlex cables to transmit data over longer distances, at higher rates, with fewer transmission errors.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationFlex Cable\nPart NumberQK735A\n\n\n\nProducts ID729058\nManufacturerHP\nApplication/UsageNetwork Cable\nConnector EndsFiber Optic\nPackaged Quantity1\nCable Length49 ft (15.0m)",null,"g"]
["QK734A","Description:HP Premier Flex Multimode OM4 CablePart Number(s)Manufacturer Part# QK734A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP PremierFlex cables are the addition to the HP fiber optic cable family, offering significantly better bend performance and signal-transmission integrity than existing OM3 and OM2 technologies. Uses bendable fiber technology reduced downtime, troubleshooting, and operation expense OM3+ (3000 MHz-km), multi-mode completely compatible with all OM2 and OM3 installations.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationFlex Cable\nPart NumberQK734A\n\n\n\nProducts ID729059\nManufacturerHP\nApplication/UsageNetwork Cable\nConnector EndsFiber Optic\nPackaged Quantity1\nCable Length16.4 ft (5.0m)",null,"g"]
["QK732A","Description:HP Premier Flex Multimode OM4 CablePart Number(s)Manufacturer Part# QK732A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP PremierFlex cables are the addition to the HP fiber optic cable family, offering significantly better bend performance and signal-transmission integrity than existing OM3 and OM2 technologies. Uses bendable fiber technology reduced downtime, troubleshooting, and operation expense OM3+ (3000 MHz-km), multi-mode completely compatible with all OM2 and OM3 installations.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationFlex Cable\nPart NumberQK732A\n\n\n\nProducts ID729057\nManufacturerHP\nApplication/UsageNetwork Cable\nConnector EndsFiber Optic\nPackaged Quantity1\nCable Length3.28 ft (1.0m)",null,"g"]
["QK724A","Description:Genuine HP B-series Short Wave Transceiver Fibre Channel 16GB FC SFP+\nPart Number(s)\nGenuine HP Part# QK724A\nGenuine HP Spare Part# 656435-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberQK724A\n\n\n\nProducts ID736467\nConnectivity TechnologyWired\nData Link Protocol16Gb Fibre Channel (SW)\nData Transfer Rate14.025 Gb/s\nProduct Dimensions (WxHxD)6.10 x 0.60 x 7.16in",null,"g"]
["QK703A","Description:HP MSA/MSA2 3TB 3.5-inch LFF SAS   6Gb/s  7.2K RPM\nDual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# QK703A\nSpare Part# 656102-001\nAssembly Part# 658430-001\nModel# ST33000650SS\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberQK703A\n\n\n\nProducts ID200215\nTypeHard Drive - Hot-Plug\nCapacity3TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed6GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QK703A SAS MSA 2 7.2K",null,"g"]
["QB576AA","Description:2TB Hot-Plug SATA NHP Hard Drive6Gb/s 7.2K 3.5-inch form factor 1.0 inch highIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nSpare Part# 674961-001\nModel# QB576AA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\nSpecifications:\nCategoryProliant Hard Drive\nSub-Category7.2K\nGenerationSATA NHP\nPart NumberQB576AA\n\n\n\nProducts ID1479947\nForm Factor3.5 inches x 1/3H\nCapacity2TB\nInterface TypeSerial ATA-300\nAverage Seek Time8.5ms\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# QB576AA SATA NHP 7.2K",null,"g"]
["Q9G82A","Description:Genuine HP 40G QSFP+ LC ER4 40km SMF Transceiver\nPart Number(s)\nManufacturer Part# Q9G82A\nSpare Part# Q9G82-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationQSFP+\nPart NumberQ9G82A\n\n\n\nProducts ID1736514\nManufacturerHP\nApplication/UsageData Networking\nInterface QSFP+\nI/O Ports1 x LC 40GBase-ER4\nForm FactorPlug-in Module\nData Transfer Rate40000MB/s\nProduct Dimensions (WxHxD) inches6.6 x 3.5 x 0.9in",null,"g"]
["Q9G82-61001","Description:Genuine HP 40G QSFP+ LC ER4 40km SMF Transceiver\nPart Number(s)\nManufacturer Part# Q9G82A\nSpare Part# Q9G82-61001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationQSFP+\nPart NumberQ9G82-61001\n\n\n\nProducts ID736515\nManufacturerHP\nApplication/UsageData Networking\nInterface QSFP+\nI/O Ports1 x LC 40GBase-ER4\nForm FactorPlug-in Module\nData Transfer Rate40000MB/s\nProduct Dimensions (WxHxD) inches6.6 x 3.5 x 0.9in",null,"g"]
["Q9D46A","Description:HP 1.6TB MSA SFF 2.5-inch Self-Encrypting Drive (SED)\nSerial Attached SCSI (SAS) Mixed-Use (MU)\n12Gb/s Hot-Plug Solid State DriveGenuine HP Serial number and firmwareGenuine HP Certified Solid State DrivePart Number(s)\nOption Part# Q9D46A\nSpare Part# P07045-001\nModel# KPM5WVUG1T60\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP HardDrive\nSub-CategorySolid State Drive\nGenerationSAS MSA\nPart NumberQ9D46A\n\n\n\nProducts ID1737843\nTypeSolid State Drive\nStorage Capacity1.6TB\nInterface TypeSerial Attached SCSI\nDrive Interface12Gb/s SAS\nForm Factor2.5\"\nHot SwapYes\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q9D46A SAS MSA Solid State Drive",null,"g"]
["Q2R42A","Description:HP MSA/MSA2 12TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\n512e Dual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# Q2R42A\nSpare Part# P00442-001\nModel# HUH721212AL5204\nModel# ST12000NM0038\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberQ2R42A\n\n\n\nProducts ID494801\nTypeHard Drive - Hot-Plug\nCapacity12TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q2R42A SAS MSA 2 7.2K",null,"g"]
["Q2R41A","Description:MSA2 2.4TB 2.5-inch Serial Attached SCSI (SAS) SFF 12Gb/sDual Port 512e Enterprise (ENT) Hot-Plug 10K MSA Hard DriveIn HP Hot-Plug MSA Hard Drive tray (as pictured)For HP MSA1040 MSA2040 MSA2050 MSA2052 MSA2000 MSA2000i\nand P2000 SAN Storage ArraysGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# Q2R41A\nSpare Part# P00441-001\nAssembly Part# 876939-002\nModel# EG002400JWJNN\nModel# EG002400JWJNT\nSeagate Model# ST2400MM0129\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000(i) / P2000 controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF  Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000 / MSA2000i or P2000 series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category10K\nGenerationSAS MSA2\nPart NumberQ2R41A\n\n\n\nProducts ID493574\nTypeHard Drive - Hot-Swap\nCapacity2.4TB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q2R41A SAS MSA2 10K",null,"g"]
["Q2429A","Description:HP-4200 LaserJet 110V Maintenance KitFor the HP LJ 4200 110VPart Number(s)Option Part# Q2429A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  printer maintenance kits ensure your HP printer remains in working condition and continues providing your workers with the highest print quality possible.The Kit includes: 110V fuser  rollers (transfer  pick-up and feed)\n\nSpecifications:\nCategoryLaserJet\nSub-CategoryMaitenance Kit\nGenerationLJ-4200\nPart NumberQ2429A\n\n\n\nProducts ID1454498\nTechnologyLaser\nPrint Yield20000 Page\nVoltage110V",null,"g"]
["Q1H47A","Description:HP MSA 900GB 2.5-inch SFF SAS 12Gb/s 15K RPMDual Port (DP) Enterprise (ENT) Hot-Plug Hard DriveIn HP MSA Hard Drive tray (as pictured)\nFor HP MSA1040 Storage Arrays\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# Q1H47A\nSpare Part# 873371-001\nAssembly Part# 867254-003\nModel# EH000900JWCPN\nModel# EH000900JWHPP\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA1040 controller enclosures and expansion enclosures accept unique HP SAS 2.5-inch SFF and 3.5-inch LFF Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA1040 series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS\nPart NumberQ1H47A\n\n\n\nProducts ID737636\nTypeHard Drive - Hot-Swap\nCapacity900GB\nInterface TypeSerial Attached SCSI\nSpindle Speed15000RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q1H47A SAS 15K",null,"g"]
["Q1595A","Description: StorageWorks Ultrium 960 Rack-mount (Carbonite) Single Drive installed in a 3U rack-mount Kit   Option Part# Q1595A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nmountable tape drive enclosure for direct-attach SCSI backup and archiving applications. Because these enclosure use standard internal tape drives  they provide a cost-effective means of mounting tape drives in rack server environments. These enclosure provide customers with scalability  allowing the customer to add drives and migrate to new tape technologies as their capacity and performance needs grow. HP StorageWorks Rack-mount Kits are supported by Proliant and AlphaServer platforms.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration400/800GB\nPart NumberQ1595A\n\n\n\nProducts ID141971\nTape TypeUltrium\nNative Capacity400 GB\nInterface TypeUltra SCSI\nEnclosure TypeInternal\nNative Data Transfer Rate80 Mbps\nCompressed Capacity800 GB\nDaa Transfer Rate - Compressed160 Mbps\nSCSI Signaling TypeLow Voltage Differential (LVD)\n \nDimensions (HxWxD)3.3 in x 5.7 in x 8.2 in",null,"g"]
["Q1587B","Description:HP StoreEver DAT160 SAS 80/160GB Internal Tape DrivePart Number(s)\nOption Part# Q1587B\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreEver DAT160 SAS 80/160GB Internal Tape Drive \n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGenerationG8\nPart NumberQ1587B\n\n\n\nProducts ID491356\nTape TypeDAT160\nNative Storage Capacity80GB\nCompressed Storage Capacity160GB\nInterface Type3GB/s SAS\nBuffer Size16MB\nNative Data Transfer Rate7.01MB/s\nCompressed Data Transfer Rate 14.02MB/s\nForm FactorInternal\n \nDimensions (HxWxD)9.1 inch x 6.3 inch x 9.3 inch\nWeight5 lbs",null,"g"]
["Q1580B","Description:HP StoreEver DAT160 USB 80/160GB Internal Tape DrivePart Number(s)\nOption Part# Q1580B\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreEver DAT160 USB 80/160GB Internal Tape Drive \n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGenerationG8\nPart NumberQ1580B\n\n\n\nProducts ID491363\nTape TypeDAT160\nNative Storage Capacity80GB\nCompressed Storage Capacity160GB\nInterface TypeUSB 2.0\nBuffer Size16MB\nNative Data Transfer Rate7.01MB/s\nCompressed Data Transfer Rate 14.02MB/s\nForm FactorInternal\n \nDimensions (HxWxD)9.1 inch x 6.3 inch x 9.3 inch\nWeight5 lbs",null,"g"]
["Q1567A","Description:\nStorageWorks DAT 72GBx6 Slot LVD DAT\nExternal AutoLoader   Option Part#  Q1567A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks DAT 72x6 Tape Autoloader is an ideal backup solution for small to medium companies with limited IT support or remote sites of larger companies. By reducing administrative tasks  the DAT 72x6 not only simplifies the backup process but reduces the risk of error as well. The autoloader includes a single tape drive inside an enclosure that holds six data cartridges in a removable magazine. With the ability to store up to 72 GB per DAT 72 data cartridge  the DAT 72x6 provides a quick  efficient means for reducing workload. The backup administrator simply loads the magazine with a week's worth of data cartridges  and the autoloader takes care of backup for an entire week. The backup schedule can be customized by the backup application to suit the user's needs.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration216 GB\nPart NumberQ1567A\n\n\n\nProducts ID141970\nTape TypeDAT\nNative Capacity216 GB\nInterface TypeSCSI LVD/SE\nEnclosure TypeExternal\nNative Data Transfer Rate3 Mbps\nSCSI Signaling TypeLow Voltage Differential (LVD)\nCompressed Capacity432 GB\nWeight10.4\n \nPowerAC 120/230V (50/60 Hz)\nDevice TypeTape Autoloader",null,"g"]
["Q1553A","Description:HP StorageWorks DAT 20/40GB Internal Tape DrivePart Number(s)\nOption Part# Q1553A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks DAT40 addresses the evolving backup needs of an exceptionally wide range of organizations and networks. It features a ground-breaking combination of speed and reliability in a cost-effective 40 GB backup for servers and workstations. \n\n\nSpecifications:\nCategoryTape Drive\nSub-CategoryDAT\nGeneration20/40GB\nPart NumberQ1553A\n\n\n\nProducts ID1015392\nTape TypeDAT\nNative Capacity20GB\nInterface TypeSCSI\nEnclosure TypeInternal\nNative Data Transfer Rate3MBps\nCompressed Capacity40GB\nData Transfer Rate - Compressed6MBps\nForm Factor3.5 inch x 1/2H\n \nSCSI Signaling TypeLow Voltage Differential (LVD)\nPlatformPC\n \nDimensions (HxWxD)1.62 in x 5.79 in x 6.36 in\nWeight2.21 lbs",null,"g"]
["Q1546A","Description:StorageWorks DAT 40 DAT Tape Drive   Option Part#  Q1546A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks DAT 40 Tape Drive is an entry level dependable solution for small to medium server storage backup needs as well as enterprise networks.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration20/40 GB\nPart NumberQ1546A\n\n\n\nProducts ID141969\nTape TypeDAT\nNative Capacity20 GB\nNative Data Transfer Rate3 Mbps\nCompressed Capacity40 GB",null,"g"]
["Q1545A","Description:HP StorageWorks LTO Ultrium 215 100/200GB External Tape DrivePart Number(s)Manufacturer Part# Q1545A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\n\n\n \n Main Features • Tape drive • LTO Ultrium 100 GB / 200 GB • SCSI • LVD As the entry point for HP ´s Ultrium tape drive family  the HP StorageWorks Ultrium 215 offers superdrive capacity in a compact half-height form factor that makes it easy to integrate into workstations and servers. An ideal solution for network backup where high capacity and low cost of ownership are critical  the Ultrium 215 stores 200 GB of compressed data on a single tape at up to 54GB per hour. Despite its low cost  the Ultrium 215´s rugged design delivers excellent reliability  even at 100% duty cycles  and includes many of the advanced features of its bigger siblings. The drive employs data rate matching to adjust to the speed of the host  reducing wear and tear on both drive and media and increasing performance  particularly on slower systems. HP One-Button Disaster Recovery takes the worry out of disaster planning - making the Ultrium 215 especially suitable for environments with limited IT support. Whether it´s for a single server or just one part of a backup environment that includes high-performance Ultrium drives  the Ultrium 215 is the ideal match for midrange servers.\n   \n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGeneration100/200GB\nPart NumberQ1545A\n\n\n\nProducts ID142278",null,"g"]
["Q1543A","Description:HP StoreWorks Ultrium 215 LTO Low Voltage Differential (LVD) Internal Tape Drive for Proliant Servers (Carbon) - 5.25in form factor  half heightPart Number(s)\nHP Part# Q1543A\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nAs the entry point for HP 's Ultrium tape drive family  the HP StorageWorks Ultrium 215 tape drive offers superdrive capacity in a compact half-height form factor that makes it easy to integrate into desktop workstations and servers. An ideal solution for network backup where capacity and low cost of ownership are critical  the Ultrium 215 stores 200 GB of compressed data on a single tape at up to 54GB per hour. ??Despite its low cost  the Ultrium 215's rugged design delivers excellent reliability  even at 100% duty cycles  and includes many of the advanced features of its bigger siblings. The drive employs data rate matching to adjust to the speed of the host  reducing wear and tear on both drive and media and increasing performance  particularly on slower systems. HP StorageWorks One-Button Disaster Recovery takes the worry out of disaster planning - making the Ultrium 215 especially suitable for environments with limited IT support.\n\nSpecifications:\nCategoryTape Drive\nSub-CategoryUtrium 215\nGeneration\nPart NumberQ1543A\n\n\n\nProducts ID141639\nTape TypeUltrium\nNative Capacity100GB\nInterface TypeSCSI\nEnclosure TypeInternal\nNative Data Transfer Rate7.5Mbps\nCompressed Capacity200GB\nData Transfer Rate15Mbps\nForm Factor5.25 inch x 1/2H\n \nSCSI Signaling TypeLow Voltage Differential (LVD)\nDimensions(HxWxD)1.62 in x 5.79 in x 8.71 in\n \nWeight3.31 lbs",null,"g"]
["Q1539B","Description: Ultrium 960 External Tape Drive U.S. - English localization   Option Part#  Q1539B \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks Ultrium 960 Tape Drive represents HP 's third-generation of LTO tape drive technology. Positioned as the highest capacity drive in the StorageWorks family  the Ultrium 960 features an 800 GB compressed (2:1) storage capacity using new LTO 3 media. By doubling the capacity of current Ultrium drives  HP customers now require fewer data cartridges to meet their storage needs  significantly reducing their IT costs and increasing their ROI. The Ultrium 960 also features a compressed (2:1) data transfer rate of 160 MB/s. Using a new 16-channel recording head  an Ultra320 SCSI interface  and increases in media tracks and bit density  the HP Ultrium 960 sets a new performance benchmark as the world's fastest tape drive. For customers that continually experience shrinking backup windows  the Ultrium 960 is the ideal direct-attach backup storage solution for enterprise and mid-range server  as well as entry-level Hard Drive arrays.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration\nPart NumberQ1539B\n\n\n\nProducts ID141896\nTape TypeLTO-3\nNative Capacity400 GB\nInterface TypeUltra320 SCSI\nEnclosure TypeExternal\nNative Data Transfer Rate80 Mbps\nCompressed Capacity800 GB\nData Transfer Rate - Compressed160 Mbps\nForm Factor5.25\" x 1H\n \nSCSI Signaling TypeLow Voltage Differential (LVD)\nPlatformPC\n \nDimensions (HxWxD)4.7 in x 8.6 in x 11.7 in\nWeight12.3 lbs",null,"g"]
["Q1539A","Description:Q1539A StorageWorks -  StorageWorks 400/800GBLTO-3 Ultrium 960 External Tape DrivePart Number(s)Option Part# Q1539A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks Ultrium 960 Tape Drive represents HP 's third-generation of LTO tape drive technology. Positioned as the highest capacity drive in the StorageWorks family  the Ultrium 960 features an 800 GB compressed (2:1) storage capacity using new LTO 3 media. By doubling the capacity of current Ultrium drives  HP customers now require fewer data cartridges to meet their storage needs  significantly reducing their IT costs and increasing their ROI. The Ultrium 960 also features a compressed (2:1) data transfer rate of 160 MB/s. Using a new 16-channel recording head  an Ultra320 SCSI interface  and increases in media tracks and bit density  the HP Ultrium 960 sets a new performance benchmark as the world's fastest tape drive. For customers that continually experience shrinking backup windows  the Ultrium 960 is the ideal direct-attach backup storage solution for enterprise and mid-range server  as well as entry-level Hard Drive arrays.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGeneration400/800GB\nPart NumberQ1539A\n\n\n\nProducts ID14096\nTape TypeUltrium\nNative Capacity400GB\nInterface TypeUltra SCSI\nEnclosure TypeExternal\nNative Data Transfer Rate80Mbps\nCompressed Capacity800GB\nData Transfer Rate - Compressed160 Mbps\nSCSI Signaling TypeLow Voltage Differential (LVD)\n \nPlatformPC, Unix, Sun\nDimensions (HxWxD)4.7 in x 8.6 in x 11.7 in\n \nWeight12.3 lbs",null,"g"]
["Q1538A","Description: StorageWorks Ultrium 960400/800GB LTO-3Internal Tape Drive-CarbonOption Part# Q1538ASpare Part# 378463-001 \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks Ultrium 960 Tape Drive represents HP 's third-generation of LTO tape drive technology. Positioned as the highest capacity drive in the StorageWorks family  the Ultrium 960 features an 800 GB compressed (2:1) storage capacity using new LTO 3 media. By doubling the capacity of current Ultrium drives  HP customers now require fewer data cartridges to meet their storage needs  significantly reducing their IT costs and increasing their ROI. The Ultrium 960 also features a compressed (2:1) data transfer rate of 160 MB/s. Using a new 16-channel recording head  an Ultra320 SCSI interface  and increases in media tracks and bit density  the HP Ultrium 960 sets a new performance benchmark as the world's fastest tape drive. For customers that continually experience shrinking backup windows  the Ultrium 960 is the ideal direct-attach backup storage solution for enterprise and mid-range server  as well as entry-level Hard Drive arrays.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGeneration400 GB\nPart NumberQ1538A\n\n\n\nProducts ID141895\nTape TypeUltrium\nnative Capacity400 GB\nInterface TypeUltra SCSI\nEnclosure TypeInternal\nNative Data Transfer Rate80 Mbps\nCompressed Capacity800 GB\nData Transfer Rate - Compressed160 Mbps\nForm Factor5.25\" x 1H\n \nSCSI Signaling TypeLow Voltage Differential (LVD)\nPlatformPC, Unix, Sun\n \nDimensions (HxWxD)3.3 in x 5.7 in x 8 in\nWeight4.9 lbs",null,"g"]
["Q1525A","Description:HP DAT 72GB Internal Tape Drive for ProliantPart Number(s)\nOption Part# Q1525A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks DAT 72 tape drive is the fifth generation of HP 's popular DDS tape format  delivering a capacity of 72 GB on a single HP DDS data cartridge (C8010A). Reinforcing HP 's leadership position in the tape market  it builds on the success of four previous generations of DDS drive technology providing unprecedented levels of capacity  reliability and cost of ownership. The StorageWorks DAT 72 tape drive is the ideal choice for small and medium businesses  remote offices or workgroups. HP 's DDS tape technology has proven itself during more than 12 years of use as one of the most reliable tape technologies on the market today. DAT 72 builds on the strengths and successes of previous generations of DDS drives. The HP StorageWorks DAT 72 tape drive has a mean time between failure (MTBF) rating of 400 000 hours at a 12% percent duty cycle  making it an ideal choice for small and medium businesses. \n\n\nSpecifications:\nCategoryTape Drive\nSub-CategoryDAT\nGeneration72GB\nPart NumberQ1525A\n\n\n\nProducts ID1015391\nDevice TypeTape drive - DAT\nEnclosure TypeInternal\nCapacity36GB (Native) / 72GB (Compressed)\nInterface TypeSCSI LVD\nForm Factor3.5 inches\nData Transfer Rate3MBps (Native) / 6MBps (Compressed)\nAverage Seek / Access Time50 sec\nBuffer Size8MB\n \nRecording StandardDDS-3, DDS-4, DAT 72\nMedia TypeDAT\n \nMedia Included Qty1",null,"g"]
["Q1524B","Description:Storage System : StorageWorks DAT 72 Array Module (Carbon) - Offline Hot-Swap Drive for Tape Array 5300Part Number(s)Hewlett-Packard Part# Q1524B\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberQ1524B\nProducts ID142279",null,"g"]
["Q1523A","Description: Q1523A  Strgwrks DAT72E 36/72GB External   Option Part#  Q1523A \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nAs data protection and high availability have become increasingly important, customers are demanding solid  uninterrupted performance. Continuous development and enhancement of high-performance software applications and operating systems is driving the need for secure backup solutions. Compaq TapeDrive customers can be assured that all of their backup needs will be met. The above issues will be addressed  and they will have equipment manufactured to the highest quality standards and subjected to the most rigorous testing procedures that only genuine components will realize.\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberQ1523A\n\n\n\nProducts ID141968",null,"g"]
["Q1522B","Description:HP StorageWorks DAT 72 Internal DDS5 Tape DriveOption Part# Q1522B\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe industry leading HP StorageWorks DAT 72 SCSI Tape Drive provides an optimum balance of dependable backup capacity and low cost of ownership for small and medium businesses  remote offices  and workgroups. The DAT 72 delivers a capacity of 72 GB on a single data cartridge and a transfer rate of 23 GB/hr (assuming a 2:1 compression ratio). This drive reads and writes DAT 72  DDS-4  and DDS-3 formats  making it the perfect upgrade from earlier generations of DDS.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTapeDrive\nGeneration36/72GB\nPart NumberQ1522B\n\n\n\nProducts ID141990\nTape TypeDAT\nNative Capacity36GB\nInterface TypeUltra3 SCSI 160\nEnclosure TypeInternal\nNative Data Transfer Rate3.2 Mbps\nCompressed Capacity72GB\nData Transfer Rate - Compressed6.4 Mbps\nForm Factor5.25\" x 1/2H\n \nSCSI Signaling TypeDifferential (HVD)\nPlatformSun, PC, Unix\n \nDimensions (HxWxD)1.6 in x 5.7 in x 6.1 in\nWeight2.1 lbs",null,"g"]
["Q1519A","Description:HP StorageWorks Ultrium 460 Tape Drive for ProLiant  External (Carbon)Part Number(s)Manufacturer Part# Q1519A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP Storageworks Ultrium 460 tape drive is the latest generation of HP Ultrium tape drives  delivering a capacity of 400 GB (assuming 2:1 compression) on a single cartridge. Ultrium 460 Tape Drive builds on the success of the HP Storageworks Ultrium 230 by offering the same broad compatibility  support for one-button disaster recovery  and utilities for manageability. Fully read and write compatible with first-generation tape drives while setting new standards for performance  capacity  and reliablility.\n\nSpecifications:\nCategoryStorageWorks\nSub-CategoryTape Drive\nGenerationUltrium 460\nPart NumberQ1519A\n\n\n\nProducts ID457722\nForm FactorExternal\nInterfaces/PortsLVD - SCSI \nStorage Capacity 200/400 GB\nData Transfer Rate (max.)30/60 MB/s\nDimensions (WxHxD)16.8 in x 5.2 in x 23.0 in",null,"g"]
["Q1516A","Description:HP StorageWorks Ultrium 230 Tape Drive for ProLiant  External (Carbon) Manufacturer Part# Q1516A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP Storageworks Ultrium 230 tape drive is the latest generation of HP Ultrium tape drives. Ultrium 230 Tape Drive builds on the success of the HP Storageworks Ultrium 215 by offering the same broad compatibility  support for one-button disaster recovery  and utilities for manageability. Fully read and write compatible with first-generation tape drives while setting new standards for performance  capacity  and reliablility.\n\nSpecifications:\nCategoryStorageWorks\nSub-CategoryTape Drive\nGenerationUltrium 230\nPart NumberQ1516A\n\n\n\nProducts ID457721\nForm Factor3U\nInterfaces/PortsLVD - SCSI \nStorage Capacity 100/220 GB\nData Transfer Rate (max.)22 MB/s\nDimensions (WxHxD)16.8 in x 5.2 in x 23.0 in",null,"g"]
["Q1512B","Description: \nStorageWorks Ultrium 460 Ultrium Tape Drive   Option Part#  Q1512B \n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StorageWorks Ultrium 460 Tape Drive is the latest generation of HP Ultrium Tape Drives  delivering a capacity of 400 GB (assuming 2: 1 data compression) on a single cartridge. Reinforcing HP 's leadership position in tape  it builds on the success of the HP StorageWorks Ultrium 230 and HP StorageWorks Ultrium 215 drives  offering the same broad compatibility  support for One-Button Disaster Recovery  HP StorageWorks Library and Tape Tools utilities for manageability. With a transfer rate of 60 MB/sec  the Ultrium 460 is the ideal choice for enterprise-class data protection needs  particularly where the backup window is shrinking. The Ultrium 460 Tape Drive is fully read and write compatible with first-generation Ultrium Tape Drives  while setting new standards for performance  capacity and reliability in the superdrive market. As part of the four-generation LTO Ultrium open format  the Ultrium 460 is the best choice for long-term investment protection.\n\nSpecifications:\nCategoryProliant\nSub-CategoryTape Drive\nGeneration200/400GB\nPart NumberQ1512B\n\n\n\nProducts ID141967\nTape TypeUltrium\nNative Capacity200 GB\nInterface TypeSCSI\nNative Data Transfer Rate30 Mbps\nCompressed Capacity400 GB\nSCSI Signaling TypeLow Voltage Differential (LVD)\nPlatformPC",null,"g"]
["Q0V79A","Description:HP NVIDIA Tesla P4 8GB Computational AcceleratorPart Number(s)\nHP Part# Q0V79A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nNVIDIA Accelerators for HP Proliant Servers seamlessly integrate graphics processing unit (GPU) computing with select HP Proliant Server families. Designed for power-efficient - high performance supercomputing - NVIDIA® Accelerators deliver dramatically higher application acceleration than a CPU-only approach for a range of deep learning - scientific - and commercial applications.  The NVIDIA Accelerators for HP Proliant Servers improve computational performance - dramatically reducing the completion time for parallel tasks - offering quicker time to solutions.\n\nSpecifications:\nCategoryProliant\nSub-CategoryAccelerator\nGenerationG10\nPart NumberQ0V79A\n\n\n\nProducts ID1490712\nProduct TypeComputational Accelerator\nStandard Memory8GB\nMemory TechnologyGDDR4\nChipset ManufacturerNVIDIA\nChipset ModelP4\nChipset LineGrid\nChipset SeriesP\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n [ Products Tour ]\n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0V79A G10 Accelerator",null,"g"]
["Q0V78A","Description:HP NVIDIA Quadro P4000 Graphics Accelerator Graphics Card\nPart Number(s)\nHP Part# Q0V78A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nNVIDIA Accelerators for HP Proliant Servers seamlessly integrate graphics processing unit (GPU) computing with select HP Proliant Server families. Designed for power-efficient - high performance supercomputing - NVIDIA® Accelerators deliver dramatically higher application acceleration than a CPU-only approach for a range of deep learning - scientific - and commercial applications.  The NVIDIA Accelerators for HP Proliant Servers improve computational performance - dramatically reducing the completion time for parallel tasks - offering quicker time to solutions.\n\nSpecifications:\nCategoryProliant\nSub-CategoryGraphics Accelerator\nGenerationG10\nPart NumberQ0V78A\n\n\n\nProducts ID1490713\nProduct TypeGraphics Accelerator\n\n\n\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n [ Products Tour ]\n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0V78A G10 Graphics Accelerator",null,"g"]
["Q0V77A","Description:HP NVIDIA Quadro P2000 Graphics AcceleratorPart Number(s)\nHP Part# Q0V77A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nNVIDIA Accelerators for HP Proliant Servers seamlessly integrate graphics processing unit (GPU) computing with select HP Proliant Server families. Designed for power-efficient - high performance supercomputing - NVIDIA® Accelerators deliver dramatically higher application acceleration than a CPU-only approach for a range of deep learning - scientific - and commercial applications.  The NVIDIA Accelerators for HP Proliant Servers improve computational performance - dramatically reducing the completion time for parallel tasks - offering quicker time to solutions.\n\nSpecifications:\nCategoryProliant\nSub-CategoryGraphics Accelerator\nGenerationG10\nPart NumberQ0V77A\n\n\n\nProducts ID1490714\nProduct TypeGraphics Accelerator\n\n\n\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n [ Products Tour ]\n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0V77A G10 Graphics Accelerator",null,"g"]
["Q0L14A","Description:HP StoreFabric SN1200E 16Gb Fibre Channel (FC) AdapterCard Dual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# Q0L14A\nSpare Part# 870002-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric SN1200E 16Gb Fibre Channel Host Bus Adapters deliver twice the I/O performance of 8Gb Fibre Channel (FC) Host Bus Adapters (HBAs) while being backward compatible with 8 and 4Gb FC environment. When using storage intensive applications like backup/restore - database transactions - virtualization and rich media - the improved I/O performance enables faster storage and retrieval of data. The HP StoreFabric SN1200E 16Gb Host Bus Adapters provides near limitless scalability to support increased virtual machine (VM) density with 2x more on-chip resources and bandwidth than previous offerings.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQ0L14A\n\n\n\nProducts ID492468\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 x8\nData Transfer Rate16Gb/s\nPortsDual Port\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n  [ Manufacturers Specs ]\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0L14A FibreChannel Host Bus Adapter",null,"g"]
["Q0L13A","Description:HP StoreFabric SN1200E 16Gb Fibre Channel (FC) Adapter CardSingle Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# Q0L13A\nSpare Part# 870001-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric SN1200E 16Gb Fibre Channel Host Bus Adapters deliver twice the I/O performance of 8Gb Fibre Channel (FC) Host Bus Adapters (HBAs) while being backward compatible with 8 and 4Gb FC environment. When using storage intensive applications like backup/restore - database transactions - virtualization and rich media - the improved I/O performance enables faster storage and retrieval of data. The HP StoreFabric SN1200E 16Gb Host Bus Adapters provides near limitless scalability to support increased virtual machine (VM) density with 2x more on-chip resources and bandwidth than previous offerings.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQ0L13A\n\n\n\nProducts ID492466\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 x8\nData Transfer Rate16Gb/s\nPortsSingle Port\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n  [ Manufacturers Specs ]",null,"g"]
["Q0L12A","Description:HP StoreFabric SN1600E 32Gb Fibre Channel (FC) Adapter CardDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# Q0L12A\nSpare Part# 870000-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric 32Gb Fibre Channel (FC) Host Bus Adapters (HBA) are designed to support Proliant Servers with PCI-Express I/O slots to connect to Hewlett Packard Enterprise Storage Arrays using the 32/16/8Gb FC protocol. When using storage intensive applications - such as backup/restore - database transactions - virtualization - and rich media - the increased performance of the 32Gb infrastructure enables rapid storage and retrieval of critical information. Designed for environments with greater virtual machine density and bandwidth requirements - the 32Gb HBAs enable more applications and VMs to run on a single host server and FC port - resulting in reduced cabling and a higher return on IT investment.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQ0L12A\n\n\n\nProducts ID1728121\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 x8\nData Transfer Rate32Gb/s\nPortsDual Port\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0L12A FibreChannel Host Bus Adapter",null,"g"]
["Q0L11A","Description:HP StoreFabric SN1600E 32Gb Fibre Channel (FC) Adapter CardSingle Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# Q0L11A\nSpare Part# 869999-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE StoreFabric SN1600E 32Gb Fibre Channel Host Bus Adapters delivers near limitless scalability to support increased VM density with 2X more on-chip resources and bandwidth than Gen5 Fibre Channel.\n\nImproves the virtual desktop infrastructure (VDI) end-user experience with low latency features providing noticeable improvements during boot storms (degradation of service that occurs when a significant number of end-users boot up within a very narrow time frame and overwhelm the network).\n\nSimplifies management and installation with OneCommand Manager plugin for VMware® vCenter® server.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberQ0L11A\n\n\n\nProducts ID728120\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express\nData Transfer Rate32Gb/s\nPortsSingle Port\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n  [ Manufacturers Specs ]",null,"g"]
["Q0F44A","Description:HP StoreServ 9000 3.84TB 2.5-inch Serial Attached\nSCSI (SAS) FIPS Self-Encrypting Drive (SED)\nSSD 12Gb/s Hot-Plug Hard Drive\nIn HP 3PAR Hot-Plug Hard Drive tray (as pictured)Part Number(s)\nOption Part# Q0F44A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP 3PAR StoreServ Storage is designed to deliver the agility and efficiency demanded by virtual data centers integrating SAP products. All HP 3PAR models are targeted towards the most demanding SAP customers for their SAP production systems and landscapes; they are simple to use - yet powerful - autonomically tiered - and multi-tenant storage arrays. They are supported by a powerful suite of software products that provide ease of management - efficient storage utilization through thin technologies - autonomic storage tiering and leading availability features such as persistent cache and full-mesh interconnect. The features of HP 3PAR StoreServ are ideally suited for integration with SAP systems that rely on a robust - scalable - and efficient storage solution.\n\nSpecifications:\nCategoryDell\nSub-Category3Par HardDrive\nGenerationSAS 3PAR\nPart NumberQ0F44A\n\n\n\nProducts ID1738213\nTypeHard Drive - Hot-Swap\nCapacity3.84TB\nInterface TypeSerial Attached SCSI\nEnclosure Type9000 - 2.5-inch\nTray Type3PAR\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# Q0F44A SAS 3PAR 3Par HardDrive",null,"g"]
["Q0F26A","Description:HP StoreFabric CN1200R 10GB Dual PortConverged Network AdapterPart Number(s)\nHP Part# Q0F26A\nSpare Part# 872527-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric Converged Network Adapters (CNAs) are dual port adapters that provide Ethernet - iSCSI - and Fibre Channel (FC) connectivity over 10 GbE using both Fibre Channel over Ethernet (FCoE) and Converged Enhanced Ethernet (CEE) standards.\n\nSpecifications:\nCategoryHP Controller\nSub-CategoryEthernet Adapter\nGenerationCN1200R\nPart NumberQ0F26A\n\n\n\nProducts ID736411\nManufacturerHP StoreFabric\nDevice TypeNetwork Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 X8\nData Link Protocol10GB CEE, Fibre Channel, FCoE\nData Transfer Rate10GB/s\nPortsDual Port\nConnectivity TechnologyWired\n \nNetwork Transport ProtocoliSCSI",null,"g"]
["Q0F09A","Description:HP StoreFabric CN1300R 10/25GB Dual Port\nConverged Network Adapter\nPart Number(s)\nOption Part# Q0F09A\nSpare Part# 872526-001\nNote:Please confirm \nLow Profile or Full Height \nBracketIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric Converged Network Adapters (CNAs) are dual port adapters that provide Ethernet - iSCSI - and Fibre Channel (FC) connectivity over 10 GbE using both Fibre Channel over Ethernet (FCoE) and Converged Enhanced Ethernet (CEE) standards.\n\nSpecifications:\nCategoryHP Controller\nSub-CategoryEthernet Adapter\nGenerationCN1300R\nPart NumberQ0F09A\n\n\n\nProducts ID736414\nManufacturerHP StoreFabric\nDevice TypeNetwork Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 X8\nData Link Protocol10GB CEE, Fibre Channel, FCoE\nData Transfer Rate10/25GB/s\nPortsDual Port\nConnectivity TechnologyWired\n \nNetwork Transport ProtocoliSCSI",null,"g"]
["PY278AA","Description:HP 250GB Non-Hot-Plug SATA II 7.2K 3.5-inch 3.0Gb/sPart Number(s)\nHP Option Part# PY278AA\nSeagate Model# ST3250318AS\nSeagate Assembly Part# 9SL131-021\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA NHP\nPart NumberPY278AA\n\n\n\nProducts ID142068\nTypeHardDrive - Internal\nCapacity250GB\nInterface TypeSerial ATA II\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate300MB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["PY277AA","Description:160GB SATA 2 (3G) Hard Drive ROHS    7200 RPM 3.5-inch form factor 1.0-inch highPart Number(s)Option Part# PY277AA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category160GB\nGenerationSATA NHP\nPart NumberPY277AA\n\n\n\nProducts ID1142067\nTypeHard Drive - Internal\nCapacity160GB\nInterface TypeSerial ATA II\nConnector22-position Serial ATA (SATA) Plug\nData Transfer Rate300MB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["PY276AA","Description: 80GB SATA 3G Hard Drive 7.2K 3.5-inch HP Desktop Hard DriveGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nHewlett-Packard Part# PY276AA\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA NHP\nPart NumberPY276AA\n\n\n\nProducts ID142066\nTypeHard Drive - Internal\nCapacity80GB\nInterface TypeSerial ATA II\nConnector22 - Position Serial ATA (SATA) Plug\nData Transfer Rate300MB/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["PV944A","Description:HP 160GB Serial ATA/300 IDE NHP Hard Drive 7200 RPM 3.5-inch form factor 1.0-inch highPart Number(s)Manufacturer Part# PV944A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA NHP\nPart NumberPV944A\n\n\n\nProducts ID1142065\nTypeHard Drive - Internal\nCapacity160GB\nInterface TypeSerial ATA - 300\nData Transfer Rate300MB/s\nSpindle Speed7200RPM\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]",null,"g"]
["PS6301-1","Description:Compaq Proliant 275W Hot-Plug Power SupplyFor the Proliant DL380 G1 ServerPart Number(s)\nSpare Part# 108859-001\nAssembly Part# PS6301-1\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nAs data protection and high availability have become increasingly important, customers are demanding solid  uninterrupted performance. Continuous development and enhancement of high-performance software applications and operating systems is driving the need for continued reliability. HP Proliant customers can be assured that all of their hardware needs will be met -  the above issues will be addressed  and they will have components manufactured to the highest quality standards and subjected to the most rigorous testing procedures that only genuine components will realize. HP manufactured Power Supplies are no exception.\n\nSpecifications:\nCategoryProliant\nSub-CategoryProliant Power Supply\nGenerationDL380 G1\nPart NumberPS6301-1\n\n\n\nProducts ID454551\nModelPS6301-1\nApplicationProliant DL380\nDevice TypePower Supply\nWattage275W\nInput Voltage110-115 V\nHot PluggableYes\nRedundantYes\nAuto SwitchingYes\n \nCoolingActive Fan\nFanInternal\n \nPFC.95\nManufacturerCompaq\n \nPackage Qty1\n\n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# PS6301-1 DL380 G1 Proliant Power Supply",null,"g"]
["PS-4241-9HB","Description:HP 240W 100/240V PSU Power SupplyPart Number(s)Model Part# PS-4241-9HBSpare Part# 611481-001Spare Part# 613762-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  240W 100/240V Power Supply\n\nSpecifications:\nCategoryHP \nSub-CategoryPSU Power Supply\nGeneration240W\nPart NumberPS-4241-9HB\n\n\n\nProducts ID480038\nManufacturerHP\nForm FactorInternal SFF\nOutput Power240W\nInput Voltage110V AC\nOutput Voltage12V DC",null,"g"]
["PS-2801-3C-LF","Description:\nHP 800W Flex Slot Universal Hot-Plug Power Supply\nPart Number(s)\nOption Part# 720484-B21\nSpare Part# 735037-001\nAssembly Part# 735039-201\nAssembly Part# 754379-001\nModel# HSTNS-PL45\nModel# PS-2801-3C-LF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHow do you improve data center power efficiency without impacting IT performance? HP Flexible Slot Power Supplies provide up to 94% power efficiency with 80Plus Platinum-certified power supplies that lower server power requirements and reduce power waste in your data center. Flex Slot Power Supplies have a form factor that is 25% smaller than previous generation power supplies - providing more space to add additional server options and improve the performance of your servers. Flex Slot Power Supplies provide fast - tool-less hot plug access to server power supplies for greater serviceability and are supported across the entire Proliant DL300 Gen9 Server family - simplifying your spares strategy and further reducing data center costs. Are you currently using or interested in the HP Power Discovery Services solution? Support for Power Discovery Services can be added to all Proliant DL300 Gen9 Servers with the Flex Slot 1400W Platinum Plus Power Supply option.\n\nSpecifications:\nCategoryProliant\nSub-CategoryProliant Power Supply\nGenerationDL360 G9\nPart NumberPS-2801-3C-LF\n\n\n\nProducts ID494854\nDevice TypePower Supply\nPower Provided800 Watts\nFanInternal\nManufacturerHewlett Packard\nForm FactorPlug-in Module\nEfficiency96%\nSpecification ComplianceFlex Slot\nVoltage RequiredAC 200-277 V\n \nHot PlugYes\nRedundantYes\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# PS-2801-3C-LF DL360 G9 Proliant Power Supply",null,"g"]
["PS-2751-7CB-LF","Description:HP 750W Common Slot Platinum PlusHot-Plug Power Supply KitPart Number(s)\nOption Part# 739254-B21\nSpare Part# 742516-001\nAssembly Part# 748281-201\nModel# PS-2751-7CB-LF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Common Slot (CS) Power Supplies share a common electrical and physical design that allows for Hot-Swap - tool-less installation into HP server and storage solutions. CS power supplies are available in multiple high-efficiency input and output options - allowing users to “right-size” a power supply for specific server/storage configurations and environments. This flexibility helps to minimize power waste - lower overall energy costs - and avoid trapped power capacity in the data center. A key part of the HP Thermal Discovery Services - CS Platinum/Platinum Plus Power Supplies provide the IT industry’s highest level of power efficiency(94%) - helping customers to reduce power requirements by up to 60W per server and reducing overall data center power requirements by up to 10% (as compared to Proliant G6 power estimates). CS Platinum/Platinum Plus power supplies also enable HP Power Discovery Services which focus on increasing compute density while reducing data center outages.\n\nSpecifications:\nCategoryProliant\nSub-CategoryProliant Power Supply\nGeneration750Watt\nPart NumberPS-2751-7CB-LF\n\n\n\nProducts ID1736607\nModel739254-B21\nDevice TypePower Supply\nWattage750W\nInput Voltage110-220 V AC\nHot PluggableYes\nFanInternal\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# PS-2751-7CB-LF 750Watt Proliant Power Supply",null,"g"]
["PS-2122-4CB-LF","Description:HP 1200W Common Slot Platinum PlusHot-Plug Power Supply Kit\nPart Number(s)\nOption Part# 748287-B21\nSpare Part# 748896-001\nAssembly Part# 746283-201\nModel# PS-2122-4CB-LF\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Common Slot (CS) Power Supplies share a common electrical and physical design that allows for Hot-Swap - tool-less installation into HP server and storage solutions. CS power supplies are available in multiple high-efficiency input and output options - allowing users to “right-size” a power supply for specific server/storage configurations and environments. This flexibility helps to minimize power waste - lower overall energy costs - and avoid trapped power capacity in the data center. A key part of the HP Thermal Discovery Services - CS Platinum/Platinum Plus Power Supplies provide the IT industry’s highest level of power efficiency(94%) - helping customers to reduce power requirements by up to 60W per server and reducing overall data center power requirements by up to 10% (as compared to Proliant G6 power estimates). CS Platinum/Platinum Plus power supplies also enable HP Power Discovery Services which focus on increasing compute density while reducing data center outages.\n\nSpecifications:\nCategoryProliant Option\nSub-CategoryProliant Power Supply\nGeneration1200 Watt\nPart NumberPS-2122-4CB-LF\n\n\n\nProducts ID1736612\nModel748287-B21\nDevice TypePower Supply\nWattage1200W\nInput Voltage110-220 V AC\nHot PluggableYes\nFanInternal\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# PS-2122-4CB-LF 1200 Watt Proliant Power Supply",null,"g"]
["PM254A","Description:HP 400GB SATA 150 IDE 7.2K Hard DriveIn HP Hot-Plug Hard Drive tray (as pictured)For HP G1-G7 Proliant SATA Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nPart# PM254A\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on our variety of new  tested  Genuine HP  SMART capable  SATA Hard Drives offering data integrity and availability in hot-pluggable models. Before final certification all HP Serial-ATA Hard Drives are optimized for compatibility and functionality  including support of SMART and HP System Insight Manager.\n\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA\nPart NumberPM254A\n\n\n\nProducts ID142064\nTypeHard Drive - Internal\nForm Factor3.5 inches x 1/3H\nCapacity400GB\nInterface TypeSerial ATA - 150\nSpindle Speed7200RPM\nBuffer Size8MB\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# PM254A SATA 7.2K",null,"g"]
["PD749AW","Description: XW4200 Workstation 3.20GHZ 512MB \n\n\n\n\n\n\n\n\n\nSpecifications:\nCategory\nSub-Category\nGeneration\nPart NumberPD749AW\nProducts ID142133",null,"g"]
["P9M82A","Description:HP MSA/MSA2 10TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM\n512e Dual Port (DP) Midline (MDL) Hot-Plug Hard Drive\nIn HP MSA/MSA2 Hard Drive tray w/interposer connector (as pictured)\nFor HP MSA1040 MSA2040 MSA2050 MSA2000 MSA2000i and\nP2000 SAN Storage Arrays\nGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# P9M82A\nSpare Part# 868230-001\nAssembly Part# 868151-002\nModel# HUH721010AL5204\nModel# ST10000NM0528\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 / MSA2000 controller enclosures and large form factor expansion enclosures accept unique HP SAS disk drive modules with different firmware and different trays than other HP storage arrays and Proliant servers. The disk drives have SAS interposers attached to the back which convert the native dual port SAS interface to an SCA-40 connector. While this SCA-40 connector has the same shape as a Fibre Channel (FC) connector - the drives are NOT utilizing the FC protocol. If you look closely at the interposer - the circuitry is rather simplistic and no bridge / translator chip is attached. The interposer is - more or less - acting as a signal filter and port relocator to connect to the MSA2's proprietary backplane.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category7.2K\nGenerationSAS MSA 2\nPart NumberP9M82A\n\n\n\nProducts ID1201031\nTypeHard Drive - Hot-Plug\nCapacity10TB\nInterface TypeSerial Attached SCSI\nSpindle Speed7200RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P9M82A SAS MSA 2 7.2K",null,"g"]
["P9M81A","Description:HP MSA2 1.2TB 2.5-inch Serial Attached SCSI (SAS) SFF 12Gb/sDual Port Enterprise (ENT) Hot-Plug 10K MSA SED Hard DriveIn HP Hot-Plug MSA Hard Drive tray (as pictured)For HP MSA1040 MSA2040 MSA2050 MSA2052 MSA2000 MSA2000i\nand P2000 SAN Storage ArraysGenuine HP serial number and MSA/MSA2 firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# P9M81A\nSpare Part# 868233-001\nAssembly Part# 868152-001\nModel# ST1200MM0108\nModel# ST1200MM0039\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000 / MSA2000i and P2000 controller enclosures accept unique HP SAS2.5-inch SFF and 3.5-inch LFF  Hard Drives with different firmware than other HP storage arrays and Proliant servers.This Genuine HP 2.5-inch SAS Hard Drive is designed and configured specifically for the HP MSA2 MSA1040 / MSA2040 / MSA2050 / MSA2052 / MSA2000 / MSA2000i or P2000 series SAN Storage Array.\nThis Hard Drive will have the correct firmware for these systems.\n\nSpecifications:\nCategoryStorageWorks HardDrive\nSub-Category10K\nGenerationSAS MSA2\nPart NumberP9M81A\n\n\n\nProducts ID494515\nTypeHard Drive - Hot-Swap\nCapacity1.2TB\nInterface TypeSerial Attached SCSI\nSpindle Speed10000RPM\nPortsDual Port\nSpeed12GB/s\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P9M81A SAS MSA2 10K",null,"g"]
["P9M80A","Description:HP MSA 800GB 3.5in SAS 12G Mixed Use (MU) SSD\nGenuine HP serial number and MSA firmware\nGenuine HP manufactured Hard DrivePart Number(s)\nOption Part# P9M80A\nSpare Part# 868232-001\nModel# XS800LE70004\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications processors memory adapters and storage devices increases high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions adding new levels of performance availability flexibility and management.\n\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberP9M80A\n\n\n\nProducts ID737672\nTypeHard Drive - Hot-Plug\nCapacity800GB\nInterface TypeSerial Attached SCSI\nCarrier TypeStandard MSA Carrier\nInterfaceSAS 12Gb/s\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P9M80A SAS MSA StorageWorks HardDrive",null,"g"]
["P9M76A","Description:HP StoreFabric (SF) SN1600Q 32Gb Fibre Channel (FC) Adapter\nDual Port (DP) PCI-e 3.0 Fibre Channel  Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# P9M76A \nSpare Part# 868141-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1600Q 32Gb Fibre Channel (FC) Adapter Dual Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9M76A \n\n\n\nProducts ID728273\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0 x8\nData Transfer Rate32GB/s\nPorts32gb Fibre Channel X 2\nConnectivity TechnologyWired\nCabling TypeFibre Optic\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P9M76A  FibreChannel Host Bus Adapter",null,"g"]
["P9M76-63001","Description:HP StoreFabric SN1600Q 32Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# P9M76-63001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE StoreFabric SN1600Q 32Gb Fibre Channel Host Bus Adapters bring data center infrastructure components to a higher level of performance and efficiency with the ability to deliver twice the bandwidth of 16Gb Fibre Channel (FC) Host Bus Adapters (HBAs). It is backward compatible with 16Gb and 8Gb FC storage networks and will protect future investments. It provides a Peripheral Component Interface express (PCIe) interface providing a number of features that work together to reduce power consumption - delivering a \"green\" benefit within the server.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9M76-63001\n\n\n\nProducts ID725550\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPortsDual Port\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)",null,"g"]
["P9M75A","Description:HP StoreFabric SN1600Q 32Gb Fibre Channel (FC) Adapter\nSingle Port PCI-e 3.0 Fibre Channel  Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# P9M75A\nSpare Part# 868140-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1600Q 32Gb Fibre Channel (FC) Adapter Single Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9M75A\n\n\n\nProducts ID728123\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0 x8\nData Transfer Rate32GB/s\nPorts32gb Fibre Channel X 1\nConnectivity TechnologyWired\nCabling TypeFibre Optic",null,"g"]
["P9H32A","Description:Genuine HP B-Series 32GB Fibre Channel Short Wave\nSmall Form Factor Pluggable Plus (SFP+) \nTransceiver Module\nPart Number(s)\nManufacturer Part# P9H32A\nSpare Part# 855073-001\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE B-Series 32GB Fibre Channel Short Wave SFP+ 2GBPS Transceiver Module. It is designed to work with HPE B-Series Fibre Channel switches and storage arrays.\n\nThe module is a Small Form-factor Pluggable (SFP+) transceiver which means it is a small hot-swappable device that connects the optical fiber cable to a network device. It is used to transmit and receive data over fiber optic cable at a speed of 2 Gbps.\n\nThe module uses short wave technology which means it operates at a wavelength of 850nm. This wavelength is commonly used in short distance data transmission such as within a data center or between buildings.\n\nThe module has a maximum distance of 300m on 50/125um multimode fiber and has a LC connector.\n\nThe product is a 32GB Fibre Channel transceiver which means it is designed to work with the Fibre Channel protocol a high-speed networking technology commonly used in storage area networks (SANs). It supports data transfer rates of up to 32 Gbps providing high-speed data transfer for large amounts of data.\n\n\n\n\n\n\n\n\n\n\n\n\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP+\nPart NumberP9H32A\n\n\n\nProducts ID737083\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP (mini-GBIC) \nOptical Wave Length850 nm\nForm FactorHot-swappable\nData Transfer Rate32Gb/s\nInterfaces / Ports Details1 x LC Fiber Channel Network",null,"g"]
["P9H30A","Description:Genuine HP B-Series 32GB Fibre Channel (FC) Short Wave (SW)\nSmall Form Factor Pluggable Plus (SFP+) \nOptical Transceiver Module\nPart Number(s)\nOption Part# Part# P9H30A \nSpare Part# 855071-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHewlett Packard Enterprise optical transceivers offer improved performance and reliability- as well as compatibility with HPE storage and computing products. Designed for customers that require the highest levels of connectivity- performance and reliability from their HPE SAN.\n\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP+\nPart NumberP9H30A \n\n\n\nProducts ID737953\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP+\nMax Transfer Distance328 ft\nForm FactorHot-swappable\nData Transfer Rate32Gb/s\nInterfaces / Ports Details1 x 32Gb Fibre Channel (SW)",null,"g"]
["P9H29A","Description:Genuine HP Long Wave B-Series 32Gb/s Fibre Channel\nSFP+ 1 Pack Transceiver Module\nPart Number(s)\nManufacturer Part# P9H29A\nSpare Part# 855070-001\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationSFP\nPart NumberP9H29A\n\n\n\nProducts ID737956\nManufacturerHP\nApplication/UsageData Networking\nInterface SFP+\nNetwork TechnologyFiber Channel\nForm FactorPlug-in Module\nData Transfer Rate32Gb/s\nInterfaces / Ports Details1 x Fiber Channel Network",null,"g"]
["P9D96A","Description:HP StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# P9D96A\nSpare Part# 853011-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9D96A\n\n\n\nProducts ID738434\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPortsDual Port\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)\n \nExpansion Slots2 (Total) 0 (Free) X SFP+\nInterfaces2 x 16GB FC (Short Wave) -LC Multi-Mode",null,"g"]
["P9D94A","Description:HP StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# P9D94A\nSpare Part# 853011-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9D94A\n\n\n\nProducts ID492470\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPortsDual Port\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)\n \nExpansion Slots2 (Total) 0 (Free) X SFP+\nInterfaces2 x 16GB FC (Short Wave) -LC Multi-Mode\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n  [ Manufacturers Specs ]",null,"g"]
["P9D94-63001","Description:HP StoreFabric SN1100Q 16Gb Fibre Channel (FC) AdapterDual Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nSpare Part#P9D94-63001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1100Q 16Gb Fibre Channel (FC) Adapter Dual Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9D94-63001\n\n\n\nProducts ID725460\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPortsDual Port\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)\n \nExpansion Slots2 (Total) 0 (Free) X SFP+\nInterfaces2 x 16GB FC (Short Wave) -LC Multi-Mode",null,"g"]
["P9D93A","Description:HP StoreFabric SN1100Q 16Gb Fibre Channel (FC) Adapter\nSingle Port PCI-e 3.0 Fibre Channel  Host Bus Adapter (HBA)\nPart Number(s)\nOption Part# P9D93A\nSpare Part# 853010-001Note:Please confirm Low Profile or Full Height Bracket\nIn comments box at checkout. Thank you\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  StoreFabric SN1100Q 16Gb Fibre Channel (FC) Adapter Single Port PCI-e Host Bus Adapter (HBA).\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9D93A\n\n\n\nProducts ID728122\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card - Low Profile\nInterface TypePCI Express 3.0\nData Transfer Rate14.025GB/s\nPorts16gb Fibre Channel X 1\nConnectivity TechnologyWired\nCabling TypeFibre Optic\nData Link Protocol4GB FC (SW) 8GB (SW) 16GB FC (SW)",null,"g"]
["P9D91A","Description:HP StoreFabric 84Q 8Gb Fibre Channel (FC) Adapter BoardQuad Port PCI-e Host Bus Adapter (HBA)Part Number(s)\nOption Part# P9D91A\nSpare Part# 853009-001Note: Requires one Low Profile or Full Height x8 PCIe Slot\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP StoreFabric 84Q Fibre Channel Host Bus Adapter Board has two fully independent 2/4/8Gb auto-negotiation short wave laser LC Ports.\n\nSpecifications:\nCategoryHP Option\nSub-CategoryHost Bus Adapter\nGenerationFibreChannel\nPart NumberP9D91A\n\n\n\nProducts ID736413\nDevice TypeHost Bus Adapter\nForm FactorPlug-In Card\nInterface TypePCI Express 3.0 x8\nData Transfer Rate8Gb/s\nPortsQuad Port",null,"g"]
["P60159-001","Description:HP ProLiant DL325 G11 Megacell Extension Cable Kit Part Number(s)\nOption Part# P56659-B21 \nSpare Part# P60159-001\n\n\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP ProLiant Megacell Extension Cable Kit \n\nSpecifications:\nCategoryProliant\nSub-CategoryCable Kit\nGenerationDL325 G11\nPart NumberP60159-001 \n\n\n\nProducts ID737135",null,"g"]
["P59819-001","Description:HP MSA 20TB 7.2K SAS 3.5 12G Midline (MDL) M.2 HDD\nPart Number(s)\nOption Part# S0F32A\nSpare Part# P59819-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HP  MSA storage system brings the performance benefits of SSDs to MSA array family customers. This array has\nbeen designed to maximize performance by using high-performance drives across all applications sharing the array.\nThe HP  MSA storage systems are positioned to provide an excellent value for customers needing increased\nperformance to support initiatives such as consolidation and virtualization.\n\nSpecifications:\nCategoryHP\nSub-CategoryStorageWorks HardDrive\nGenerationSAS MSA\nPart NumberP59819-001\n\n\n\nProducts ID738341\nCapacity20TB\nInterfaceSAS 12Gb/s\nCarrier TypeStandard MSA Carrier\nForm Factor3.5 inches\nWorkload TypeEnterprise\nDrive Rotational Speed7200 RPM",null,"g"]
["P59668-B21","Description:HP DL325 Gen11 Liquid Cooling Fan Kit\nPart Number(s)\nOption Part# P59668-B21\nSpare Part# P53225-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL325 G11 Liquid Cooling Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP59668-B21\n\n\n\nProducts ID1737483\nProduct TypeFan Kit",null,"g"]
["P58543-001","Description:HP MR408i-o Gen11 x8 Lanes 4GB Cache OCP SPDM Storage ControllerPart Number(s)\nOption Part# P58335-B21\nSpare Part# P58543-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need a versatile simplified and flexible choice for your data centers? HPE Compute MR Gen11 Controllers are expansive and agile PCIe Gen4.0 storage controllers based on Broadcom MegaRAID technology that deliver quality performance and security for mission-critical applications. The HPE Gen11 Controllers are ideal for all data center environments where RAID is applicable offering reduced rebuild times high-bandwidth and 240K RAID5 Random Write IOPS. The HPE Gen11 Controllers are ideal for all virtualized environments where HBA / pass-through mode is applicable offering high bandwidth and 3 million Random Write IOPS. HPE Compute MR Gen11 Controllers offer solutions for multiple workflows across multiple applications to deliver customer satisfaction.\n\n\nSpecifications:\nCategoryProliant Controller\nSub-CategoryRAID \nGenerationGen11\nPart NumberP58543-001\n\n\n\nProducts ID736974\nManufacturerHP\nProduct TypeStorage Controller (RAID)\nInterfacePCI Express 4.0 \nRAID Level0, 1, 5, 6, 10, 50, 60\nMaximum Physical Drives 240\nMaximum Logical Drives64\nPorts1x8 LP SlimSAS\nCache4GB\n \nInternal SAS lanesx8",null,"g"]
["P58540-B21","Description:1 x AMD EPYC 9224 DL385 Gen11(2.5GHz/24-core/200W)\nPart Number(s)\nOption Part# P58540-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP58540-B21\n\n\n\nProducts ID736988\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreTetracosa-Core\nProcessor Qty1\nClock Speed2.5GHz\nThermal Design Power200W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58540-B21 G11 EPYC",null,"g"]
["P58488-001","Description:HPE 64GB (1 x 64GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56431-B21\nSpare Part# P58488-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P58488-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP58488-001\n\n\n\nProducts ID1737144\nProduct TypeMemory Module\nMemory Size64GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 64GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58488-001 G10 G11 Genuine HP Memory",null,"g"]
["P58487-001","Description:HPE 32GB (1 x 32GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56429-B21\nSpare Part# P58487-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P58487-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP58487-001\n\n\n\nProducts ID737142\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58487-001 G10 G11 Genuine HP Memory",null,"g"]
["P58486-001","Description:HPE 32GB (1 x 32GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56427-B21\nSpare Part# P58486-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P58486-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP58486-001\n\n\n\nProducts ID1737139\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58486-001 G10 G11 Genuine HP Memory",null,"g"]
["P58485-001","Description:HPE 16GB (1 x 16GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56425-B21\nSpare Part# P58485-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P58485-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP58485-001\n\n\n\nProducts ID737137\nProduct TypeMemory Module\nMemory Size16GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 16GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58485-001 G10 G11 Genuine HP Memory",null,"g"]
["P58465-B21","Description:HP DL3X5 G11 2U Standard Fan Kit\nPart Number(s)\nOption Part# P58465-B21\nSpare Part# P52434-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL3X5 G11 2U Standard Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP58465-B21\n\n\n\nProducts ID737484\nProduct TypeFan Kit",null,"g"]
["P58464-B21","Description:HP DL3X5 G11 2U Standard Fan Kit\nPart Number(s)\nOption Part# P58464-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL3X5 G11 2U Standard Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP58464-B21\n\n\n\nProducts ID1737482\nProduct TypeFan Kit",null,"g"]
["P58462-B21","Description:HP DL325 G11 1U Performance Fan KitPart Number(s)\nOption Part# P58462-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  DL325 G11 1U Performance Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP58462-B21\n\n\n\nProducts ID737133\nProduct TypeFan Kit",null,"g"]
["P58461-B21","Description:HP ProLiant DL365 Gen11 1U Standard Fan KitPart Number(s)\nOption Part# P58461-B21\nSpare Part# P53226-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Standard Fan Module for works in HPE ProLiant DL300 series Gen11 Servers.\n\nSpecifications:\nCategoryHP\nSub-CategoryFan Option\nGenerationGen11\nPart NumberP58461-B21\n\n\n\nProducts ID736969\nHeight (Rack Units)1U",null,"g"]
["P58433-001","Description:HP 7.68TB 3.5-inch LFF SATA   6Gb/s  \nVery Read Optimized (VRO) Solid State Drive (SSD)\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)Hot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive (SSD)\nPart Number(s)\nOption Part# P58232-B21\nSpare Part# P58433-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA LPc SSD\nPart NumberP58433-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736778\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nData Transfer Rate600 MB/s\nInterfaceSerial ATA\nBest ApplicationVery Read Optimized (VRO)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58433-001 SATA LPc SSD Solid State Drive",null,"g"]
["P58432-001","Description:HP 7.68TB 2.5-inch SFF SATA Very-Read-Optimized (VRO) 6Gb/s\nDigitally Signed Firmware (DS) Solid State Drive (SSD) 5400\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P58228-B21\nSpare Part# P58432-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58432-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736770\nTypeSolid State Drive\nCapacity7.68-TB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58432-001 SATA BC SSD Solid State Drive",null,"g"]
["P58430-001","Description:HP 960GB 2.5-inch SFF SATA Mixed-Use (MU) 6Gb/s\nSelf-Encrypting (SED) 5400M Digitally Signed Firmware (DS) \nSolid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part#  P58244-B21\nSpare Part# P58430-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58430-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1737036\nTypeSolid State Drive\nCapacity960-GB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58430-001 SATA BC SSD Solid State Drive",null,"g"]
["P58428-001","Description:HP 480GB 2.5-inch SFF SATA Mixed-Use (MU) 6Gb/s\nSelf-Encrypting (SED) 5400P Digitally Signed Firmware (DS) \nSolid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part#  P58236-B21\nSpare Part# P58428-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58428-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID737044\nTypeSolid State Drive\nCapacity480-GB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58428-001 SATA BC SSD Solid State Drive",null,"g"]
["P58335-B21","Description:HP MR408i-o Gen11 x8 Lanes 4GB Cache OCP SPDM Storage ControllerPart Number(s)\nOption Part# P58335-B21\nSpare Part# P58543-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need a versatile simplified and flexible choice for your data centers? HPE Compute MR Gen11 Controllers are expansive and agile PCIe Gen4.0 storage controllers based on Broadcom MegaRAID technology that deliver quality performance and security for mission-critical applications. The HPE Gen11 Controllers are ideal for all data center environments where RAID is applicable offering reduced rebuild times high-bandwidth and 240K RAID5 Random Write IOPS. The HPE Gen11 Controllers are ideal for all virtualized environments where HBA / pass-through mode is applicable offering high bandwidth and 3 million Random Write IOPS. HPE Compute MR Gen11 Controllers offer solutions for multiple workflows across multiple applications to deliver customer satisfaction.\n\n\nSpecifications:\nCategoryProliant Controller\nSub-CategoryRAID \nGenerationGen11\nPart NumberP58335-B21\n\n\n\nProducts ID736973\nManufacturerHP\nProduct TypeStorage Controller (RAID)\nInterfacePCI Express 4.0 \nRAID Level0, 1, 5, 6, 10, 50, 60\nMaximum Physical Drives 240\nMaximum Logical Drives64\nPorts1x8 LP SlimSAS\nCache4GB\n \nInternal SAS lanesx8",null,"g"]
["P58244-B21","Description:HP 960GB 2.5-inch SFF SATA Mixed-Use (MU) 6Gb/s\nSelf-Encrypting (SED) 5400M Digitally Signed Firmware (DS) \nSolid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part#  P58244-B21\nSpare Part# P58430-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58244-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1737032\nTypeSolid State Drive\nCapacity960-GB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58244-B21 SATA BC SSD Solid State Drive",null,"g"]
["P58236-B21","Description:HP 480GB 2.5-inch SFF SATA Mixed-Use (MU) 6Gb/s\nSelf-Encrypting (SED) 5400P Digitally Signed Firmware (DS) \nSolid State Drive (SSD)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part#  P58236-B21\nSpare Part# P58428-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58236-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID737040\nTypeSolid State Drive\nCapacity480-GB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58236-B21 SATA BC SSD Solid State Drive",null,"g"]
["P58232-K21","Description:HP 7.68TB 3.5-inch LFF SATA   6Gb/s  \nVery Read Optimized (VRO) Solid State Drive (SSD)\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)Hot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive (SSD)\nPart Number(s)\nOption Part# P58232-K21\nSpare Part# P58433-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA LPc SSD\nPart NumberP58232-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1736782\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nData Transfer Rate600 MB/s\nInterfaceSerial ATA\nBest ApplicationVery Read Optimized (VRO)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58232-K21 SATA LPc SSD Solid State Drive",null,"g"]
["P58232-H21","Description:HP 7.68TB 3.5-inch LFF SATA   6Gb/s  \nVery Read Optimized (VRO) Solid State Drive (SSD)\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)Hot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive (SSD)\nPart Number(s)\nOption Part# P58232-H21\nSpare Part# P58433-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA LPc SSD\nPart NumberP58232-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736786\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nData Transfer Rate600 MB/s\nInterfaceSerial ATA\nBest ApplicationVery Read Optimized (VRO)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58232-H21 SATA LPc SSD Solid State Drive",null,"g"]
["P58232-B21","Description:HP 7.68TB 3.5-inch LFF SATA   6Gb/s  \nVery Read Optimized (VRO) Solid State Drive (SSD)\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)Hot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive (SSD)\nPart Number(s)\nOption Part# P58232-B21\nSpare Part# P58433-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA LPc SSD\nPart NumberP58232-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736774\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nData Transfer Rate600 MB/s\nInterfaceSerial ATA\nBest ApplicationVery Read Optimized (VRO)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58232-B21 SATA LPc SSD Solid State Drive",null,"g"]
["P58228-K21","Description:HP 7.68TB 2.5-inch SFF SATA Very-Read-Optimized (VRO) 6Gb/s\nDigitally Signed Firmware (DS) Solid State Drive (SSD) 5400\nIn HP G10+ (G10-Plus) Hot-PlugBasic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P58228-K21\nSpare Part# P58432-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58228-K21\n\nBest Use:    \nManufacturer:Hewlett Packard\n\n\nProducts ID736790\nTypeSolid State Drive\nCapacity7.68-TB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58228-K21 SATA BC SSD Solid State Drive",null,"g"]
["P58228-B21","Description:HP 7.68TB 2.5-inch SFF SATA Very-Read-Optimized (VRO) 6Gb/s\nDigitally Signed Firmware (DS) Solid State Drive (SSD) 5400\nIn HP G10+ (G10-Plus) Hot-PlugBasic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P58228-B21\nSpare Part# P58432-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSATA BC SSD\nPart NumberP58228-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID736766\nTypeSolid State Drive\nCapacity7.68-TB\nInterface TypeSATA\nDrive Interface StandardSATA\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P58228-B21 SATA BC SSD Solid State Drive",null,"g"]
["P58212-001","Description:HP ML350 Gen11 4LFF SAS/SATA Basic Drive Cage Kit \nPart Number(s)\nOption Part# P47216-B21\nSpare Part# P58212-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nEnhance the capabilities of your server with the HPE Storage Drive Cage. This 3.5-inch SFF 4-bay cage eliminates corrupted disks read errors and data write issues caused by vibrations by keeping HDD drives firmly mounted. It is designed for use with the HPE ProLiant DL350 Gen11 (3.5-inch).\n\nSpecifications:\nCategoryHP Proliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP58212-001\n\n\n\nProducts ID1738327\nProduct TypeFan Kit",null,"g"]
["P56915-B21","Description:HP DL365 Gen11 1U x16 Riser KitPart Number(s)\nOption Part# P56915-B21\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL365 Gen11 1U x16 Riser Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryRiser Kit\nGenerationG11\nPart NumberP56915-B21\n\n\n\nProducts ID736968\nProduct TypeRiser Kit",null,"g"]
["P56659-B21","Description:HP ProLiant DL325 G11 Megacell Extension Cable Kit Part Number(s)\nOption Part# P56659-B21 \nSpare Part# P60159-001\n\n\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP ProLiant Megacell Extension Cable Kit \n\nSpecifications:\nCategoryProliant\nSub-CategoryCable Kit\nGenerationDL325 G11\nPart NumberP56659-B21 \n\n\n\nProducts ID1737134",null,"g"]
["P56652-B21","Description:HP DL325 G11 1U 2SFF x4 NVMe U.3 Backplane KitIncludes 2 cables/drive cage and backplaneFor the DL325 G11 Servers\nPart Number(s)\nOption Part# P56652-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management.\n\nSpecifications:\nCategoryProliant Option\nSub-CategoryDL325\nGenerationG11\nPart NumberP56652-B21\n\n\n\nProducts ID737488\nManufacturerHP",null,"g"]
["P56435-B21","Description:HPE 256GB (1x256GB) Octal Rank x4 DDR4-3200\nCAS-26-22-22 Load Reduced 3DS Smart Memory Kit\nPart Number(s)\nOption Part# P56435-B21\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56435-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity - along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization - runs at top throughput speed - and is among the most power-efficient memory available. In addition to performance and efficiency - HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever - DRAM quality is critical - as data center trends such as server virtualization - cloud computing - and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG11\nPart NumberP56435-B21\n\n\n\nProducts ID1737145\nProduct TypeMemory Module\nMemory Size256GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 256GB\nMemory Speed3200MHz\nMemory StandardDDR4-3200/PC4-25600\nSignal ProcessingRegistered\nForm Factor288-pin LRDIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes",null,"g"]
["P56431-B21","Description:HPE 64GB (1 x 64GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56431-B21\nSpare Part# P58488-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56431-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP56431-B21\n\n\n\nProducts ID1737143\nProduct TypeMemory Module\nMemory Size64GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 64GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56431-B21 G10 G11 Genuine HP Memory",null,"g"]
["P56429-B21","Description:HPE 32GB (1 x 32GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56429-B21\nSpare Part# P58487-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56429-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP56429-B21\n\n\n\nProducts ID1737140\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56429-B21 G10 G11 Genuine HP Memory",null,"g"]
["P56427-B21","Description:HPE 32GB (1 x 32GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56427-B21\nSpare Part# P58486-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56427-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP56427-B21\n\n\n\nProducts ID737138\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56427-B21 G10 G11 Genuine HP Memory",null,"g"]
["P56425-B21","Description:HPE 16GB (1 x 16GB) Single Rank x4 DDR4-3200\nCAS-22-22-22 Registered SmartMemory KitPart Number(s)\nOption Part# P56425-B21\nSpare Part# P58485-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56425-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHPE DDR4 SmartMemory is designed for small to large enterprise customers with a significant need for performance and capacity along with a desire to manage total cost of ownership. HPE DDR4 SmartMemory enables total server memory optimization runs at top throughput speed and is among the most power-efficient memory available. In addition to performance and efficiency HPE DDR4 SmartMemory also delivers on reliability. Only the highest-quality DRAM modules are selected from top suppliers. Now more than ever DRAM quality is critical as data center trends such as server virtualization cloud computing and the use of large database applications have increased the need for higher-capacity memory with greater up-time. HPE DDR4 SmartMemory undergoes rigorous qualification and testing processes that unlock memory performance features available only with HPE servers.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationG10 G11\nPart NumberP56425-B21\n\n\n\nProducts ID737136\nProduct TypeMemory Module\nMemory Size16GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 16GB\nMemory CL22\nMemory StandardDDR4-3200\nSignal ProcessingRegistered\nForm Factor288-pin DIMM\n \nError CheckingECC\nManufacturerHewlett Packard\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56425-B21 G10 G11 Genuine HP Memory",null,"g"]
["P56153-001","Description:HPE 64GB (1 x64GB) Dual Rank x4 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50312-B21\nSpare Part# P56153-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56153-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen11\nPart NumberP56153-001\n\n\n\nProducts ID736966\nProduct TypeMemory Module\nMemory Size64GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 64GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56153-001 Gen11 Genuine HP Memory",null,"g"]
["P56152-001","Description:HPE 32GB (1 x32GB) Dual Rank x8 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50311-B21\nSpare Part# P56152-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56152-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen11\nPart NumberP56152-001\n\n\n\nProducts ID736964\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56152-001 Gen11 Genuine HP Memory",null,"g"]
["P56151-001","Description:HPE 32GB (1 x32GB) Single Rank x4 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50310-B21\nSpare Part# P56151-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56151-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen 11\nPart NumberP56151-001\n\n\n\nProducts ID1736962\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56151-001 Gen 11 Genuine HP Memory",null,"g"]
["P56150-001","Description:HPE 16GB (1 x16GB) Single Rank x8 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50309-B21\nSpare Part# P56150-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P56150-001 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen11\nPart NumberP56150-001\n\n\n\nProducts ID1736960\nProduct TypeMemory Module\nMemory Size16GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 16GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P56150-001 Gen11 Genuine HP Memory",null,"g"]
["P55698-B21","Description:HP DL380 Gen10 Plus  SFF SAS/SATA Basic Carrier Drive Cage Kit\nPart Number(s)\nOption Part# P55698-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL380 Gen10 Plus  2SFF SAS/SATA BC Drive Cage Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG10+\nPart NumberP55698-B21\n\n\n\nProducts ID1737494\nProduct TypeFan Kit",null,"g"]
["P55516-B21","Description:HP DL380 G10+ 8SFF SAS/SATA to Tri-Mode Controller Backplane KitPart Number(s)\nOption Part# P55516-B21\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL380 G10+ 8SFF SAS/SATA to Tri-Mode Controller Backplane Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryBackplane\nGenerationG10+\nPart NumberP55516-B21\n\n\n\nProducts ID1737159\nProduct TypeBackplane Kit",null,"g"]
["P55029-B21","Description:HP G11 1U x16 Low Profile Secondary Riser KitPart Number(s)\nOption Part# P55029-B21\n\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL365 G11 1U x16 Low Profile Secondary Riser Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryRiser Kit\nGenerationG11\nPart NumberP55029-B21\n\n\n\nProducts ID1736967\nProduct TypeRiser Kit",null,"g"]
["P54683-001","Description:HP 1TB 2.5-inch SFF SATA \nBusiness Critical (BC) 12Gb/s 7.2K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53563-B21\nSpare Part# P54683-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads?\n\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSATA BC HDD\nPart NumberP54683-001\n\n\n\nProducts ID1733273\nTypeHard Disk Drive\nCapacity1-TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nDrive CarrierBasic Carrier (BC)\nRPM7.2K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54683-001 SATA BC HDD Hard Disk Drive",null,"g"]
["P54682-001","Description:HP 1.8TB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53562-B21\nSpare Part# P54682-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP54682-001\n\n\n\nProducts ID733265\nTypeHard Disk Drive\nCapacity1.8TB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54682-001 SAS BC HDD Hard Disk Drive",null,"g"]
["P54681-001","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53561-B21\nSpare Part# P54681-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP54681-001\n\n\n\nProducts ID733257\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54681-001 SAS BC HDD Hard Disk Drive",null,"g"]
["P54680-001","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53560-B21\nSpare Part# P54680-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP54680-001\n\n\n\nProducts ID733249\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54680-001 SAS BC HDD Hard Disk Drive",null,"g"]
["P54679-001","Description:HP 20TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\nInstant Secure Erase (ISE) Helium (HE) Hot-Plug\nHard Drive in 3.5in LFF SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53555-B21\nSpare Part# P54679-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberP54679-001\n\n\n\nProducts ID1730515\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate600MB/s\nAverage Seek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54679-001 SATA SC 7.2K",null,"g"]
["P54678-001","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nInstant Secure Erase (ISE) Hot-Plug Hard Drive\nIn G10 (Gen10) G10+ (G10-Plus)\n Low Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53554-B21\nSpare Part# P54678-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SATA Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SATA interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP54678-001\n\n\n\nProducts ID731171\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54678-001 SATA LPc 7.2K",null,"g"]
["P54677-001","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53553-B21\nSpare Part# P54677-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP54677-001\n\n\n\nProducts ID730554\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54677-001 SAS SC 7.2K",null,"g"]
["P54676-001","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53552-B21\nSpare Part# P54676-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP54676-001\n\n\n\nProducts ID730507\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54676-001 SAS SC 7.2K",null,"g"]
["P54675-001","Description:HP 10TB 3.5-inch (LPc) SATA   6Gb/s  7.2K RPM\n512e Business Critical (BC) Digitally Signed (DS) LPc\nHot-Plug Hard Drive In G10 (Gen10) G10+ (G10-Plus) \nLow Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53559-B21\nSpare Part# P54675-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP54675-001\n\n\n\nProducts ID734934\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity10TB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nAverage Seek Time8.0ms\n \nNative Command QueuingSupported\nBytes/Sector512\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54675-001 SATA LPc 7.2K",null,"g"]
["P54674-001","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM Helium (He)\n512e Business Critical Instant Secure Erase (ISE)\nDigitally Signed (DS) Hot-Plug Hard Drive\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 G10 Proliant SAS Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53558-B21\nSpare Part# P54674-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP54674-001\n\n\n\nProducts ID1736762\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate12G = 12Gb/sec\nAverage Seek Time8.0ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54674-001 SAS SC 7.2K",null,"g"]
["P54673-001","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nBusiness Critical (BC) 512e Instant Secure Erase (ISE)\nLow Profile Carrier (LPc) Hot-Plug Hard Drive\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)\nHot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53557-B21\nSpare Part# P54673-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP54673-001\n\n\n\nProducts ID1734918\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54673-001 SATA LPc 7.2K",null,"g"]
["P54672-001","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53556-B21\nSpare Part# P54672-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP54672-001\n\n\n\nProducts ID730538\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P54672-001 SAS SC 7.2K",null,"g"]
["P53710-B21","Description:1 x AMD EPYC 9374F DL385 Gen11(3.85GHz/32-core/320W)\nPart Number(s)\nOption Part# P53710-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53710-B21\n\n\n\nProducts ID1736993\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed3.85GHz\nThermal Design Power320W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53710-B21 G11 EPYC",null,"g"]
["P53704-B21","Description:1 x AMD EPYC 9354P Gen11(3.25GHz/32-core/ 280W)\nPart Number(s)\nOption Part# P53704-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL325 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL325 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53704-B21\n\n\n\nProducts ID737130\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed3.25GHz\nThermal Design Power280W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53704-B21 G11 EPYC",null,"g"]
["P53703-B21","Description:1 x AMD EPYC 9554P Gen11(3.1GHz/64-core/ 360W)\nPart Number(s)\nOption Part# P53703-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL325 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL325 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53703-B21\n\n\n\nProducts ID1737131\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreTetrahexaconta-core\nProcessor Qty1\nClock Speed3.1GHz\nThermal Design Power360W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53703-B21 G11 EPYC",null,"g"]
["P53702-B21","Description:1 x AMD EPYC 9124 DL385 Gen11(3.0GHz/16-core/200W)\nPart Number(s)\nOption Part# P53702-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53702-B21\n\n\n\nProducts ID736987\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreHexadeca-Core\nProcessor Qty1\nClock Speed3.0GHz\nThermal Design Power200W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53702-B21 G11 EPYC",null,"g"]
["P53701-B21","Description:1 x AMD EPYC 9354 DL385 Gen11(3.25GHz/32-core/280W)\nPart Number(s)\nOption Part# P53701-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53701-B21\n\n\n\nProducts ID736989\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed3.25GHz\nThermal Design Power280W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53701-B21 G11 EPYC",null,"g"]
["P53700-B21","Description:1 x AMD EPYC 9554 DL385 Gen11(3.1GHz/64-core/360W)\nPart Number(s)\nOption Part# P53700-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53700-B21\n\n\n\nProducts ID736990\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreTetrahexaconta-core\nProcessor Qty1\nClock Speed3.1GHz\nThermal Design Power360W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53700-B21 G11 EPYC",null,"g"]
["P53698-B21","Description:1 x AMD EPYC 9174F DL385 Gen11(4.1GHz/16-core/320W)\nPart Number(s)\nOption Part# P53698-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53698-B21\n\n\n\nProducts ID736992\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreHexadeca-Core\nProcessor Qty1\nClock Speed4.1GHz\nThermal Design Power320W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53698-B21 G11 EPYC",null,"g"]
["P53697-B21","Description:1 x AMD EPYC 9654P Gen11(2.4GHz/96-core/ 360W)\nPart Number(s)\nOption Part# P53697-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL325 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53697-B21\n\n\n\nProducts ID737132\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor Corehexanonaconta-core\nProcessor Qty1\nClock Speed2.4GHz\nThermal Design Power360W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53697-B21 G11 EPYC",null,"g"]
["P53696-B21","Description:1 x AMD EPYC 9654 DL385 Gen11(2.4GHz/96-core/360W)\nPart Number(s)\nOption Part# P53696-B21Note:\nThis processor does not include a fan kit or a heat sink kit.\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe new HPE ProLiant DL385 Gen11 server is an acceleratoroptimized 2U 2P solution that delivers exceptional compute performance upgraded high-speed data transfer rate and memory depth at 2P compute capability. Powered by 4th Generation AMD EPYC™ 9004 Series Processors with up to 96 cores increased memory bandwidth (up to 6TB), high-speed PCIe Gen5 I/O Gen5 EDSFF storage and the newly designed chassis supporting 8 single wide (SW) or 4 double wide (DW) GPUs*. The HPE ProLiant DL385 Gen11 server is a perfect accelerator-optimized 2U 2P solution. \n\nSpecifications:\nCategoryProliant AMD Processor\nSub-CategoryEPYC\nGenerationG11\nPart NumberP53696-B21\n\n\n\nProducts ID736991\nProduct TypeProcessor Upgrade\nProcessor TypeAMD EPYC\nProcessor CoreHexanonaconta-core\nProcessor Qty1\nClock Speed2.4GHz\nThermal Design Power360W\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53696-B21 G11 EPYC",null,"g"]
["P53563-K21","Description:HP 1TB 2.5-inch SFF SATA \nBusiness Critical (BC) 12Gb/s 7.2K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53563-K21\nSpare Part# P54683-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads?\n\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSATA BC HDD\nPart NumberP53563-K21\n\n\n\nProducts ID734886\nTypeHard Disk Drive\nCapacity1-TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nDrive CarrierBasic Carrier (BC)\nRPM7.2K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53563-K21 SATA BC HDD Hard Disk Drive",null,"g"]
["P53563-H21","Description:HP 1TB 2.5-inch SFF SATA \nBusiness Critical (BC) 12Gb/s 7.2K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53563-H21\nSpare Part# P54683-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads?\n\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSATA BC HDD\nPart NumberP53563-H21\n\n\n\nProducts ID734882\nTypeHard Disk Drive\nCapacity1-TB\nInterface TypeSATA\nDrive Interface Standard6Gb/s SATA\nDrive CarrierBasic Carrier (BC)\nRPM7.2K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53563-H21 SATA BC HDD Hard Disk Drive",null,"g"]
["P53563-B21","Description:HP 1TB 2.5-inch SFF SATA \nBusiness Critical (BC) 12Gb/s 7.2K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53563-B21\nSpare Part# P54683-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads?\n\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA BC HDD\nPart NumberP53563-B21\n\n\n\nProducts ID733269\nTypeHard Disk Drive\nCapacity1-TB\nInterface TypeSATA\nDrive Interface Standard12Gb/s SATA\nDrive CarrierBasic Carrier (BC)\nRPM7.2K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53563-B21 SATA BC HDD 7.2K",null,"g"]
["P53562-H21","Description:HP 1.8TB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53562-H21\nSpare Part# P54682-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP53562-H21\n\n\n\nProducts ID734626\nTypeHard Disk Drive\nCapacity1.8TB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53562-H21 SAS BC HDD Hard Disk Drive",null,"g"]
["P53562-B21","Description:HP 1.8TB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53562-B21\nSpare Part# P54682-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS BC HDD\nPart NumberP53562-B21\n\n\n\nProducts ID733261\nTypeHard Disk Drive\nCapacity1.8TB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53562-B21 SAS BC HDD 15K",null,"g"]
["P53561-K21","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53561-K21\nSpare Part# P54681-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP53561-K21\n\n\n\nProducts ID1734622\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53561-K21 SAS BC HDD Hard Disk Drive",null,"g"]
["P53561-B21","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53561-B21\nSpare Part# P54681-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS BC HDD\nPart NumberP53561-B21\n\n\n\nProducts ID733253\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53561-B21 SAS BC HDD 15K",null,"g"]
["P53560-K21","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53560-K21\nSpare Part# P54680-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategoryHard Disk Drive\nGenerationSAS BC HDD\nPart NumberP53560-K21\n\n\n\nProducts ID1734630\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53560-K21 SAS BC HDD Hard Disk Drive",null,"g"]
["P53560-B21","Description:HP 600GB 2.5-inch SFF SAS \nMission Critical (MC) 12Gb/s 15K RPM\nDigitally Signed Firmware (DS) Hard Drive\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53560-B21\nSpare Part# P54680-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your servers need high-performance enterprise hard drives for both your mission-critical and I/O-intensive applications?\n\nHPE Server Enterprise Hard Drives offer the highest level of performance and reliability for your most demanding application workloads. Enterprise drives help you improve server response times - power more transactions per second - and accelerate data transfer (I/O) speeds. HPE Server Enterprise Hard Drives are backed by over 3.35 million hours of the industry’s most rigorous testing and qualification program - ensuring customers reliable - rugged drives. Prevent unauthorized access to your data with HPE Digitally Signed Firmware. It provides the security and assurance that drive firmware comes from a trusted source and protects against malicious attacks.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category15K\nGenerationSAS BC HDD\nPart NumberP53560-B21\n\n\n\nProducts ID1733245\nTypeHard Disk Drive\nCapacity600-GB\nInterface TypeSAS\nDrive Interface Standard12Gb/s SAS\nDrive CarrierBasic Carrier (BC)\nRPM15K\nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53560-B21 SAS BC HDD 15K",null,"g"]
["P53559-K21","Description:HP 10TB 3.5-inch (LPc) SATA   6Gb/s  7.2K RPM\n512e Business Critical (BC) Digitally Signed (DS) LPc\nHot-Plug Hard Drive In G10 (Gen10) G10+ (G10-Plus) \nLow Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53559-K21\nSpare Part# P54675-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53559-K21\n\n\n\nProducts ID734938\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity10TB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nAverage Seek Time8.0ms\n \nNative Command QueuingSupported\nBytes/Sector512\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53559-K21 SATA LPc 7.2K",null,"g"]
["P53559-B21","Description:HP 10TB 3.5-inch (LPc) SATA   6Gb/s  7.2K RPM\n512e Business Critical (BC) Digitally Signed (DS) LPc\nHot-Plug Hard Drive In G10 (Gen10) G10+ (G10-Plus) \nLow Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53559-B21\nSpare Part# P54675-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53559-B21\n\n\n\nProducts ID1734930\nTypeHard Drive - Hot-Swap - Gen8\nLarge Form Factor3.5 inches\nCapacity10TB\nInterface TypeSerial ATA\nConnector22-Position Serial ATA (SATA) Plug\nData Transfer Rate6G = 6Gb/sec (750 MB/s)\nSpindle Speed7200RPM\nAverage Seek Time8.0ms\n \nNative Command QueuingSupported\nBytes/Sector512\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53559-B21 SATA LPc 7.2K",null,"g"]
["P53558-B21","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s 7.2K RPM Helium (He)\n512e Business Critical Instant Secure Erase (ISE)\nDigitally Signed (DS) Hot-Plug Hard Drive\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)\n Hot-Plug SmartDrive Carrier (SC) (as pictured)\nFor HP G8 G9 G10 Proliant SAS Servers and Storage ArraysGenuine HP serial number and firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53558-B21\nSpare Part# P54674-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53558-B21\n\n\n\nProducts ID1736758\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate12G = 12Gb/sec\nAverage Seek Time8.0ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53558-B21 SAS SC 7.2K",null,"g"]
["P53557-K21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nBusiness Critical (BC) 512e Instant Secure Erase (ISE)\nLow Profile Carrier (LPc) Hot-Plug Hard Drive\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)\nHot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53557-K21\nSpare Part# P54673-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53557-K21\n\n\n\nProducts ID1734922\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53557-K21 SATA LPc 7.2K",null,"g"]
["P53557-H21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nBusiness Critical (BC) 512e Instant Secure Erase (ISE)\nLow Profile Carrier (LPc) Hot-Plug Hard Drive\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)\nHot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53557-H21\nSpare Part# P54673-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53557-H21\n\n\n\nProducts ID1734926\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53557-H21 SATA LPc 7.2K",null,"g"]
["P53557-B21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nBusiness Critical (BC) 512e Instant Secure Erase (ISE)\nLow Profile Carrier (LPc) Hot-Plug Hard Drive\nIn HP G10 G10+ G11 (Gen10 Gen10-Plus Gen11)\nHot-Plug Low Profile Carrier (LPc) (as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53557-B21\nSpare Part# P54673-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE Business Critical Hard Drives are engineered to deliver the highest capacity performance reliability and data security across your data center applications. HPE Business Critical Hard Drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53557-B21\n\n\n\nProducts ID734914\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53557-B21 SATA LPc 7.2K",null,"g"]
["P53556-K21","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53556-K21\nSpare Part# P54672-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53556-K21\n\n\n\nProducts ID1730546\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53556-K21 SAS SC 7.2K",null,"g"]
["P53556-H21","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53556-H21\nSpare Part# P54672-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53556-H21\n\n\n\nProducts ID730542\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53556-H21 SAS SC 7.2K",null,"g"]
["P53556-B21","Description:HP 10TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53556-B21\nSpare Part# P54672-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53556-B21\n\n\n\nProducts ID1730534\nCapacity10TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53556-B21 SAS SC 7.2K",null,"g"]
["P53555-K21","Description:HP 20TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\nInstant Secure Erase (ISE) Helium (HE) Hot-Plug\nHard Drive in 3.5in LFF SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53555-K21\nSpare Part# P54679-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberP53555-K21\n\n\n\nProducts ID734862\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate600MB/s\nAverage Seek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53555-K21 SATA SC 7.2K",null,"g"]
["P53555-B21","Description:HP 20TB 3.5-inch LFF SATA   6Gb/s  7.2K RPM\nInstant Secure Erase (ISE) Helium (HE) Hot-Plug\nHard Drive in 3.5in LFF SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certified Hard Drive\nPart Number(s)\nOption Part# P53555-B21\nSpare Part# P54679-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SAS Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SAS Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SAS interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA SC\nPart NumberP53555-B21\n\n\n\nProducts ID1730511\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches\nRotational Speed7200RPM\nData Transfer Rate600MB/s\nAverage Seek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53555-B21 SATA SC 7.2K",null,"g"]
["P53554-K21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nInstant Secure Erase (ISE) Hot-Plug Hard Drive\nIn G10 (Gen10) G10+ (G10-Plus)\n Low Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53554-K21\nSpare Part# P54678-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SATA Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SATA interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53554-K21\n\n\n\nProducts ID734870\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53554-K21 SATA LPc 7.2K",null,"g"]
["P53554-H21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nInstant Secure Erase (ISE) Hot-Plug Hard Drive\nIn G10 (Gen10) G10+ (G10-Plus)\n Low Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmware\nGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53554-H21\nSpare Part# P54678-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SATA Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SATA interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53554-H21\n\n\n\nProducts ID734874\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53554-H21 SATA LPc 7.2K",null,"g"]
["P53554-B21","Description:HP 20TB 3.5-inch SATA 6Gb/s 7.2K RPM Helium (He)\nInstant Secure Erase (ISE) Hot-Plug Hard Drive\nIn G10 (Gen10) G10+ (G10-Plus)\n Low Profile Carrier (LPc)(as pictured)\nDesigned for select HP Proliant SATA Servers with\n3.5-inch Low Profile Carrier (LPc) Drive Bays\nGenuine HP serial number and Digitally Signed  firmwareGenuine HP Certified Hard DrivePart Number(s)\nOption Part# P53554-B21\nSpare Part# P54678-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP SATA Enterprise and Midline Hard Drives deliver high performance solutions for hosting high transaction based applications. Available in HP hot plug carriers or non-hot plug. The HP SATA Enterprise and Midline Hard Drives come in both 2.5in (SFF) and 3.5in (LFF) industry standard form factors and are available in a variety of capacity points to meet a wide range of requirements. The SATA interface was designed and engineered for high availability - enterprise-class data storage where performance - reliability and data integrity are crucial.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSATA LPc\nPart NumberP53554-B21\n\n\n\nProducts ID1731167\nCapacity20TB\nInterfaceSerial ATA (SATA)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate6G = 6Gb/sec\nSeek Time8.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53554-B21 SATA LPc 7.2K",null,"g"]
["P53553-K21","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53553-K21\nSpare Part# P54677-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53553-K21\n\n\n\nProducts ID1734858\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53553-K21 SAS SC 7.2K",null,"g"]
["P53553-H21","Description:2 x HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53553-H21\nSpare Part# P54677-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53553-H21\n\n\n\nProducts ID734879\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53553-H21 SAS SC 7.2K",null,"g"]
["P53553-B21","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53553-B21\nSpare Part# P54677-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53553-B21\n\n\n\nProducts ID730550\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53553-B21 SAS SC 7.2K",null,"g"]
["P53552-K21","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53552-K21\nSpare Part# P54676-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53552-K21\n\n\n\nProducts ID1734866\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53552-K21 SAS SC 7.2K",null,"g"]
["P53552-B21","Description:HP 20TB 3.5-inch LFF SAS 12Gb/s  7.2K RPM\n512e Business Critical (BC) Helium (He)Multi Vendor (MV)\nInstant Secure Erase (ISE)\nHot-Plug Hard Drive SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and firmware\nGenuine HP Certifed Hard Drive\nPart Number(s)\nOption Part# P53552-B21\nSpare Part# P54676-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo your HPE servers and storage platforms need high capacity and proven performance hard drives to optimize your business critical data storage workloads. HPE Business Critical Hard Drives are engineered to deliver the highest capacity - performance - reliability and data security across your data center applications. Business Critical hard drives allow you to store more data without sacrificing performance or reliability. HPE Business Critical Hard Drives are available in both 3.5-inch Large Form Factor (LFF) and 2.5-inch Small Form Factor (SFF) and ship with a standard one-year warranty. All HPE hard drives pass a rigorous qualification process - which certify that every drive is proven to perform in your HPE server and storage environments. All HPE hard drives include digitally signed firmware which helps prevent unauthorized access to your data.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-Category7.2K\nGenerationSAS SC\nPart NumberP53552-B21\n\n\n\nProducts ID1730503\nCapacity20TB\nInterfaceSerial Attached SCSI (SAS)\nEnclosureInternal\nDrive Dimensions3.5 inches x 1/3H (Low Profile)\nSpindle Speed7200RPM\nData Transfer Rate12G = 12Gb/sec (750 MB/s)\nSeek Time3.5ms\nHotSwapYes\n \nManufacturerHewlett Packard\nPre-Failure WarrantyYes\n \nHot Swap TrayIncluded/Attached\n\n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P53552-B21 SAS SC 7.2K",null,"g"]
["P53226-001","Description:HP ProLiant DL365 Gen11 1U Standard Fan KitPart Number(s)\nOption Part# P58461-B21\nSpare Part# P53226-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Standard Fan Module for works in HPE ProLiant DL300 series Gen11 Servers.\n\nSpecifications:\nCategoryHP\nSub-CategoryFan Option\nGenerationGen11\nPart NumberP53226-001\n\n\n\nProducts ID736970\nHeight (Rack Units)1U",null,"g"]
["P53225-001","Description:HP DL325 Gen11 Liquid Cooling Fan Kit\nPart Number(s)\nOption Part# P59668-B21\nSpare Part# P53225-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL325 G11 Liquid Cooling Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP53225-001\n\n\n\nProducts ID1737911\nProduct TypeFan Kit",null,"g"]
["P52792-001","Description:HP ML350 Gen11 Redundant Fan Cage Kit\nPart Number(s)\nOption Part# P47219-B21\nSpare Part# P52792-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nML350 Gen11 Redundant Fan Cage Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG10\nPart NumberP52792-001\n\n\n\nProducts ID738328\nProduct TypeFan Kit",null,"g"]
["P52434-001","Description:HP DL3X5 G11 2U Standard Fan Kit\nPart Number(s)\nOption Part# P58465-B21\nSpare Part# P52434-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP DL3X5 G11 2U Standard Fan Kit\n\nSpecifications:\nCategoryProliant\nSub-CategoryFan Kit\nGenerationG11\nPart NumberP52434-001\n\n\n\nProducts ID737915\nProduct TypeFan Kit",null,"g"]
["P52333-001","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51463-B21\nSpare Part# P52333-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52333-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733241\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52333-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52332-001","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51462-B21\nSpare Part# P52332-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52332-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733233\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52332-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52331-001","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51461-B21\nSpare Part# P52331-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52331-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733225\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52331-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52330-001","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51460-B21\nSpare Part# P52330-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52330-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733217\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52330-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52329-001","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4\nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS)HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51459-B21\nSpare Part# P52329-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52329-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733209\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52329-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52328-001","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51458-B21\nSpare Part# P52328-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52328-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733201\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52328-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52327-001","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51457-B21\nSpare Part# P52327-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52327-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733193\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52327-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52326-001","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51456-B21\nSpare Part# P52326-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52326-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733185\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52326-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52325-001","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51455-B21\nSpare Part# P52325-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52325-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733177\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52325-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52324-001","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51454-B21\nSpare Part# P52324-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52324-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733169\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52324-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52323-001","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) NVMe Solid State Drive (SSD) in\nG10 G10+ (Gen10 G10-Plus Gen10-Plus) Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51453-B21\nSpare Part# P52323-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52323-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733161\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52323-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52322-001","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51452-B21\nSpare Part# P52322-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52322-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733153\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52322-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P52109-001","Description:HP 800GB 2.5-inch SFF NVMe x4 Lanes SSD\nHigh Performance (HP) Low Latency (LL)\nWrite-Intensive (WI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD)In G10+ G11 (G10-Plus Gen 11) Hot-Plug \nHP Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51467-B21\nSpare Part# P52109-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Low Latency (LL) Write Intensive (WI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance Low Latency WI SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP52109-001\n\nBest Use:    Write-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1734086\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity800GB\nInterface TypeNVMe\nWorkload TypeWrite Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52109-001 NVMe BC SSD Solid State Drive",null,"g"]
["P52106-001","Description:HP 400GB 2.5-inch SFF NVMe x4 Lanes SSD\nHigh Performance (HP) Low Latency (LL)\nWrite-Intensive (WI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51464-B21\nSpare Part# P52106-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Low Latency (LL) Write Intensive (WI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance Low Latency WI SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP52106-001\n\nBest Use:    Write-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733290\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity400GB\nInterface TypeNVMe\nWorkload TypeWrite Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P52106-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P51467-B21","Description:HP 800GB 2.5-inch SFF NVMe x4 Lanes SSD\nHigh Performance (HP) Low Latency (LL)\nWrite-Intensive (WI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD)In G10+ G11 (G10-Plus Gen 11) Hot-Plug \nHP Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51467-B21\nSpare Part# P52109-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Low Latency (LL) Write Intensive (WI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance Low Latency WI SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51467-B21\n\nBest Use:    Write-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID734082\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity800GB\nInterface TypeNVMe\nWorkload TypeWrite Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51467-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51464-K21","Description:HP 400GB 2.5-inch SFF NVMe x4 Lanes SSD\nHigh Performance (HP) Low Latency (LL)\nWrite-Intensive (WI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51464-K21\nSpare Part# P52106-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Low Latency (LL) Write Intensive (WI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance Low Latency WI SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51464-K21\n\nBest Use:    Write-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1734090\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity400GB\nInterface TypeNVMe\nWorkload TypeWrite Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51464-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51464-B21","Description:HP 400GB 2.5-inch SFF NVMe x4 Lanes SSD\nHigh Performance (HP) Low Latency (LL)\nWrite-Intensive (WI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)In HP G9 G10 (Gen9 Gen10)\nHot-Plug SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51464-B21\nSpare Part# P52106-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe High Performance (HP) Low Latency (LL) Write Intensive (WI) Solid State Drives (SSDs) deliver an industry-leading combination of high throughput - low latency - high QoS - and high endurance which is optimized to break through data access bottlenecks. HPE NVMe High Performance Low Latency WI SSDs are based on P4800X SSDs featuring 3D XPoint technology. They deliver extremely low latency to accelerate applications for fast caching and fast storage to increase scale per server and reduce transaction costs for latency-sensitive workloads.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51464-B21\n\nBest Use:    Write-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733286\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity400GB\nInterface TypeNVMe\nWorkload TypeWrite Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51464-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51463-K21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51463-K21\nSpare Part# P52333-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51463-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734397\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51463-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51463-B21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51463-B21\nSpare Part# P52333-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51463-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733237\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51463-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51462-K21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51462-K21\nSpare Part# P52332-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51462-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734405\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51462-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51462-B21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51462-B21\nSpare Part# P52332-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51462-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733229\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51462-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51461-K21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51461-K21\nSpare Part# P52331-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51461-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734401\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51461-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51461-B21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51461-B21\nSpare Part# P52331-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51461-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733221\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51461-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51460-K21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51460-K21\nSpare Part# P52330-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51460-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734393\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51460-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51460-B21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51460-B21\nSpare Part# P52330-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51460-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733213\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51460-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51459-K21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS)HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51459-K21\nSpare Part# P52329-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51459-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734389\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51459-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51459-B21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Mixed-Use (MU)\nDigitally Signed Firmware (DS)HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51459-B21\nSpare Part# P52329-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51459-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1733205\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51459-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51458-K21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51458-K21\nSpare Part# P52328-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51458-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734385\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51458-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51458-H21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51458-H21\nSpare Part# P52328-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51458-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734381\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51458-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51458-B21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51458-B21\nSpare Part# P52328-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51458-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID733197\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51458-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51457-K21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51457-K21\nSpare Part# P52327-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51457-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733846\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51457-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51457-B21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51457-B21\nSpare Part# P52327-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51457-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733189\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51457-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51456-K21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe SCN Solid State Drive (SSD)\nIn G9 G10 (Gen9 Gen10)\nHot-Swap SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51456-K21\nSpare Part# P52326-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51456-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733858\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51456-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51456-B21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe SCN Solid State Drive (SSD)\nIn G9 G10 (Gen9 Gen10)\nHot-Swap SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51456-B21\nSpare Part# P52326-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51456-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733181\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51456-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51455-K21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51455-K21\nSpare Part# P52325-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51455-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733850\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51455-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51455-B21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) HP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51455-B21\nSpare Part# P52325-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51455-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733173\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51455-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51454-K21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51454-K21\nSpare Part# P52324-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51454-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733854\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51454-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51454-B21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51454-B21\nSpare Part# P52324-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51454-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733165\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51454-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51453-K21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) NVMe Solid State Drive (SSD) in\nG10 G10+ (Gen10 G10-Plus Gen10-Plus) Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51453-K21\nSpare Part# P52323-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51453-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733862\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51453-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P51453-B21","Description:HP 1.92TB 2.5-inch SFF NVMe  PCIe Gen4\nU.2 SSD High Performance (HP) Read-Intensive (RI)\nDigitally Signed Firmware (DS) NVMe Solid State Drive (SSD) in\nG10 G10+ (Gen10 G10-Plus Gen10-Plus) Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe BC SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51453-B21\nSpare Part# P52323-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS- low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage- at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching- web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP51453-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733157\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51453-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P51452-K21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51452-K21\nSpare Part# P52322-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51452-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733838\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51452-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51452-H21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51452-H21\nSpare Part# P52322-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51452-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733842\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51452-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51452-B21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.2 SSD\nHigh Performance (HP) Read-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P51452-B21\nSpare Part# P52322-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.2 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification1 ensuring reliable high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP51452-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733149\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.2\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P51452-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P51305-001","Description:HP Broadcom BCM5719 Ethernet 4-Port 1Gb/s BASE-T OCP3 AdapterPart Number(s)\nOption Part# P51181-B21\nSpare Part# P51305-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Gen10 Plus Ethernet adapters are 1 Gb 10 Gb 10/25 Gb 100 Gb and 200 Gb Ethernet solutions that are scalable and compatible with HPE Gen10 Plus servers for hybrid cloud services, mobile data and streaming video applications.\nYour server is the foundation of your data center but it doesn’t work alone. When one link in your component chain slows down so does the rest of your operation. Keep your network and data flowing with a seamless ecosystem of HPE servers networking adapters transceivers cables, and switches.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationPCI-e\nPart NumberP51305-001\n\n\n\nProducts ID1735331\nDevice TypeNetwork Adapter\nPorts4",null,"g"]
["P51304-001","Description:HP Broadcom BCM5719 Ethernet 4-Port 1Gb BASE-T AdapterPart Number(s)\nOption Part# P51178-B21\nSpare Part# P51304-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Gen10 Plus Ethernet adapters are 1 Gb 10 Gb 10/25 Gb 100 Gb and 200 Gb Ethernet solutions that are scalable and compatible with HPE Gen10 Plus servers for hybrid cloud services, mobile data and streaming video applications.\nYour server is the foundation of your data center but it doesn’t work alone. When one link in your component chain slows down so does the rest of your operation. Keep your network and data flowing with a seamless ecosystem of HPE servers networking adapters transceivers cables, and switches.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationPCI-e\nPart NumberP51304-001\n\n\n\nProducts ID735329\nDevice TypeNetwork Adapter\nPorts4",null,"g"]
["P51181-B21","Description:HP Broadcom BCM5719 Ethernet 4-Port 1Gb BASE-T OCP3 AdapterPart Number(s)\nOption Part# P51181-B21\nSpare Part# P51305-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Gen10 Plus Ethernet adapters are 1 Gb 10 Gb 10/25 Gb 100 Gb and 200 Gb Ethernet solutions that are scalable and compatible with HPE Gen10 Plus servers for hybrid cloud services, mobile data and streaming video applications.\nYour server is the foundation of your data center but it doesn’t work alone. When one link in your component chain slows down so does the rest of your operation. Keep your network and data flowing with a seamless ecosystem of HPE servers networking adapters transceivers cables, and switches.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationPCI-e\nPart NumberP51181-B21\n\n\n\nProducts ID1735330\nDevice TypeNetwork Adapter\nPorts4",null,"g"]
["P51178-B21","Description:HP Broadcom BCM5719 Ethernet 4-Port 1Gb BASE-T AdapterPart Number(s)\nOption Part# P51178-B21\nSpare Part# P51304-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nThe HPE Gen10 Plus Ethernet adapters are 1 Gb 10 Gb 10/25 Gb 100 Gb and 200 Gb Ethernet solutions that are scalable and compatible with HPE Gen10 Plus servers for hybrid cloud services, mobile data and streaming video applications.\nYour server is the foundation of your data center but it doesn’t work alone. When one link in your component chain slows down so does the rest of your operation. Keep your network and data flowing with a seamless ecosystem of HPE servers networking adapters transceivers cables, and switches.\n\nSpecifications:\nCategoryHP Networking\nSub-CategoryEthernet Adapter\nGenerationPCI-e\nPart NumberP51178-B21\n\n\n\nProducts ID735328\nDevice TypeNetwork Adapter\nPorts4",null,"g"]
["P50970-001","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50233-B21\nSpare Part# P50970-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50970-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731398\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50970-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50969-001","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.3 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50232-B21\nSpare Part# P50969-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50969-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734369\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50969-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50968-001","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50231-B21\nSpare Part# P50968-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50968-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID731229\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50968-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50967-001","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50230-B21\nSpare Part# P50967-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50967-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731386\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50967-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50966-001","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50229-B21\nSpare Part# P50966-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50966-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734441\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50966-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50965-001","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50228-B21\nSpare Part# P50965-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe Mainstream Performance (MP) Mixed Use (MU) Solid State Drives are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe Mainstream Performance (MP) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads requiring outstanding IOPS per watt and cost per IOPS as an upgrade from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50965-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731237\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50965-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50964-001","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50227-B21\nSpare Part# P50964-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50964-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID731378\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50964-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50963-001","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50226-B21\nSpare Part# P50963-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50963-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734425\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50963-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50962-001","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50225-B21\nSpare Part# P50962-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe Mainstream Performance (MP) Mixed Use (MU) Solid State Drives are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe Mainstream Performance (MP) SSDs are advanced data center drives optimized for greater performance and endurance in a cost-effective design. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads requiring outstanding IOPS per watt and cost per IOPS as an upgrade from SATA SSDs.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50962-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731245\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50962-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50961-001","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50224-B21\nSpare Part# P50961-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50961-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731370\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50961-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50960-001","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50223-B21\nSpare Part# P50960-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50960-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733954\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50960-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50959-001","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50222-B21\nSpare Part# P50959-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50959-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731277\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50959-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50958-001","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50221-B21\nSpare Part# P50958-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50958-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733990\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50958-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50957-001","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50220-B21\nSpare Part# P50957-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50957-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731269\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50957-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50956-001","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50219-B21\nSpare Part# P50956-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50956-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731293\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50956-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50955-001","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50218-B21\nSpare Part# P50955-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50955-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733830\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50955-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50954-001","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50217-B21\nSpare Part# P50954-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50954-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731261\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50954-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50953-001","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50216-B21\nSpare Part# P50953-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50953-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731285\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50953-001 NVMe BC SSD Solid State Drive",null,"g"]
["P50952-001","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50215-B21\nSpare Part# P50952-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50952-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID734006\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50952-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50951-001","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50214-B21\nSpare Part# P50951-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50951-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731253\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50951-001 NVMe SCN SSD Solid State Drive",null,"g"]
["P50312-B21","Description:HPE 64GB (1 x64GB) Dual Rank x4 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50312-B21\nSpare Part# P56153-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P50312-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen11\nPart NumberP50312-B21\n\n\n\nProducts ID736965\nProduct TypeMemory Module\nMemory Size64GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 64GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50312-B21 Gen11 Genuine HP Memory",null,"g"]
["P50311-B21","Description:HPE 32GB (1 x32GB) Dual Rank x8 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50311-B21\nSpare Part# P56152-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P50311-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen11\nPart NumberP50311-B21\n\n\n\nProducts ID1736963\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50311-B21 Gen11 Genuine HP Memory",null,"g"]
["P50310-B21","Description:HPE 32GB (1 x32GB) Single Rank x4 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50310-B21\nSpare Part# P56151-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P50310-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen 11\nPart NumberP50310-B21\n\n\n\nProducts ID1736961\nProduct TypeMemory Module\nMemory Size32GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 32GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50310-B21 Gen 11 Genuine HP Memory",null,"g"]
["P50309-B21","Description:HPE 16GB (1 x16GB) Single Rank x8 DDR5-4800\nCAS-42-42-42 EC8 Registered Smart Memory Kit\n\nPart Number(s)\nOption Part# P50309-B21\nSpare Part# P56150-001\n\n\n\n\n\n\n\n\n \n\n \n\n\nNote:Our HP Part# P50309-B21 is guaranteed genuine\nHP product with a HP serial number and logo.\nWe do not sell 3rd party HP memory.\n \n\n \n\n \n\n \n\n\nOverview:\nHP DDR5 SmartMemory delivers on great performance - reliability - and efficiency. Our large selection of server memory solutions provides the compatibility - capacity and bandwidth you need to productively manage your expanding workload with the HP Proliant Gen11 and Gen10 server - Apollo Family - Synergy and Blade Systems.\n\nSpecifications:\nCategoryProliant Memory\nSub-CategoryGenuine HP Memory\nGenerationGen 11\nPart NumberP50309-B21\n\n\n\nProducts ID1736959\nProduct TypeMemory Module\nMemory Size16GB\nMemory TechnologyDDR4 SDRAM\nNumber of Modules1 x 16GB\nMemory StandardDDR5-4800\nSignal ProcessingRegistered\nForm Factor288-pin RDIMM\nError CheckingECC\n \nManufacturerHewlett Packard\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\nApplicationServer Memory\nServer ModelHP Proliant\nCompatibilityHP Proliant Servers\nManufacturerHewlett-Packard\nHP Serial NumberYes\nHP LogoYes\nGuaranteed Genuine HPYes\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50309-B21 Gen 11 Genuine HP Memory",null,"g"]
["P50233-K21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50233-K21\nSpare Part# P50970-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50233-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734469\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50233-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50233-H21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50233-H21\nSpare Part# P50970-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50233-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734473\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50233-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50233-B21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50233-B21\nSpare Part# P50970-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50233-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731394\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50233-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50232-H21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.3 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50232-H21\nSpare Part# P50969-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50232-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734373\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50232-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50232-B21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 U.3 SSD\nHigh Performance (HP) Mixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50232-B21\nSpare Part# P50969-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50232-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734365\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50232-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50231-K21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50231-K21\nSpare Part# P50968-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50231-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734477\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50231-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50231-H21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50231-H21\nSpare Part# P50968-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50231-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734377\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50231-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50231-B21","Description:HP 6.4TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50231-B21\nSpare Part# P50968-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50231-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID731225\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity6.4TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50231-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50230-K21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50230-K21\nSpare Part# P50967-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50230-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734417\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50230-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50230-H21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50230-H21\nSpare Part# P50967-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50230-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734433\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50230-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50230-B21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50230-B21\nSpare Part# P50967-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50230-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731382\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50230-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50229-H21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50229-H21\nSpare Part# P50966-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50229-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734461\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50229-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50229-B21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50229-B21\nSpare Part# P50966-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50229-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734437\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50229-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50228-K21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50228-K21\nSpare Part# P50965-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50228-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734429\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50228-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50228-H21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50228-H21\nSpare Part# P50965-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50228-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734409\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50228-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50228-B21","Description:HP 3.2TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50228-B21\nSpare Part# P50965-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50228-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID731233\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.2TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50228-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50227-K21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50227-K21\nSpare Part# P50964-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50227-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734413\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50227-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50227-H21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50227-H21\nSpare Part# P50964-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50227-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734481\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50227-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50227-B21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50227-B21\nSpare Part# P50964-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\n\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics-HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50227-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1731374\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50227-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50226-H21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50226-H21\nSpare Part# P50963-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50226-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734449\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50226-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50226-B21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50226-B21\nSpare Part# P50963-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50226-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734421\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50226-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50225-K21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50225-K21\nSpare Part# P50962-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50225-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734465\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50225-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50225-H21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50225-H21\nSpare Part# P50962-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50225-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734445\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50225-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50225-B21","Description:HP 1.6TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1735a SSD High Performance (HP)\nMixed-Use (MU) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50225-B21\nSpare Part# P50962-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Mixed Use (MU) SSDs are best suited for high I/O applications that require a balanced performance between reads and writes to deliver high performance and endurance for data intensive applications. NVMe High Performance MU SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency.\nHPE NVMe High Performance MU SSDs deliver high performance, lower latency data transfers from storage significantly faster than SAS or SATA SSDs. Utilizes the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for mixed use workloads such as Big Data analytics HPC and virtualization.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50225-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID731241\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.6TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeMixed Use\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50225-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50224-K21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50224-K21\nSpare Part# P50961-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50224-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733890\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50224-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50224-H21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50224-H21\nSpare Part# P50961-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50224-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733922\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50224-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50224-B21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50224-B21\nSpare Part# P50961-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50224-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731366\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50224-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50223-H21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50223-H21\nSpare Part# P50960-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50223-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733962\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50223-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50223-B21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50223-B21\nSpare Part# P50960-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50223-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733950\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50223-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50222-K21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50222-K21\nSpare Part# P50959-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50222-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733946\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50222-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50222-H21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50222-H21\nSpare Part# P50959-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50222-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733958\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50222-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50222-B21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50222-B21\nSpare Part# P50959-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50222-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731273\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50222-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50221-H21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50221-H21\nSpare Part# P50958-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50221-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733994\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50221-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50221-B21","Description:HP 15.36TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50221-B21\nSpare Part# P50958-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50221-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733986\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity15.36TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50221-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50220-K21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50220-K21\nSpare Part# P50957-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50220-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733970\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50220-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50220-H21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50220-H21\nSpare Part# P50957-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50220-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733998\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50220-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50220-B21","Description:HP 7.68TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50220-B21\nSpare Part# P50957-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50220-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731265\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity7.68TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50220-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50219-K21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50219-K21\nSpare Part# P50956-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50219-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733814\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50219-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50219-H21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50219-H21\nSpare Part# P50956-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50219-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733822\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50219-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50219-B21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50219-B21\nSpare Part# P50956-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50219-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731289\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50219-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50218-H21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50218-H21\nSpare Part# P50955-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50218-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733834\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50218-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50218-B21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50218-B21\nSpare Part# P50955-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50218-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733826\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50218-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50217-K21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50217-K21\nSpare Part# P50954-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50217-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733818\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50217-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50217-H21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50217-H21\nSpare Part# P50954-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50217-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733926\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50217-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50217-B21","Description:HP 3.84TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50217-B21\nSpare Part# P50954-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50217-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731257\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity3.84TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50217-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50216-K21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50216-K21\nSpare Part# P50953-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50216-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733974\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50216-K21 NVMe BC SSD Solid State Drive",null,"g"]
["P50216-H21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50216-H21\nSpare Part# P50953-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50216-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733978\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50216-H21 NVMe BC SSD Solid State Drive",null,"g"]
["P50216-B21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nHP NVMe Solid State Drive (SSD)\nIn G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Swap Basic Carrier (BC) (as pictured) \nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50216-B21\nSpare Part# P50953-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe BC SSD\nPart NumberP50216-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID731281\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeBC\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50216-B21 NVMe BC SSD Solid State Drive",null,"g"]
["P50215-H21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50215-H21\nSpare Part# P50952-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50215-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1734010\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50215-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50215-B21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50215-B21\nSpare Part# P50952-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50215-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID734002\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50215-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50214-K21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50214-K21\nSpare Part# P50951-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50214-K21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1733966\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50214-K21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50214-H21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50214-H21\nSpare Part# P50951-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50214-H21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID733982\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50214-H21 NVMe SCN SSD Solid State Drive",null,"g"]
["P50214-B21","Description:HP 1.92TB 2.5-inch SFF NVMe x4 Lanes PCIe Gen4 \nU.3 PM1733a SSD High Performance (HP)\nRead-Intensive (RI) Digitally Signed Firmware (DS)\nNVMe Solid State Drive (SSD) in G10 G10+\n(Gen10 G10-Plus Gen10-Plus) SmartDrive Carrier NVMe (SCN) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified NVMe SCN SSD (Solid State Drive)\nPart Number(s)\nOption Part# P50214-B21\nSpare Part# P50951-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHPE NVMe PCIe Gen4 U.3 SSDs deliver higher performance for server-storage solutions to better meet the challenges within high performance workloads.\n\nHPE NVMe High Performance Read Intensive (RI) Solid State Drives (SSDs) are best suited for applications requiring a strong blend of high read IOPS, low latency and high endurance at a strong price point. NVMe SSDs communicate directly to applications via the PCIe bus to boost I/O bandwidth and reduce latency. HPE NVMe High Performance RI SSDs provide high-performance data transfers from storage, at rates faster than SAS or SATA SSDs. Designed to utilize the high bandwidth of PCIe Gen3 and PCIe Gen4 in select servers for workloads high in reads such as read caching, web servers and boot/swap. HPE SSDs are backed by up to 3.35 million hours of testing and qualification ensuring reliable, high performing drives. HPE Digitally Signed Firmware prevents unauthorized access to data by providing the assurance that drive firmware comes from a trusted source.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationNVMe SCN SSD\nPart NumberP50214-B21\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1731249\nPlug TypeHot Plug\nForm Factor2.5 inches / SFF\nCapacity1.92TB\nInterface TypeNVMe Gen 4 U.3\nWorkload TypeRead Intensive\nCarrier TypeSCN\nFlash TypeTLC\nPortSingle\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n Installation Instructions for NVMe Drives    \n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P50214-B21 NVMe SCN SSD Solid State Drive",null,"g"]
["P49913-001","Description:Genuine HP InfiniBand NDR 1x400Gb OSFP Multi-mode 50m HCA-side Transceiver\nPart Number(s)\nOption Part# P49764-B21\nSpare Part# P49913-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationOSFP\nPart NumberP49913-001\n\n\n\nProducts ID738467\nManufacturerHP\nApplication/UsageData Networking\nInterface OSFP\nForm FactorPlug-in Module",null,"g"]
["P49911-001","Description:Genuine HP InfiniBand NDR 2x400Gb OSFP Multi-mode 50m Switch-side Transceiver\nPart Number(s)\nOption Part# P49762-B21\nSpare Part# P49911-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationOSFP\nPart NumberP49911-001\n\n\n\nProducts ID1738447\nManufacturerHP\nApplication/UsageData Networking\nInterface OSFP\nForm FactorPlug-in Module",null,"g"]
["P49764-B21","Description:Genuine HP InfiniBand NDR 1x400Gb OSFP Multi-mode 50m HCA-side Transceiver\nPart Number(s)\nOption Part# P49764-B21\nSpare Part# P49913-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationOSFP\nPart NumberP49764-B21\n\n\n\nProducts ID738466\nManufacturerHP\nApplication/UsageData Networking\nInterface OSFP\nForm FactorPlug-in Module",null,"g"]
["P49762-B21","Description:Genuine HP InfiniBand NDR 2x400Gb OSFP Multi-mode 50m Switch-side Transceiver\nPart Number(s)\nOption Part# P49762-B21\nSpare Part# P49911-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nInformation technology professionals rely on HP quality to ensure maximum productivity. As the power of applications  processors  memory adapters and storage devices increases  high-end computer users are seeking ways to optimize their system performance. HP provides leading solutions  adding new levels of performance  availability  flexibility  and management. \n\nSpecifications:\nCategoryHP Networking\nSub-CategoryTransceiver\nGenerationOSFP\nPart NumberP49762-B21\n\n\n\nProducts ID1738446\nManufacturerHP\nApplication/UsageData Networking\nInterface OSFP\nForm FactorPlug-in Module",null,"g"]
["P49751-001","Description:HP 6.4TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49057-B21\nSmartBuy Part# P49057-S21\nSpare Part# P49751-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49751-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727105\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49751-001 SAS BC SSD Solid State Drive",null,"g"]
["P49750-001","Description:HP 6.4TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49056-B21\nSmartBuy Part# P49056-S21\nSpare Part# P49750-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49750-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727751\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49750-001 SAS SC SSD Solid State Drive",null,"g"]
["P49749-001","Description:HP 3.2TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49053-B21\nSmartBuy Part# P49053-S21\nSpare Part# P49749-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49749-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727141\nTypeSolid State Drive\nCapacity3.2-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49749-001 SAS BC SSD Solid State Drive",null,"g"]
["P49748-001","Description:HP 3.2TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49052-B21\nSmartBuy Part# P49052-S21\nSpare Part# P49748-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49748-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727763\nTypeSolid State Drive\nCapacity3.2TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49748-001 SAS SC SSD Solid State Drive",null,"g"]
["P49747-001","Description:HP 1.6TB 2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49049-B21\nSmartBuy Part# P49049-S21\nSpare Part# P49747-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49747-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727177\nTypeSolid State Drive\nCapacity1.6-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49747-001 SAS BC SSD Solid State Drive",null,"g"]
["P49746-001","Description:HP 1.6TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49048-B21\nSmartBuy Part# P49048-S21\nSpare Part# P49746-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49746-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727775\nTypeSolid State Drive\nCapacity1.6TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49746-001 SAS SC SSD Solid State Drive",null,"g"]
["P49745-001","Description:HP 800GB 2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49047-B21\nSmartBuy Part# P49047-S21\nSpare Part# P49745-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49745-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727213\nTypeSolid State Drive\nCapacity800-GB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49745-001 SAS BC SSD Solid State Drive",null,"g"]
["P49744-001","Description:HP 800GB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49046-B21\nSmartBuy Part# P49046-S21\nSpare Part# P49744-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49744-001\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727787\nTypeSolid State Drive\nCapacity800GB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49744-001 SAS SC SSD Solid State Drive",null,"g"]
["P49743-001","Description:HP 15.36TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49045-B21\nSmartBuy Part# P49045-S21\nSpare Part# P49743-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49743-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726781\nTypeSolid State Drive\nCapacity15.36-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49743-001 SAS BC SSD Solid State Drive",null,"g"]
["P49742-001","Description:HP 15.36TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49044-B21\nSmartBuy Part# P49044-S21\nSpare Part# P49742-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49742-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1728704\nTypeSolid State Drive\nCapacity15.36TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49742-001 SAS SC SSD Solid State Drive",null,"g"]
["P49741-001","Description:HP 7.68TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s\nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G10+ (G10-Plus) Hot-Plug \nBasic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49041-B21\nSpare Part# P49741-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49741-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID734198\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49741-001 SAS BC SSD Solid State Drive",null,"g"]
["P49740-001","Description:HP 7.68TB 2.5-inch SFF Serial Attached SCSI (SAS)\n24Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49040-B21\nSmartBuy Part# P49040-S21\nSpare Part# P49740-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49740-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1727739\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard24Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49740-001 SAS SC SSD Solid State Drive",null,"g"]
["P49739-001","Description:HP 7.68TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49039-B21\nSmartBuy Part# P49039-S21\nSpare Part# P49739-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49739-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID727691\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49739-001 SAS SC SSD Solid State Drive",null,"g"]
["P49738-001","Description:HP 7.68TB 3.5-inch LFF SAS 24Gb/s Read-Intensive (RI) \nDigitally Signed Firmware (DS) Solid State Drive (SSD)\nIn HP G8 G9 G10 (Gen8 Gen9 Gen10)Hot-Plug SmartDrive Carrier (SC) (as pictured) \nwith 2 ½ inch - 3 ½ inch Hybrid Adapter Module (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Solid State Drive\nPart Number(s)\nOption Part# P49038-B21\nSpare Part# P49738-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49738-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1734997\nTypeSolid State Drive\nCapacity7.68TB\nInterface TypeSAS\nDrive Interface Standard24Gb/s SAS\nData Transfer Rate1.2GB/s\nInterfaceSerial Attached SCSI\n4KB Random Read155000 IOPS\n4KB Random Write140000 IOPS\n \nBest UseRead Intensive (RI)\n\n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49738-001 SAS SC SSD Solid State Drive",null,"g"]
["P49737-001","Description:HP 3.84TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49035-B21\nSmartBuy Part# P49035-S21\nSpare Part# P49737-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49737-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726841\nTypeSolid State Drive\nCapacity3.84-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49737-001 SAS BC SSD Solid State Drive",null,"g"]
["P49736-001","Description:HP 3.84TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49034-B21\nSmartBuy Part# P49034-S21\nSpare Part# P49736-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49736-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1727703\nTypeSolid State Drive\nCapacity3.84TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49736-001 SAS SC SSD Solid State Drive",null,"g"]
["P49735-001","Description:HP 1.92TB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49031-B21\nSmartBuy Part# P49031-S21\nSpare Part# P49735-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49735-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726877\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49735-001 SAS BC SSD Solid State Drive",null,"g"]
["P49734-001","Description:HP 1.92TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49030-B21\nSmartBuy Part# P49030-S21\nSpare Part# P49734-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49734-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1727715\nTypeSolid State Drive\nCapacity1.92TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49734-001 SAS SC SSD Solid State Drive",null,"g"]
["P49733-001","Description:HP 960GB 2.5-inch SFF SAS Read-Intensive (RI) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49029-B21\nSmartBuy Part# P49029-S21\nSpare Part# P49733-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49733-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID726917\nTypeSolid State Drive\nCapacity960-GB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49733-001 SAS BC SSD Solid State Drive",null,"g"]
["P49732-001","Description:HP 960GB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Read-Intensive (RI)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49028-B21\nSmartBuy Part# P49028-S21\nSpare Part# P49732-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49732-001\n\nBest Use:    Read-Intensive\nManufacturer:Hewlett Packard\n\n\nProducts ID1727727\nTypeSolid State Drive\nCapacity960GB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49732-001 SAS SC SSD Solid State Drive",null,"g"]
["P49654-B21","Description:HP Intel® Xeon® Gold 6454S G11(2.2GHz/32-core/270W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49654-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49654-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49654-B21\n\n\n\nProducts ID737316\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.2GHz\n64-bit ProcessingYes\nThermal Design Power270W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49654-B21 G11 Intel Xeon",null,"g"]
["P49649-B21","Description:HP Intel® Xeon® Platinum 8470N G11(1.7GHz/52-core/300W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49649-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49649-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49649-B21\n\n\n\nProducts ID1737322\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDi-Pentaconta\nProcessor Qty1\nClock Speed1.7GHz\n64-bit ProcessingYes\nThermal Design Power300W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49649-B21 G11 Intel Xeon",null,"g"]
["P49641-B21","Description:HP Intel® Xeon® Gold 6421N G11(1.8GHz/32-core/185W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49641-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49641-B21\n\n\n\nProducts ID738235\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed1.8GHz\n64-bit ProcessingYes\nThermal Design Power185W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49641-B21 G11 Intel Xeon",null,"g"]
["P49640-B21","Description:HP Intel® Xeon® Gold 5418Y G11(2.0GHz/24-core/185W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49640-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49640-B21\n\n\n\nProducts ID1738239\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTetraicosa-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power185W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49640-B21 G11 Intel Xeon",null,"g"]
["P49639-B21","Description:HP Intel® Xeon® Gold 5415+ G11(2.9GHz/8-core/150W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49639-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49639-B21\n\n\n\nProducts ID738241\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Core\nProcessor Qty1\nClock Speed2.9GHz\n64-bit ProcessingYes\nThermal Design Power150W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49639-B21 G11 Intel Xeon",null,"g"]
["P49638-B21","Description:HP Intel® Xeon® Gold 6438N G11(2.0GHz/32-core/205W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49638-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49638-B21\n\n\n\nProducts ID1738231\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power205W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49638-B21 G11 Intel Xeon",null,"g"]
["P49632-B21","Description:HP Intel® Xeon® Platinum 8458P G11(2.7GHz/44-core/350W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49632-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49632-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49632-B21\n\n\n\nProducts ID737324\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTetra-Tentraconta\nProcessor Qty1\nClock Speed2.7GHz\n64-bit ProcessingYes\nThermal Design Power350W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49632-B21 G11 Intel Xeon",null,"g"]
["P49631-B21","Description:HP Intel® Xeon® Platinum 8468V G11(2.4GHz/48-core/330W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49631-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49631-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49631-B21\n\n\n\nProducts ID1737323\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Tentraconta\nProcessor Qty1\nClock Speed2.4GHz\n64-bit ProcessingYes\nThermal Design Power330W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49631-B21 G11 Intel Xeon",null,"g"]
["P49619-B21","Description:HP Intel® Xeon® Gold 6414U G11(2.0GHz/32-core/250W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49619-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49619-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49619-B21\n\n\n\nProducts ID1737315\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power250W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49619-B21 G11 Intel Xeon",null,"g"]
["P49617-B21","Description:HP Intel® Xeon® Bronze 3408U G11(1.8GHz/8-core/125W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49617-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Bronze processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49617-B21\n\n\n\nProducts ID738245\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Core\nProcessor Qty1\nClock Speed1.8GHz\n64-bit ProcessingYes\nThermal Design Power125W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49617-B21 G11 Intel Xeon",null,"g"]
["P49616-B21","Description:HP Intel® Xeon® Platinum 8452Y G11(2.0GHz/36-core/300W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49616-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49616-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49616-B21\n\n\n\nProducts ID1737321\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreHexa-Triaconta\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power300W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49616-B21 G11 Intel Xeon",null,"g"]
["P49615-B21","Description:HP Intel® Xeon® Gold 6438Y+ G11(2.0GHz/32-core/205W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49615-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49615-B21\n\n\n\nProducts ID738233\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power205W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49615-B21 G11 Intel Xeon",null,"g"]
["P49614-B21","Description:HP Intel® Xeon® Gold 6430 G11(2.1GHz/32-core/270W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49614-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49614-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49614-B21\n\n\n\nProducts ID1737314\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.1GHz\n64-bit ProcessingYes\nThermal Design Power270W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49614-B21 G11 Intel Xeon",null,"g"]
["P49613-B21","Description:HP Intel® Xeon® Gold 5420+ G11(2.0GHz/28-core/205W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49613-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49613-B21\n\n\n\nProducts ID738238\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOctacosa-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power205W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49613-B21 G11 Intel Xeon",null,"g"]
["P49612-B21","Description:HP Intel® Xeon® Gold 5418Y G11(2.0GHz/24-core/185W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49612-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49612-B21\n\n\n\nProducts ID1738240\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTetraicosa-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power185W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49612-B21 G11 Intel Xeon",null,"g"]
["P49611-B21","Description:HP Intel® Xeon® Silver 4416+ G11(2.0GHz/20-core/165W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49611-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Silver processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49611-B21\n\n\n\nProducts ID738243\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreIcosa-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power165W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49611-B21 G11 Intel Xeon",null,"g"]
["P49610-B21","Description:HP Intel® Xeon® Silver 4410Y G11(2.0GHz/12-core/150W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49610-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Silver processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49610-B21\n\n\n\nProducts ID1738244\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDideca-Core\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power150W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49610-B21 G11 Intel Xeon",null,"g"]
["P49607-B21","Description:HP Intel® Xeon® Platinum 8480+ G11(2.0GHz/56-core/350W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49607-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49607-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49607-B21\n\n\n\nProducts ID737320\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreHexa-Pentaconta\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power350W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49607-B21 G11 Intel Xeon",null,"g"]
["P49606-B21","Description:HP Intel® Xeon® Platinum 8470 G11(2.0GHz/52-core/350W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49606-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49606-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49606-B21\n\n\n\nProducts ID1737319\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDi-Pentaconta\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power350W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49606-B21 G11 Intel Xeon",null,"g"]
["P49605-B21","Description:HP Intel® Xeon® Platinum 8468 G11(2.1GHz/48-core/350W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49605-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49605-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49605-B21\n\n\n\nProducts ID737318\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Tentraconta\nProcessor Qty1\nClock Speed2.1GHz\n64-bit ProcessingYes\nThermal Design Power350W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49605-B21 G11 Intel Xeon",null,"g"]
["P49604-B21","Description:HP Intel® Xeon® Platinum 8460Y+ G11(2.0GHz/40-core/300W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49604-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49604-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Platinum processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49604-B21\n\n\n\nProducts ID1737317\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTentraconta\nProcessor Qty1\nClock Speed2.0GHz\n64-bit ProcessingYes\nThermal Design Power300W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49604-B21 G11 Intel Xeon",null,"g"]
["P49601-B21","Description:HP Intel® Xeon® Gold 6434 G11(3.7GHz/8-core/195W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49601-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49601-B21\n\n\n\nProducts ID738236\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Core\nProcessor Qty1\nClock Speed3.7GHz\n64-bit ProcessingYes\nThermal Design Power195W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49601-B21 G11 Intel Xeon",null,"g"]
["P49600-B21","Description:HP Intel® Xeon® Gold 6448Y G11(2.1GHz/32-core/225W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49600-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49600-B21\n\n\n\nProducts ID1738232\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreDotriaconta-Core\nProcessor Qty1\nClock Speed2.1GHz\n64-bit ProcessingYes\nThermal Design Power225W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49600-B21 G11 Intel Xeon",null,"g"]
["P49599-B21","Description:HP Intel® Xeon® Gold 6442Y G11(2.6GHz/24-core/225W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49599-B21\n\n\n\n\n\n\n\n\n \n\n\nHP Processor Kits:\nManufacturer Part# P49599-B21\nThis is the full processor option kit. It includes the\nProcessor(s), Heat-Sink(s), Fan(s), Thermal paste\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryProliant Processor\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49599-B21\n\n\n\nProducts ID738234\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreTetracosa-Core\nProcessor Qty1\nClock Speed2.6GHz\n64-bit ProcessingYes\nThermal Design Power225W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49599-B21 G11 Intel Xeon",null,"g"]
["P49598-B21","Description:HP Intel® Xeon® Gold 6426Y G11(2.5GHz/16-core/185W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49598-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49598-B21\n\n\n\nProducts ID1738237\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreHexadeca-Core\nProcessor Qty1\nClock Speed2.5GHz\n64-bit ProcessingYes\nThermal Design Power185W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49598-B21 G11 Intel Xeon",null,"g"]
["P49597-B21","Description:HP Intel® Xeon® Gold 5415+ G11(2.9GHz/8-core/150W)Full Processor Option KitPart Number(s)\nManufacturer Part# P49597-B21\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nHP  Intel® Xeon® Gold processors offer the industry's best performance for mission-critical and hybrid cloud workloads - real-time analytics - machine learning - and artificial intelligence - with monumental leaps in I/O - memory - storage - and network technologies.\n\nSpecifications:\nCategoryHP\nSub-CategoryIntel Xeon\nGenerationG11\nPart NumberP49597-B21\n\n\n\nProducts ID738242\nProduct TypeProcessor Kit\nProcessor TypeIntel Xeon\nProcessor CoreOcta-Core\nProcessor Qty1\nClock Speed2.9GHz\n64-bit ProcessingYes\nThermal Design Power150W\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49597-B21 G11 Intel Xeon",null,"g"]
["P49057-S21","Description:HP 6.4TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49057-B21\nSmartBuy Part# P49057-S21\nSpare Part# P49751-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49057-S21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727101\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49057-S21 SAS BC SSD Solid State Drive",null,"g"]
["P49057-K21","Description:HP 6.4TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49057-K21\nSmartBuy Part# P49057-S21\nSpare Part# P49751-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49057-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734130\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49057-K21 SAS BC SSD Solid State Drive",null,"g"]
["P49057-H21","Description:HP 6.4TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49057-H21\nSmartBuy Part# P49057-S21\nSpare Part# P49751-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49057-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734150\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49057-H21 SAS BC SSD Solid State Drive",null,"g"]
["P49057-B21","Description:HP 6.4TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49057-B21\nSmartBuy Part# P49057-S21\nSpare Part# P49751-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49057-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727097\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49057-B21 SAS BC SSD Solid State Drive",null,"g"]
["P49056-S21","Description:HP 6.4TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49056-B21\nSmartBuy Part# P49056-S21\nSpare Part# P49750-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49056-S21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727747\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49056-S21 SAS SC SSD Solid State Drive",null,"g"]
["P49056-K21","Description:HP 6.4TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49056-K21\nSmartBuy Part# P49056-S21\nSpare Part# P49750-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49056-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734146\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49056-K21 SAS SC SSD Solid State Drive",null,"g"]
["P49056-H21","Description:HP 6.4TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49056-H21\nSmartBuy Part# P49056-S21\nSpare Part# P49750-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49056-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1728788\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49056-H21 SAS SC SSD Solid State Drive",null,"g"]
["P49056-B21","Description:HP 6.4TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49056-B21\nSmartBuy Part# P49056-S21\nSpare Part# P49750-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49056-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727743\nTypeSolid State Drive\nCapacity6.4TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49056-B21 SAS SC SSD Solid State Drive",null,"g"]
["P49053-S21","Description:HP 3.2TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49053-B21\nSmartBuy Part# P49053-S21\nSpare Part# P49749-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49053-S21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727137\nTypeSolid State Drive\nCapacity3.2-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49053-S21 SAS BC SSD Solid State Drive",null,"g"]
["P49053-K21","Description:HP 3.2TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49053-K21\nSmartBuy Part# P49053-S21\nSpare Part# P49749-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49053-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734186\nTypeSolid State Drive\nCapacity3.2-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49053-K21 SAS BC SSD Solid State Drive",null,"g"]
["P49053-H21","Description:HP 3.2TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49053-H21\nSmartBuy Part# P49053-S21\nSpare Part# P49749-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49053-H21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1734182\nTypeSolid State Drive\nCapacity3.2-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49053-H21 SAS BC SSD Solid State Drive",null,"g"]
["P49053-B21","Description:HP 3.2TB2.5-inch SFF SAS Mixed-Use (MU) 24Gb/s\nDigitally Signed Firmware (DS)Solid State Drive (SSD) Mutli-Vendor (MV)\nIn HP G10+ G11 (G10-Plus Gen10-Plus Gen11)Hot-Plug Basic Carrier (BC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49053-B21\nSmartBuy Part# P49053-S21\nSpare Part# P49749-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS BC SSD\nPart NumberP49053-B21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID727133\nTypeSolid State Drive\nCapacity3.2-TB\nInterface TypeSAS\nDrive Interface StandardSAS\nDrive CarrierBasic Carrier (BC)\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49053-B21 SAS BC SSD Solid State Drive",null,"g"]
["P49052-S21","Description:HP 3.2TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49052-B21\nSmartBuy Part# P49052-S21\nSpare Part# P49748-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49052-S21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID1727759\nTypeSolid State Drive\nCapacity3.2TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49052-S21 SAS SC SSD Solid State Drive",null,"g"]
["P49052-K21","Description:HP 3.2TB 2.5-inch SFF Serial Attached SCSI (SAS)\n12Gb/s Smart Carrier (SC) Solid State Drive (SSD)\nMulti Vendor (MV) Mixed-Use (MU)\nIn HP Hot-Plug SmartDrive Carrier (SC) (as pictured)\nGenuine HP serial number and SSD firmware\nGenuine HP Certified Solid State Drive\nPart Number(s)\nOption Part# P49052-K21\nSmartBuy Part# P49052-S21\nSpare Part# P49748-001\n\n\n\n\n\n\n\n\n \n\n \n\n \n\n \n\n \n\n \n\n\nOverview:\nDo you need more performance from your HP Proliant Server series platforms? HP Enterprise Solid State Drives (SSDs) deliver exceptional performance and endurance while reducing power consumption for customers with applications requiring high random read and write IOPs performance. You can prevent data loss and monitor the SSD life with HP SmartSSD Wear Gauge compatibility in management tools.These drives deliver higher performance - better latency and more power-efficient solutions when compared with traditional rotating media (HDDs). Plus they fit seamlessly into the existing HP server infrastructure.\n\nSpecifications:\nCategoryProliant HardDrive\nSub-CategorySolid State Drive\nGenerationSAS SC SSD\nPart NumberP49052-K21\n\nBest Use:    Mixed-Use\nManufacturer:Hewlett Packard\n\n\nProducts ID734142\nTypeSolid State Drive\nCapacity3.2TB\nInterface TypeSerial Attached SCSI\nDrive Interface Standard12Gb/s SAS\n\n\n \n \n \n \n \n \n \n \n\n\n\n\n\n\n\n\n \n \n\n\n\n \n \n\n\n\n\n\n \n [ Replacement Instructions ]\n \n\n\n\n\n\n \n \n \n \n\n\n \n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\n\nPart# P49052-K21 SAS SC SSD Solid State Drive",null,"g"]