{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[[13,1,13,8],[18,1,18,7],[19,1,19,7]]}
["Модель расчета длины плеча от точки опоры"]
[]
[]
[]
[null,null,{"$f":"C16","v":3.5},{"$f":"D16","v":5.3},{"$f":"E16","v":5.3},{"$f":"F16","v":5.3},{"$f":"G16","v":5.3},3.5]
[null,null,"Н1  ","Н2  ","Н3  ","Н4  ","Н5  "]
[]
[]
[]
[]
[]
[]
[]
[null,"Исходные данные"]
["Нагрузки",null,"Н1","Н2","Н3","Н4","Н5",null,"Длина балки","Середина балки"]
["Растояние между нагрузками",null,3.5,5.3,5.3,5.3,5.3,3.5,{"$f":"SUM(C16:H16)","v":28.200000000000003}]
[]
[null,null,null,null,null,null,null,null,{"$f":"I16/2","v":14.100000000000001}]
["User Defined Function","Результат"]
[null,"Распределение нагрузок относительно середины балки"]
["Нагрузки",null,{"$f":"C15","v":"Н1"},{"$f":"D15","v":"Н2"},"Н3","Н4","Н5"]
["Плечо от точки опоры",null,{"$f":"LoadDistributionModel(C16,$C$16:$G$16,$I$16,$I$18)","v":3.5},{"$f":"LoadDistributionModel(C16:D16,$C$16:$H$16,$I$16,$I$18)","v":8.8000000000000007},{"$f":"LoadDistributionModel(C16:E16,$C$16:$H$16,$I$16,$I$18)","v":14.100000000000001},{"$f":"LoadDistributionModel(C16:F16,$C$16:$H$16,$I$16,$I$18)","v":14.1},{"$f":"LoadDistributionModel(C16:G16,$C$16:$H$16,$I$16,$I$18)","v":8.8000000000000007}]
["Плечо от точки опоры",null,null,null,{"$f":"H5+G5+F5","v":14.100000000000001},{"$f":"H5+G5","v":8.8000000000000007},{"$f":"H5","v":3.5}]